FSP Configuration
  Board "RA6|RA6E1|VOICE-RA6E1"
  R7FA6E10F2CFM
    part_number: R7FA6E10F2CFM
    rom_size_bytes: 1048576
    ram_size_bytes: 262144
    data_flash_size_bytes: 8192
    package_style: QFP
    package_pins: 64
    
  RA6E1
    series: 6
    
  RA6E1 Family
    Enable inline BSP IRQ functions: Enabled
    Security: Exceptions: Exception Response: Non-Maskable Interrupt
    Security: Exceptions: BusFault, HardFault, and NMI Target: Secure State
    Security: System Reset Request Accessibility: Secure State
    Security: Exceptions: Prioritize Secure Exceptions: Disabled
    Security: Cache Accessibility: Both Secure and Non-Secure State
    Security: System Reset Status Accessibility: Both Secure and Non-Secure State
    Security: Battery Backup Accessibility: Both Secure and Non-Secure State
    Security: SRAM Accessibility: SRAM Protection: Both Secure and Non-Secure State
    Security: SRAM Accessibility: SRAM ECC: Both Secure and Non-Secure State
    Security: SRAM Accessibility: Standby RAM: Regions 7-0 are all Secure.
    Security: BUS Accessibility: Bus Security Attribution Register A: Both Secure and Non-Secure State
    Security: BUS Accessibility: Bus Security Attribution Register B: Both Secure and Non-Secure State
    Security: Flash Bank Select Accessibility: Both Secure and Non-Secure State
    Security: Uninitialized Non-Secure Application Fallback: Enable Uninitialized Non-Secure Application Fallback
    Startup C-Cache Line Size: 32 Bytes
    OFS0 register settings: Independent WDT: Start Mode: IWDT is stopped after a reset
    OFS0 register settings: Independent WDT: Timeout Period: 2048 cycles
    OFS0 register settings: Independent WDT: Dedicated Clock Frequency Divisor: 128
    OFS0 register settings: Independent WDT: Window End Position:  0% (no window end position)
    OFS0 register settings: Independent WDT: Window Start Position: 100% (no window start position)
    OFS0 register settings: Independent WDT: Reset Interrupt Request Select: Reset is enabled
    OFS0 register settings: Independent WDT: Stop Control: Stop counting when in Sleep, Snooze mode, or Software Standby
    OFS0 register settings: WDT: Start Mode Select: Stop WDT after a reset (register-start mode)
    OFS0 register settings: WDT: Timeout Period: 16384 cycles
    OFS0 register settings: WDT: Clock Frequency Division Ratio: 128
    OFS0 register settings: WDT: Window End Position:  0% (no window end position)
    OFS0 register settings: WDT: Window Start Position: 100% (no window start position)
    OFS0 register settings: WDT: Reset Interrupt Request: Reset
    OFS0 register settings: WDT: Stop Control: Stop counting when entering Sleep mode
    OFS1_SEL register settings: Voltage Detection 0 Level Security Attribution: VDSEL setting loads from OFS1_SEC
    OFS1_SEL register settings: Voltage Detection 0 Circuit Start Security Attribution: LVDAS setting loads from OFS1_SEC
    OFS1 register settings: Voltage Detection 0 Circuit Start: Voltage monitor 0 reset is disabled after reset
    OFS1 register settings: Voltage Detection 0 Level: 2.80 V
    OFS1 register settings: HOCO Oscillation Enable: HOCO oscillation is enabled after reset
    Block Protection Settings (BPS): BPS0: 
    Block Protection Settings (BPS): BPS1: 
    Block Protection Settings (BPS): BPS2: 
    Permanent Block Protection Settings (PBPS): PBPS0: 
    Permanent Block Protection Settings (PBPS): PBPS1: 
    Permanent Block Protection Settings (PBPS): PBPS2: 
    Dual Bank Mode: Disabled
    Clocks: HOCO FLL Function: Disabled
    Main Oscillator Wait Time: 8163 cycles
    
  RA6E1 event data
  RA Common
    Main stack size (bytes): 0x12000
    Heap size (bytes): 0
    MCU Vcc (mV): 3300
    Parameter checking: Disabled
    Assert Failures: Return FSP_ERR_ASSERTION
    Error Log: No Error Log
    Clock Registers not Reset Values during Startup: Disabled
    Main Oscillator Populated: Not Populated
    PFS Protect: Enabled
    C Runtime Initialization : Enabled
    Early BSP Initialization : Disabled
    Main Oscillator Clock Source: Crystal or Resonator
    Subclock Populated: Populated
    Subclock Drive (Drive capacitance availability varies by MCU): Standard/Normal mode
    Subclock Stabilization Time (ms): 1000
    
  Clocks
    XTAL 24000000Hz
    HOCO 20MHz
    PLL Src: HOCO
    PLL Div /2
    PLL Mul x20.0
    PLL2 Src: HOCO
    PLL2 Div /2
    PLL2 Mul x24.0
    Clock Src: PLL
    CLKOUT Disabled
    UCLK Src: PLL2
    ICLK Div /1
    PCLKA Div /2
    PCLKB Div /4
    PCLKC Div /4
    PCLKD Div /2
    FCLK Div /4
    CLKOUT Div /1
    UCLK Div /5
    
  Pin Configurations
    R7FA6E10F2CFM.pincfg -> 
      AVCC0 56 SYSTEM_AVCC0 - - - - - - - - IO "Read only" - 
      AVSS0 57 SYSTEM_AVSS0 - - - - - - - - IO "Read only" - 
      P000 64 - - - - Disabled - - "ADC0: AN000; ICU: IRQ6-DS" AMIC_L I - - 
      P001 63 - - - - Disabled - - "ADC0: AN001; ICU: IRQ7-DS" AMIC_R I - - 
      P002 62 - - - - Disabled - - "ADC0: AN002; ICU: IRQ8-DS" - None - - 
      P003 61 - - - - Disabled - - "ADC0: AN003" - None - - 
      P004 60 - - - - Disabled - - "ADC0: AN004; ICU: IRQ9-DS" - None - - 
      P014 53 - - - - Disabled - - "ADC0: AN012; DAC120: DA0" PLAYBACK O - - 
      P015 52 - - - - Disabled - - "ADC0: AN013; ICU: IRQ13" - None - - 
      P100 48 - - L None Disabled - - "AGT0: AGTIO0; GPT5: GTIOC5B; GPT_POEGA: GTETRGA; ICU: IRQ2; QSPI: QSPCLK; SCI0: RXD0; SCI1: SCK1; SPI1: MISO1" "QSPI_CLK / (SPI1_MISO)" IO - - 
      P101 47 - - L None Disabled - - "AGT0: AGTEE0; GPT5: GTIOC5A; GPT_POEGB: GTETRGB; ICU: IRQ1; QSPI: QIO1; SCI0: TXD0; SCI1: CTS_RTS1; SPI1: MOSI1" "QSPI_DQ1 / SPI1_MOSI (DMIC_R)" IO - - 
      P102 46 - - L - Disabled - - "ADC0: ADTRG0; AGT0: AGTO0; CAN0: CRX0; GPT2: GTIOC2B; QSPI: QIO0; SCI0: SCK0; SPI1: RSPCK1" "QSPI_DQ0 / SPI1_SCK" IO - - 
      P103 45 - - L - Disabled - - "AGT2: AGTIO2; CAN0: CTX0; GPT2: GTIOC2A; QSPI: QIO3; SCI0: CTS_RTS0; SPI1: SSLB0" "QSPI_DQ3 / SPI1_SSL" IO - - 
      P104 44 - - - - Disabled - - "AGT2: AGTEE2; GPT1: GTIOC1B; GPT_POEGB: GTETRGB; ICU: IRQ1; QSPI: QIO2; SPI1: SSLB1" QSPI_DQ2 None - - 
      P105 43 - - L None Disabled - - "AGT2: AGTO2; GPT1: GTIOC1A; GPT_POEGA: GTETRGA; ICU: IRQ0; SPI1: SSLB2" "SCKO (as I2S_CLK)" IO - - 
      P106 42 - - - - Disabled - - "AGT0: AGTOB0; SPI1: SSLB3" - None - - 
      P108 33 JTAG/SWD_TMS - L - "Peripheral mode" - - "AGT3: AGTOA3; JTAG/SWD: SWDIO; JTAG/SWD: TMS; SCI9: CTS_RTS9; SPI0: SSLA0" SWD_SWDIO IO - - 
      P109 34 JTAG/SWD_TDO - L - "Peripheral mode" - - "AGT3: AGTOB3; CGC: CLKOUT; GPT1: GTIOC1A; JTAG/SWD: TDO; JTAG/SWD: TRACESWO; SCI9: TXD9; SPI0: MOSI0" "SPI0_MOSI (DMIC_L), TXD9" IO - - 
      P110 35 JTAG/SWD_TDI - L None "Peripheral mode" - - "AGT3: AGTEE3; GPT1: GTIOC1B; ICU: IRQ3; JTAG/SWD: TDI; SCI2: CTS_RTS2; SCI9: RXD9; SPI0: MISO0" "(SPI0_MISO), RXD9" IO - - 
      P111 36 - - L None Disabled - - "AGT5: AGTOA5; ICU: IRQ4; SCI2: SCK2; SCI9: SCK9; SPI0: RSPCK0" "SPI0_SCK (as SCKI)" IO - - 
      P112 37 - - L - Disabled - - "AGT5: AGTOB5; QSPI: QSSL; SCI1: SCK1; SCI2: TXD2; SPI0: SSLA0" QSPI_CS IO - - 
      P113 38 - - L - Disabled - - "AGT5: AGTEE5; GPT2: GTIOC2A; SCI2: RXD2" LED3 IO - - 
      P200 27 - - - - Disabled - - "ICU: NMI" - None - - 
      P201 26 - - - - Disabled - - "SYSTEM: MD" - None - - 
      P205 23 - - L None Disabled - - "AGT1: AGTO1; CGC: CLKOUT; GPT4: GTIOC4A; ICU: IRQ1-DS; IIC1: SCL1; SCI4: TXD4; SCI9: CTS_RTS9; SPI0: SSLA0; USB FS: USB_OVRCURA_A-DS" SPI0_SSL IO - - 
      P206 22 - - L None Disabled - - "ICU: IRQ0-DS; IIC1: SDA1; SCI4: RXD4; SCI9: CTS9; SPI0: SSLA1; USB FS: USB_VBUSEN" VCOM_TXD I - - 
      P207 21 - - L - Disabled - - "QSPI: QSSL; SCI4: TXD4; SPI0: SSLA2" VCOM_RXD O - - 
      P208 24 - - - - Disabled - - "QSPI: QIO3; TRACE: TRDATA3" "PMOD IO3" IO - - 
      P212 10 - - - - Disabled - - "AGT1: AGTEE1; CGC: EXTAL; GPT_POEGD: GTETRGD; ICU: IRQ3; SCI1: RXD1" - None - - 
      P213 9 - - - - Disabled - - "AGT2: AGTEE2; CGC: XTAL; GPT_POEGC: GTETRGC; ICU: IRQ2; SCI1: TXD1" - None - - 
      P300 32 JTAG/SWD_TCK - L - "Peripheral mode" - - "JTAG/SWD: SWCLK; JTAG/SWD: TCK; SPI0: SSLA1" SWD_SWCLK IO - - 
      P301 31 - - L None Disabled - - "AGT0: AGTIO0; GPT4: GTIOC4B; ICU: IRQ6; SCI2: RXD2; SCI9: CTS_RTS9; SPI0: SSLA2" I2S_WS IO - - 
      P302 30 - - - - Disabled - - "GPT4: GTIOC4A; ICU: IRQ5; SCI2: TXD2; SPI0: SSLA3" "PMOD IRQ" None - - 
      P303 29 - - - - Disabled - - "GPT7: GTIOC7B; SCI9: CTS9" "PMOD IO1" IO - - 
      P304 28 - - - None Disabled - - "AGT2: AGTEE2; GPT7: GTIOC7A; ICU: IRQ9" "PMOD IO2" IO - - 
      P400 1 - - L None Disabled - - "AGT1: AGTIO1; GPT6: GTIOC6A; ICU: IRQ0; IIC0: SCL0; SCI4: SCK4" LED2 IO - - 
      P401 2 - - - - Disabled - - "CAN0: CTX0; GPT6: GTIOC6B; GPT_POEGA: GTETRGA; ICU: IRQ5-DS; IIC0: SDA0; SCI4: CTS_RTS4" - None - - 
      P402 3 - - - - Disabled - - "AGT0: AGTIO0; AGT1: AGTIO1; AGT2: AGTIO2; AGT3: AGTIO3; CAC: CACREF; CAN0: CRX0; ICU: IRQ4-DS; RTC: RTCIC0; SCI4: CTS4" "USER SW" None - - 
      P407 16 - - L - Disabled - - "ADC0: ADTRG0; AGT0: AGTIO0; GPT6: GTIOC6A; IIC0: SDA0; RTC: RTCOUT; SCI4: CTS_RTS4; SPI0: SSLA3; USB FS: USB_VBUS" "USB VBUS" IO - - 
      P408 15 - - L None Disabled - - "AGT2: AGTOB2; GPT6: GTIOC6B; ICU: IRQ7; IIC0: SCL0; SCI3: RXD3; SCI4: CTS4; USB FS: USB_ID" SCI3_RXD3 I - - 
      P409 14 - - L None Disabled - - "AGT2: AGTOA2; ICU: IRQ6; SCI3: TXD3; USB FS: USB_EXICEN" SCI3_TXD3 O - - 
      P410 13 - - L None Disabled - - "AGT1: AGTOB1; ICU: IRQ5; SCI0: RXD0; SCI3: SCK3; SPI1: MISO1" SCI3_SCK3 IO - - 
      P411 12 - - L None Disabled - - "AGT1: AGTOA1; ICU: IRQ4; SCI0: TXD0; SCI3: CTS_RTS3; SPI1: MOSI1" SCI3_CTS_RTS3 IO - - 
      P500 49 - - L - Disabled - - "AGT0: AGTOA0; CAC: CACREF; QSPI: QSPCLK; USB FS: USB_VBUSEN" LED1 IO - - 
      RES 25 SYSTEM_RES - - - - - - - - IO "Read only" - 
      USB_DM 18 SYSTEM_USB_DM - - - - - - - - IO "Read only" - 
      USB_DP 19 SYSTEM_USB_DP - - - - - - - - IO "Read only" - 
      VBATT 4 SYSTEM_VBATT - - - - - - - - IO "Read only" - 
      VCC 50 SYSTEM_VCC - - - - - - - - IO "Read only" - 
      VCC 11 SYSTEM_VCC - - - - - - - - IO "Read only" - 
      VCC 39 SYSTEM_VCC - - - - - - - - IO "Read only" - 
      VCC_USB 20 SYSTEM_VCC_USB - - - - - - - - IO "Read only" - 
      VCL 41 SYSTEM_VCL - - - - - - - - IO "Read only" - 
      VCL0 5 SYSTEM_VCL0 - - - - - - - - IO "Read only" - 
      VREFH 55 SYSTEM_VREFH - - - - - - - - IO "Read only" - 
      VREFH0 59 SYSTEM_VREFH0 - - - - - - - - IO "Read only" - 
      VREFL 54 SYSTEM_VREFL - - - - - - - - IO "Read only" - 
      VREFL0 58 SYSTEM_VREFL0 - - - - - - - - IO "Read only" - 
      VSS 51 SYSTEM_VSS - - - - - - - - IO "Read only" - 
      VSS 8 SYSTEM_VSS - - - - - - - - IO "Read only" - 
      VSS 40 SYSTEM_VSS - - - - - - - - IO "Read only" - 
      VSS_USB 17 SYSTEM_VSS_USB - - - - - - - - IO "Read only" - 
      XCIN 6 CGC_XCIN - - - - - - - - IO "Read only" - 
      XCOUT 7 CGC_XCOUT - - - - - - - - IO "Read only" - 
    VOICE_RA6E1_2DMIC.pincfg -> g_bsp_pin_cfg
      AVCC0 56 SYSTEM_AVCC0 - - - - - - - - IO "Read only" - 
      AVSS0 57 SYSTEM_AVSS0 - - - - - - - - IO "Read only" - 
      P000 64 ADC0_AN000 - - - "Analog mode" - - "ADC0: AN000; ICU: IRQ6-DS" AMIC_L I - - 
      P001 63 ADC0_AN001 - - - "Analog mode" - - "ADC0: AN001; ICU: IRQ7-DS" AMIC_R I - - 
      P002 62 - - - - Disabled - - "ADC0: AN002; ICU: IRQ8-DS" - None - - 
      P003 61 - - - - Disabled - - "ADC0: AN003" - None - - 
      P004 60 - - - - Disabled - - "ADC0: AN004; ICU: IRQ9-DS" - None - - 
      P014 53 DAC120_DA0 - - - "Analog mode" - - "ADC0: AN012; DAC120: DA0" PLAYBACK O - - 
      P015 52 - - - - Disabled - - "ADC0: AN013; ICU: IRQ13" - None - - 
      P100 48 SPI1_MISO1 - M None "Peripheral mode" - - "AGT0: AGTIO0; GPT5: GTIOC5B; GPT_POEGA: GTETRGA; ICU: IRQ2; QSPI: QSPCLK; SCI0: RXD0; SCI1: SCK1; SPI1: MISO1" "QSPI_CLK / (SPI1_MISO)" IO - - 
      P101 47 SPI1_MOSI1 - M None "Peripheral mode" - - "AGT0: AGTEE0; GPT5: GTIOC5A; GPT_POEGB: GTETRGB; ICU: IRQ1; QSPI: QIO1; SCI0: TXD0; SCI1: CTS_RTS1; SPI1: MOSI1" "QSPI_DQ1 / SPI1_MOSI (DMIC_R)" IO - - 
      P102 46 SPI1_RSPCK1 - L - "Peripheral mode" - - "ADC0: ADTRG0; AGT0: AGTO0; CAN0: CRX0; GPT2: GTIOC2B; QSPI: QIO0; SCI0: SCK0; SPI1: RSPCK1" "QSPI_DQ0 / SPI1_SCK" IO - - 
      P103 45 SPI1_SSLB0 - M - "Peripheral mode" - - "AGT2: AGTIO2; CAN0: CTX0; GPT2: GTIOC2A; QSPI: QIO3; SCI0: CTS_RTS0; SPI1: SSLB0" "QSPI_DQ3 / SPI1_SSL" IO - - 
      P104 44 - - - - Disabled - - "AGT2: AGTEE2; GPT1: GTIOC1B; GPT_POEGB: GTETRGB; ICU: IRQ1; QSPI: QIO2; SPI1: SSLB1" QSPI_DQ2 None - - 
      P105 43 GPT1_GTIOC1A - L None "Peripheral mode" - - "AGT2: AGTO2; GPT1: GTIOC1A; GPT_POEGA: GTETRGA; ICU: IRQ0; SPI1: SSLB2" "SCKO (as I2S_CLK)" IO - - 
      P106 42 - - - - Disabled - - "AGT0: AGTOB0; SPI1: SSLB3" - None - - 
      P108 33 JTAG/SWD_SWDIO - L - "Peripheral mode" - - "AGT3: AGTOA3; JTAG/SWD: SWDIO; JTAG/SWD: TMS; SCI9: CTS_RTS9; SPI0: SSLA0" SWD_SWDIO IO - - 
      P109 34 SPI0_MOSI0 - M - "Peripheral mode" - - "AGT3: AGTOB3; CGC: CLKOUT; GPT1: GTIOC1A; JTAG/SWD: TDO; JTAG/SWD: TRACESWO; SCI9: TXD9; SPI0: MOSI0" "SPI0_MOSI (DMIC_L), TXD9" IO - - 
      P110 35 SPI0_MISO0 - M None "Peripheral mode" - - "AGT3: AGTEE3; GPT1: GTIOC1B; ICU: IRQ3; JTAG/SWD: TDI; SCI2: CTS_RTS2; SCI9: RXD9; SPI0: MISO0" "(SPI0_MISO), RXD9" IO - - 
      P111 36 SPI0_RSPCK0 - L None "Peripheral mode" - - "AGT5: AGTOA5; ICU: IRQ4; SCI2: SCK2; SCI9: SCK9; SPI0: RSPCK0" "SPI0_SCK (as SCKI)" IO - - 
      P112 37 GPIO - L - "Output mode (Initial High)" - - "AGT5: AGTOB5; QSPI: QSSL; SCI1: SCK1; SCI2: TXD2; SPI0: SSLA0" QSPI_CS IO - - 
      P113 38 GPIO - L - "Output mode (Initial High)" - - "AGT5: AGTEE5; GPT2: GTIOC2A; SCI2: RXD2" LED3 IO - - 
      P200 27 - - - - Disabled - - "ICU: NMI" - None - - 
      P201 26 - - - - Disabled - - "SYSTEM: MD" - None - - 
      P205 23 SPI0_SSLA0 - L IRQ1-DS "Peripheral mode" - - "AGT1: AGTO1; CGC: CLKOUT; GPT4: GTIOC4A; ICU: IRQ1-DS; IIC1: SCL1; SCI4: TXD4; SCI9: CTS_RTS9; SPI0: SSLA0; USB FS: USB_OVRCURA_A-DS" SPI0_SSL IO - - 
      P206 22 SCI4_RXD4 - L None "Peripheral mode" - - "ICU: IRQ0-DS; IIC1: SDA1; SCI4: RXD4; SCI9: CTS9; SPI0: SSLA1; USB FS: USB_VBUSEN" VCOM_TXD I - - 
      P207 21 SCI4_TXD4 - L - "Peripheral mode" - - "QSPI: QSSL; SCI4: TXD4; SPI0: SSLA2" VCOM_RXD O - - 
      P208 24 GPIO - - - "Input mode" - - "QSPI: QIO3; TRACE: TRDATA3" "PMOD IO3" IO - - 
      P212 10 - - - - Disabled - - "AGT1: AGTEE1; CGC: EXTAL; GPT_POEGD: GTETRGD; ICU: IRQ3; SCI1: RXD1" - None - - 
      P213 9 - - - - Disabled - - "AGT2: AGTEE2; CGC: XTAL; GPT_POEGC: GTETRGC; ICU: IRQ2; SCI1: TXD1" - None - - 
      P300 32 JTAG/SWD_SWCLK - L - "Peripheral mode" - - "JTAG/SWD: SWCLK; JTAG/SWD: TCK; SPI0: SSLA1" SWD_SWCLK IO - - 
      P301 31 GPT4_GTIOC4B - L None "Peripheral mode" - - "AGT0: AGTIO0; GPT4: GTIOC4B; ICU: IRQ6; SCI2: RXD2; SCI9: CTS_RTS9; SPI0: SSLA2" I2S_WS IO - - 
      P302 30 - - - - Disabled - - "GPT4: GTIOC4A; ICU: IRQ5; SCI2: TXD2; SPI0: SSLA3" "PMOD IRQ" None - - 
      P303 29 GPIO - - - "Input mode" - - "GPT7: GTIOC7B; SCI9: CTS9" "PMOD IO1" IO - - 
      P304 28 GPIO - - None "Input mode" - - "AGT2: AGTEE2; GPT7: GTIOC7A; ICU: IRQ9" "PMOD IO2" IO - - 
      P400 1 GPT6_GTIOC6A - L None "Peripheral mode" - - "AGT1: AGTIO1; GPT6: GTIOC6A; ICU: IRQ0; IIC0: SCL0; SCI4: SCK4" LED2 IO - - 
      P401 2 - - - - Disabled - - "CAN0: CTX0; GPT6: GTIOC6B; GPT_POEGA: GTETRGA; ICU: IRQ5-DS; IIC0: SDA0; SCI4: CTS_RTS4" - None - - 
      P402 3 - - - - Disabled - - "AGT0: AGTIO0; AGT1: AGTIO1; AGT2: AGTIO2; AGT3: AGTIO3; CAC: CACREF; CAN0: CRX0; ICU: IRQ4-DS; RTC: RTCIC0; SCI4: CTS4" "USER SW" None - - 
      P407 16 "USB FS_USB_VBUS" - L - "Peripheral mode" - - "ADC0: ADTRG0; AGT0: AGTIO0; GPT6: GTIOC6A; IIC0: SDA0; RTC: RTCOUT; SCI4: CTS_RTS4; SPI0: SSLA3; USB FS: USB_VBUS" "USB VBUS" IO - - 
      P408 15 SCI3_RXD3 - L None "Peripheral mode" - - "AGT2: AGTOB2; GPT6: GTIOC6B; ICU: IRQ7; IIC0: SCL0; SCI3: RXD3; SCI4: CTS4; USB FS: USB_ID" SCI3_RXD3 I - - 
      P409 14 SCI3_TXD3 - L None "Peripheral mode" - - "AGT2: AGTOA2; ICU: IRQ6; SCI3: TXD3; USB FS: USB_EXICEN" SCI3_TXD3 O - - 
      P410 13 SCI3_SCK3 - L None "Peripheral mode" - - "AGT1: AGTOB1; ICU: IRQ5; SCI0: RXD0; SCI3: SCK3; SPI1: MISO1" SCI3_SCK3 IO - - 
      P411 12 SCI3_CTS_RTS3 - L None "Peripheral mode" - - "AGT1: AGTOA1; ICU: IRQ4; SCI0: TXD0; SCI3: CTS_RTS3; SPI1: MOSI1" SCI3_CTS_RTS3 IO - - 
      P500 49 GPIO - L - "Output mode (Initial High)" - - "AGT0: AGTOA0; CAC: CACREF; QSPI: QSPCLK; USB FS: USB_VBUSEN" LED1 IO - - 
      RES 25 SYSTEM_RES - - - - - - - - IO "Read only" - 
      USB_DM 18 SYSTEM_USB_DM - - - - - - - - IO "Read only" - 
      USB_DP 19 SYSTEM_USB_DP - - - - - - - - IO "Read only" - 
      VBATT 4 SYSTEM_VBATT - - - - - - - - IO "Read only" - 
      VCC 50 SYSTEM_VCC - - - - - - - - IO "Read only" - 
      VCC 11 SYSTEM_VCC - - - - - - - - IO "Read only" - 
      VCC 39 SYSTEM_VCC - - - - - - - - IO "Read only" - 
      VCC_USB 20 SYSTEM_VCC_USB - - - - - - - - IO "Read only" - 
      VCL 41 SYSTEM_VCL - - - - - - - - IO "Read only" - 
      VCL0 5 SYSTEM_VCL0 - - - - - - - - IO "Read only" - 
      VREFH 55 SYSTEM_VREFH - - - - - - - - IO "Read only" - 
      VREFH0 59 SYSTEM_VREFH0 - - - - - - - - IO "Read only" - 
      VREFL 54 SYSTEM_VREFL - - - - - - - - IO "Read only" - 
      VREFL0 58 SYSTEM_VREFL0 - - - - - - - - IO "Read only" - 
      VSS 51 SYSTEM_VSS - - - - - - - - IO "Read only" - 
      VSS 8 SYSTEM_VSS - - - - - - - - IO "Read only" - 
      VSS 40 SYSTEM_VSS - - - - - - - - IO "Read only" - 
      VSS_USB 17 SYSTEM_VSS_USB - - - - - - - - IO "Read only" - 
      XCIN 6 CGC_XCIN - - - - - - - - IO "Read only" - 
      XCOUT 7 CGC_XCOUT - - - - - - - - IO "Read only" - 
    VOICE_RA6E1_QSPI.pincfg -> 
      AVCC0 56 SYSTEM_AVCC0 - - - - - - - - IO "Read only" - 
      AVSS0 57 SYSTEM_AVSS0 - - - - - - - - IO "Read only" - 
      P000 64 ADC0_AN000 - - - "Analog mode" - - "ADC0: AN000; ICU: IRQ6-DS" AMIC_L I - - 
      P001 63 ADC0_AN001 - - - "Analog mode" - - "ADC0: AN001; ICU: IRQ7-DS" AMIC_R I - - 
      P002 62 - - - - Disabled - - "ADC0: AN002; ICU: IRQ8-DS" - None - - 
      P003 61 - - - - Disabled - - "ADC0: AN003" - None - - 
      P004 60 - - - - Disabled - - "ADC0: AN004; ICU: IRQ9-DS" - None - - 
      P014 53 DAC120_DA0 - - - "Analog mode" - - "ADC0: AN012; DAC120: DA0" PLAYBACK O - - 
      P015 52 - - - - Disabled - - "ADC0: AN013; ICU: IRQ13" - None - - 
      P100 48 QSPI_QSPCLK - L None "Peripheral mode" - - "AGT0: AGTIO0; GPT5: GTIOC5B; GPT_POEGA: GTETRGA; ICU: IRQ2; QSPI: QSPCLK; SCI0: RXD0; SCI1: SCK1; SPI1: MISO1" "QSPI_CLK / (SPI1_MISO)" IO - - 
      P101 47 QSPI_QIO1 - M None "Peripheral mode" - - "AGT0: AGTEE0; GPT5: GTIOC5A; GPT_POEGB: GTETRGB; ICU: IRQ1; QSPI: QIO1; SCI0: TXD0; SCI1: CTS_RTS1; SPI1: MOSI1" "QSPI_DQ1 / SPI1_MOSI (DMIC_R)" IO - - 
      P102 46 QSPI_QIO0 - L - "Peripheral mode" - - "ADC0: ADTRG0; AGT0: AGTO0; CAN0: CRX0; GPT2: GTIOC2B; QSPI: QIO0; SCI0: SCK0; SPI1: RSPCK1" "QSPI_DQ0 / SPI1_SCK" IO - - 
      P103 45 QSPI_QIO3 - L - "Peripheral mode" - - "AGT2: AGTIO2; CAN0: CTX0; GPT2: GTIOC2A; QSPI: QIO3; SCI0: CTS_RTS0; SPI1: SSLB0" "QSPI_DQ3 / SPI1_SSL" IO - - 
      P104 44 QSPI_QIO2 - - - "Peripheral mode" - - "AGT2: AGTEE2; GPT1: GTIOC1B; GPT_POEGB: GTETRGB; ICU: IRQ1; QSPI: QIO2; SPI1: SSLB1" QSPI_DQ2 None - - 
      P105 43 GPT1_GTIOC1A - L None "Peripheral mode" - - "AGT2: AGTO2; GPT1: GTIOC1A; GPT_POEGA: GTETRGA; ICU: IRQ0; SPI1: SSLB2" "SCKO (as I2S_CLK)" IO - - 
      P106 42 - - - - Disabled - - "AGT0: AGTOB0; SPI1: SSLB3" - None - - 
      P108 33 JTAG/SWD_SWDIO - L - "Peripheral mode" - - "AGT3: AGTOA3; JTAG/SWD: SWDIO; JTAG/SWD: TMS; SCI9: CTS_RTS9; SPI0: SSLA0" SWD_SWDIO IO - - 
      P109 34 SPI0_MOSI0 - M - "Peripheral mode" - - "AGT3: AGTOB3; CGC: CLKOUT; GPT1: GTIOC1A; JTAG/SWD: TDO; JTAG/SWD: TRACESWO; SCI9: TXD9; SPI0: MOSI0" "SPI0_MOSI (DMIC_L), TXD9" IO - - 
      P110 35 SPI0_MISO0 - M None "Peripheral mode" - - "AGT3: AGTEE3; GPT1: GTIOC1B; ICU: IRQ3; JTAG/SWD: TDI; SCI2: CTS_RTS2; SCI9: RXD9; SPI0: MISO0" "(SPI0_MISO), RXD9" IO - - 
      P111 36 SPI0_RSPCK0 - L None "Peripheral mode" - - "AGT5: AGTOA5; ICU: IRQ4; SCI2: SCK2; SCI9: SCK9; SPI0: RSPCK0" "SPI0_SCK (as SCKI)" IO - - 
      P112 37 QSPI_QSSL - L - "Peripheral mode" - - "AGT5: AGTOB5; QSPI: QSSL; SCI1: SCK1; SCI2: TXD2; SPI0: SSLA0" QSPI_CS IO - - 
      P113 38 GPT2_GTIOC2A - L - "Peripheral mode" - - "AGT5: AGTEE5; GPT2: GTIOC2A; SCI2: RXD2" LED3 IO - - 
      P200 27 - - - - Disabled - - "ICU: NMI" - None - - 
      P201 26 - - - - Disabled - - "SYSTEM: MD" - None - - 
      P205 23 SPI0_SSLA0 - L IRQ1-DS "Peripheral mode" - - "AGT1: AGTO1; CGC: CLKOUT; GPT4: GTIOC4A; ICU: IRQ1-DS; IIC1: SCL1; SCI4: TXD4; SCI9: CTS_RTS9; SPI0: SSLA0; USB FS: USB_OVRCURA_A-DS" SPI0_SSL IO - - 
      P206 22 SCI4_RXD4 - L None "Peripheral mode" - - "ICU: IRQ0-DS; IIC1: SDA1; SCI4: RXD4; SCI9: CTS9; SPI0: SSLA1; USB FS: USB_VBUSEN" VCOM_TXD I - - 
      P207 21 SCI4_TXD4 - L - "Peripheral mode" - - "QSPI: QSSL; SCI4: TXD4; SPI0: SSLA2" VCOM_RXD O - - 
      P208 24 GPIO - - - "Input mode" - - "QSPI: QIO3; TRACE: TRDATA3" "PMOD IO3" IO - - 
      P212 10 - - - - Disabled - - "AGT1: AGTEE1; CGC: EXTAL; GPT_POEGD: GTETRGD; ICU: IRQ3; SCI1: RXD1" - None - - 
      P213 9 - - - - Disabled - - "AGT2: AGTEE2; CGC: XTAL; GPT_POEGC: GTETRGC; ICU: IRQ2; SCI1: TXD1" - None - - 
      P300 32 JTAG/SWD_SWCLK - L - "Peripheral mode" - - "JTAG/SWD: SWCLK; JTAG/SWD: TCK; SPI0: SSLA1" SWD_SWCLK IO - - 
      P301 31 GPT4_GTIOC4B - L None "Peripheral mode" - - "AGT0: AGTIO0; GPT4: GTIOC4B; ICU: IRQ6; SCI2: RXD2; SCI9: CTS_RTS9; SPI0: SSLA2" I2S_WS IO - - 
      P302 30 - - - - Disabled - - "GPT4: GTIOC4A; ICU: IRQ5; SCI2: TXD2; SPI0: SSLA3" "PMOD IRQ" None - - 
      P303 29 GPIO - - - "Input mode" - - "GPT7: GTIOC7B; SCI9: CTS9" "PMOD IO1" IO - - 
      P304 28 GPIO - - None "Input mode" - - "AGT2: AGTEE2; GPT7: GTIOC7A; ICU: IRQ9" "PMOD IO2" IO - - 
      P400 1 GPT6_GTIOC6A - L None "Peripheral mode" - - "AGT1: AGTIO1; GPT6: GTIOC6A; ICU: IRQ0; IIC0: SCL0; SCI4: SCK4" LED2 IO - - 
      P401 2 - - - - Disabled - - "CAN0: CTX0; GPT6: GTIOC6B; GPT_POEGA: GTETRGA; ICU: IRQ5-DS; IIC0: SDA0; SCI4: CTS_RTS4" - None - - 
      P402 3 - - - - Disabled - - "AGT0: AGTIO0; AGT1: AGTIO1; AGT2: AGTIO2; AGT3: AGTIO3; CAC: CACREF; CAN0: CRX0; ICU: IRQ4-DS; RTC: RTCIC0; SCI4: CTS4" "USER SW" None - - 
      P407 16 "USB FS_USB_VBUS" - L - "Peripheral mode" - - "ADC0: ADTRG0; AGT0: AGTIO0; GPT6: GTIOC6A; IIC0: SDA0; RTC: RTCOUT; SCI4: CTS_RTS4; SPI0: SSLA3; USB FS: USB_VBUS" "USB VBUS" IO - - 
      P408 15 SCI3_RXD3 - L None "Peripheral mode" - - "AGT2: AGTOB2; GPT6: GTIOC6B; ICU: IRQ7; IIC0: SCL0; SCI3: RXD3; SCI4: CTS4; USB FS: USB_ID" SCI3_RXD3 I - - 
      P409 14 SCI3_TXD3 - L None "Peripheral mode" - - "AGT2: AGTOA2; ICU: IRQ6; SCI3: TXD3; USB FS: USB_EXICEN" SCI3_TXD3 O - - 
      P410 13 SCI3_SCK3 - L None "Peripheral mode" - - "AGT1: AGTOB1; ICU: IRQ5; SCI0: RXD0; SCI3: SCK3; SPI1: MISO1" SCI3_SCK3 IO - - 
      P411 12 SCI3_CTS_RTS3 - L None "Peripheral mode" - - "AGT1: AGTOA1; ICU: IRQ4; SCI0: TXD0; SCI3: CTS_RTS3; SPI1: MOSI1" SCI3_CTS_RTS3 IO - - 
      P500 49 GPIO - L - "Output mode (Initial High)" - - "AGT0: AGTOA0; CAC: CACREF; QSPI: QSPCLK; USB FS: USB_VBUSEN" LED1 IO - - 
      RES 25 SYSTEM_RES - - - - - - - - IO "Read only" - 
      USB_DM 18 SYSTEM_USB_DM - - - - - - - - IO "Read only" - 
      USB_DP 19 SYSTEM_USB_DP - - - - - - - - IO "Read only" - 
      VBATT 4 SYSTEM_VBATT - - - - - - - - IO "Read only" - 
      VCC 50 SYSTEM_VCC - - - - - - - - IO "Read only" - 
      VCC 11 SYSTEM_VCC - - - - - - - - IO "Read only" - 
      VCC 39 SYSTEM_VCC - - - - - - - - IO "Read only" - 
      VCC_USB 20 SYSTEM_VCC_USB - - - - - - - - IO "Read only" - 
      VCL 41 SYSTEM_VCL - - - - - - - - IO "Read only" - 
      VCL0 5 SYSTEM_VCL0 - - - - - - - - IO "Read only" - 
      VREFH 55 SYSTEM_VREFH - - - - - - - - IO "Read only" - 
      VREFH0 59 SYSTEM_VREFH0 - - - - - - - - IO "Read only" - 
      VREFL 54 SYSTEM_VREFL - - - - - - - - IO "Read only" - 
      VREFL0 58 SYSTEM_VREFL0 - - - - - - - - IO "Read only" - 
      VSS 51 SYSTEM_VSS - - - - - - - - IO "Read only" - 
      VSS 8 SYSTEM_VSS - - - - - - - - IO "Read only" - 
      VSS 40 SYSTEM_VSS - - - - - - - - IO "Read only" - 
      VSS_USB 17 SYSTEM_VSS_USB - - - - - - - - IO "Read only" - 
      XCIN 6 CGC_XCIN - - - - - - - - IO "Read only" - 
      XCOUT 7 CGC_XCOUT - - - - - - - - IO "Read only" - 
    R7FA6E10F2CFP.pincfg -> 
      AVCC0 56 SYSTEM_AVCC0 - - - - - - - - IO "Read only" - 
      AVSS0 57 SYSTEM_AVSS0 - - - - - - - - IO "Read only" - 
      P000 64 - - - - Disabled - - "ADC0: AN000; ICU: IRQ6-DS" AMIC_L I - - 
      P001 63 - - - - Disabled - - "ADC0: AN001; ICU: IRQ7-DS" AMIC_R I - - 
      P002 62 - - - - Disabled - - "ADC0: AN002; ICU: IRQ8-DS" - None - - 
      P003 61 - - - - Disabled - - "ADC0: AN003" - None - - 
      P004 60 - - - - Disabled - - "ADC0: AN004; ICU: IRQ9-DS" - None - - 
      P014 53 - - - - Disabled - - "ADC0: AN012; DAC120: DA0" PLAYBACK O - - 
      P015 52 - - - - Disabled - - "ADC0: AN013; ICU: IRQ13" - None - - 
      P100 48 - - L None Disabled - - "AGT0: AGTIO0; GPT5: GTIOC5B; GPT_POEGA: GTETRGA; ICU: IRQ2; QSPI: QSPCLK; SCI0: RXD0; SCI1: SCK1; SPI1: MISO1" "QSPI_CLK / (SPI1_MISO)" IO - - 
      P101 47 - - L None Disabled - - "AGT0: AGTEE0; GPT5: GTIOC5A; GPT_POEGB: GTETRGB; ICU: IRQ1; QSPI: QIO1; SCI0: TXD0; SCI1: CTS_RTS1; SPI1: MOSI1" "QSPI_DQ1 / SPI1_MOSI (DMIC_R)" IO - - 
      P102 46 - - L - Disabled - - "ADC0: ADTRG0; AGT0: AGTO0; CAN0: CRX0; GPT2: GTIOC2B; QSPI: QIO0; SCI0: SCK0; SPI1: RSPCK1" "QSPI_DQ0 / SPI1_SCK" IO - - 
      P103 45 - - L - Disabled - - "AGT2: AGTIO2; CAN0: CTX0; GPT2: GTIOC2A; QSPI: QIO3; SCI0: CTS_RTS0; SPI1: SSLB0" "QSPI_DQ3 / SPI1_SSL" IO - - 
      P104 44 - - - - Disabled - - "AGT2: AGTEE2; GPT1: GTIOC1B; GPT_POEGB: GTETRGB; ICU: IRQ1; QSPI: QIO2; SPI1: SSLB1" QSPI_DQ2 None - - 
      P105 43 - - L None Disabled - - "AGT2: AGTO2; GPT1: GTIOC1A; GPT_POEGA: GTETRGA; ICU: IRQ0; SPI1: SSLB2" "SCKO (as I2S_CLK)" IO - - 
      P106 42 - - - - Disabled - - "AGT0: AGTOB0; SPI1: SSLB3" - None - - 
      P108 33 JTAG/SWD_TMS - L - "Peripheral mode" - - "AGT3: AGTOA3; JTAG/SWD: SWDIO; JTAG/SWD: TMS; SCI9: CTS_RTS9; SPI0: SSLA0" SWD_SWDIO IO - - 
      P109 34 JTAG/SWD_TDO - L - "Peripheral mode" - - "AGT3: AGTOB3; CGC: CLKOUT; GPT1: GTIOC1A; JTAG/SWD: TDO; JTAG/SWD: TRACESWO; SCI9: TXD9; SPI0: MOSI0" "SPI0_MOSI (DMIC_L), TXD9" IO - - 
      P110 35 JTAG/SWD_TDI - L None "Peripheral mode" - - "AGT3: AGTEE3; GPT1: GTIOC1B; ICU: IRQ3; JTAG/SWD: TDI; SCI2: CTS_RTS2; SCI9: RXD9; SPI0: MISO0" "(SPI0_MISO), RXD9" IO - - 
      P111 36 - - L None Disabled - - "AGT5: AGTOA5; ICU: IRQ4; SCI2: SCK2; SCI9: SCK9; SPI0: RSPCK0" "SPI0_SCK (as SCKI)" IO - - 
      P112 37 - - L - Disabled - - "AGT5: AGTOB5; QSPI: QSSL; SCI1: SCK1; SCI2: TXD2; SPI0: SSLA0" QSPI_CS IO - - 
      P113 38 - - L - Disabled - - "AGT5: AGTEE5; GPT2: GTIOC2A; SCI2: RXD2" LED3 IO - - 
      P200 27 - - - - Disabled - - "ICU: NMI" - None - - 
      P201 26 - - - - Disabled - - "SYSTEM: MD" - None - - 
      P205 23 - - L None Disabled - - "AGT1: AGTO1; CGC: CLKOUT; GPT4: GTIOC4A; ICU: IRQ1-DS; IIC1: SCL1; SCI4: TXD4; SCI9: CTS_RTS9; SPI0: SSLA0; USB FS: USB_OVRCURA_A-DS" SPI0_SSL IO - - 
      P206 22 - - L None Disabled - - "ICU: IRQ0-DS; IIC1: SDA1; SCI4: RXD4; SCI9: CTS9; SPI0: SSLA1; USB FS: USB_VBUSEN" VCOM_TXD I - - 
      P207 21 - - L - Disabled - - "QSPI: QSSL; SCI4: TXD4; SPI0: SSLA2" VCOM_RXD O - - 
      P208 24 - - - - Disabled - - "QSPI: QIO3; TRACE: TRDATA3" "PMOD IO3" IO - - 
      P212 10 - - - - Disabled - - "AGT1: AGTEE1; CGC: EXTAL; GPT_POEGD: GTETRGD; ICU: IRQ3; SCI1: RXD1" - None - - 
      P213 9 - - - - Disabled - - "AGT2: AGTEE2; CGC: XTAL; GPT_POEGC: GTETRGC; ICU: IRQ2; SCI1: TXD1" - None - - 
      P300 32 JTAG/SWD_TCK - L - "Peripheral mode" - - "JTAG/SWD: SWCLK; JTAG/SWD: TCK; SPI0: SSLA1" SWD_SWCLK IO - - 
      P301 31 - - L None Disabled - - "AGT0: AGTIO0; GPT4: GTIOC4B; ICU: IRQ6; SCI2: RXD2; SCI9: CTS_RTS9; SPI0: SSLA2" I2S_WS IO - - 
      P302 30 - - - - Disabled - - "GPT4: GTIOC4A; ICU: IRQ5; SCI2: TXD2; SPI0: SSLA3" "PMOD IRQ" None - - 
      P303 29 - - - - Disabled - - "GPT7: GTIOC7B; SCI9: CTS9" "PMOD IO1" IO - - 
      P304 28 - - - None Disabled - - "AGT2: AGTEE2; GPT7: GTIOC7A; ICU: IRQ9" "PMOD IO2" IO - - 
      P400 1 - - L None Disabled - - "AGT1: AGTIO1; GPT6: GTIOC6A; ICU: IRQ0; IIC0: SCL0; SCI4: SCK4" LED2 IO - - 
      P401 2 - - - - Disabled - - "CAN0: CTX0; GPT6: GTIOC6B; GPT_POEGA: GTETRGA; ICU: IRQ5-DS; IIC0: SDA0; SCI4: CTS_RTS4" - None - - 
      P402 3 - - - - Disabled - - "AGT0: AGTIO0; AGT1: AGTIO1; AGT2: AGTIO2; AGT3: AGTIO3; CAC: CACREF; CAN0: CRX0; ICU: IRQ4-DS; RTC: RTCIC0; SCI4: CTS4" "USER SW" None - - 
      P407 16 - - L - Disabled - - "ADC0: ADTRG0; AGT0: AGTIO0; GPT6: GTIOC6A; IIC0: SDA0; RTC: RTCOUT; SCI4: CTS_RTS4; SPI0: SSLA3; USB FS: USB_VBUS" "USB VBUS" IO - - 
      P408 15 - - L None Disabled - - "AGT2: AGTOB2; GPT6: GTIOC6B; ICU: IRQ7; IIC0: SCL0; SCI3: RXD3; SCI4: CTS4; USB FS: USB_ID" SCI3_RXD3 I - - 
      P409 14 - - L None Disabled - - "AGT2: AGTOA2; ICU: IRQ6; SCI3: TXD3; USB FS: USB_EXICEN" SCI3_TXD3 O - - 
      P410 13 - - L None Disabled - - "AGT1: AGTOB1; ICU: IRQ5; SCI0: RXD0; SCI3: SCK3; SPI1: MISO1" SCI3_SCK3 IO - - 
      P411 12 - - L None Disabled - - "AGT1: AGTOA1; ICU: IRQ4; SCI0: TXD0; SCI3: CTS_RTS3; SPI1: MOSI1" SCI3_CTS_RTS3 IO - - 
      P500 49 - - L - Disabled - - "AGT0: AGTOA0; CAC: CACREF; QSPI: QSPCLK; USB FS: USB_VBUSEN" LED1 IO - - 
      RES 25 SYSTEM_RES - - - - - - - - IO "Read only" - 
      USB_DM 18 SYSTEM_USB_DM - - - - - - - - IO "Read only" - 
      USB_DP 19 SYSTEM_USB_DP - - - - - - - - IO "Read only" - 
      VBATT 4 SYSTEM_VBATT - - - - - - - - IO "Read only" - 
      VCC 50 SYSTEM_VCC - - - - - - - - IO "Read only" - 
      VCC 11 SYSTEM_VCC - - - - - - - - IO "Read only" - 
      VCC 39 SYSTEM_VCC - - - - - - - - IO "Read only" - 
      VCC_USB 20 SYSTEM_VCC_USB - - - - - - - - IO "Read only" - 
      VCL 41 SYSTEM_VCL - - - - - - - - IO "Read only" - 
      VCL0 5 SYSTEM_VCL0 - - - - - - - - IO "Read only" - 
      VREFH 55 SYSTEM_VREFH - - - - - - - - IO "Read only" - 
      VREFH0 59 SYSTEM_VREFH0 - - - - - - - - IO "Read only" - 
      VREFL 54 SYSTEM_VREFL - - - - - - - - IO "Read only" - 
      VREFL0 58 SYSTEM_VREFL0 - - - - - - - - IO "Read only" - 
      VSS 51 SYSTEM_VSS - - - - - - - - IO "Read only" - 
      VSS 8 SYSTEM_VSS - - - - - - - - IO "Read only" - 
      VSS 40 SYSTEM_VSS - - - - - - - - IO "Read only" - 
      VSS_USB 17 SYSTEM_VSS_USB - - - - - - - - IO "Read only" - 
      XCIN 6 CGC_XCIN - - - - - - - - IO "Read only" - 
      XCOUT 7 CGC_XCOUT - - - - - - - - IO "Read only" - 
    
  User Events
    
  User Event Links
    
  Module "I/O Port (r_ioport)"
    Parameter Checking: Default (BSP)
    
  Module "SPI (r_spi)"
    Parameter Checking: Default (BSP)
    Enable Support for using a transfer API: Enabled
    Enable Transmitting from RXI Interrupt: Disabled
    
  Module "Transfer (r_dtc)"
    Parameter Checking: Default (BSP)
    Linker section to keep DTC vector table: .fsp_dtc_vector_table
    
  Module "Timer, General PWM (r_gpt)"
    Parameter Checking: Default (BSP)
    Pin Output Support: Enabled
    Write Protect Enable: Disabled
    
  Module "Event Link Controller (r_elc)"
    Parameter Checking: Default (BSP)
    
  Module "Data Shipper (rm_rai_data_shipper)"
    Parameter Checking: Default (BSP)
    Max Number Of DC Instances: 8
    
  Module "Data Collector (rm_rai_data_collector)"
    Parameter Checking: Default (BSP)
    Max Number Of Channels: 16
    
  Module "UART Communication Device (rm_comms_uart)"
    Parameter Checking: Default (BSP)
    
  Module "UART (r_sci_uart)"
    Parameter Checking: Default (BSP)
    FIFO Support: Disable
    DTC Support: Disable
    Flow Control Support: Disable
    RS-485 Support: Disable
    IrDA Support: Disabled
    
  Module "CRC (r_crc)"
    Parameter Checking: Default (BSP)
    
  HAL
    Instance "g_ioport I/O Port (r_ioport)"
      Name: g_ioport
      1st Port ELC Trigger Source: Disabled
      2nd Port ELC Trigger Source: Disabled
      3rd Port ELC Trigger Source: Disabled
      4th Port ELC Trigger Source: Disabled
      Pin Configuration Name: g_bsp_pin_cfg
      
    Instance "g_spi0 SPI (r_spi)"
      Name: g_spi0
      Channel: 0
      Receive Interrupt Priority: Priority 2
      Transmit Buffer Empty Interrupt Priority: Priority 2
      Transfer Complete Interrupt Priority: Priority 2
      Error Interrupt Priority: Priority 2
      Operating Mode: Slave
      Clock Phase: Data sampling on odd edge, data variation on even edge
      Clock Polarity: Low when idle
      Mode Fault Error: Disable
      Bit Order: MSB First
      Callback: g_spi0_cb
      SPI Mode: SPI Operation
      Full or Transmit Only Mode: Full Duplex
      Slave Select Polarity: Active Low
      Select SSL(Slave Select): SSL0
      MOSI Idle State: MOSI Idle Value Fixing Disable
      Parity Mode: Disabled
      Byte Swapping: Disable
      Bitrate: 16000000
      Clock Delay: 1 Clock
      SSL Negation Delay: 1 Clock
      Next Access Delay: 1 Clock
      
      Instance "g_transfer0 Transfer (r_dtc) SPI0 TXI (Transmit buffer empty)"
        Name: g_transfer0
        Mode: Normal
        Transfer Size: 2 Bytes
        Destination Address Mode: Fixed
        Source Address Mode: Incremented
        Repeat Area (Unused in Normal Mode): Source
        Interrupt Frequency: After all transfers have completed
        Number of Transfers: 0
        Number of Blocks (Valid only in Block Mode): 0
        Number of Transfer Descriptors: 1
        Activation Source: SPI0 TXI (Transmit buffer empty)
        
      Instance "g_transfer1 Transfer (r_dtc) SPI0 RXI (Receive buffer full)"
        Name: g_transfer1
        Mode: Normal
        Transfer Size: 2 Bytes
        Destination Address Mode: Incremented
        Source Address Mode: Fixed
        Repeat Area (Unused in Normal Mode): Destination
        Interrupt Frequency: After all transfers have completed
        Number of Transfers: 0
        Number of Blocks (Valid only in Block Mode): 0
        Number of Transfer Descriptors: 1
        Activation Source: SPI0 RXI (Receive buffer full)
        
    Instance "g_timer_bclk Timer, General PWM (r_gpt)"
      General: Name: g_timer_bclk
      General: Channel: 1
      General: Mode: Periodic
      General: Period: 1
      General: Compare Match: Compare Match A: Status: Disabled
      General: Compare Match: Compare Match A: Compare match value: 0
      General: Compare Match: Compare Match B: Status: Disabled
      General: Compare Match: Compare Match B: Compare match value: 0
      General: Period Unit: Hertz
      Output: Custom Waveform: GTIOA: Initial Output Level: Pin Level Low
      Output: Custom Waveform: GTIOA: Cycle End Output Level: Pin Level Retain
      Output: Custom Waveform: GTIOA: Compare Match Output Level: Pin Level Retain
      Output: Custom Waveform: GTIOA: Retain Output Level at Count Stop: Disabled
      Output: Custom Waveform: GTIOB: Initial Output Level: Pin Level Low
      Output: Custom Waveform: GTIOB: Cycle End Output Level: Pin Level Retain
      Output: Custom Waveform: GTIOB: Compare Match Output Level: Pin Level Retain
      Output: Custom Waveform: GTIOB: Retain Output Level at Count Stop: Disabled
      Output: Custom Waveform: Custom Waveform Enable: Disabled
      Output: Duty Cycle Percent (only applicable in PWM mode): 50
      Output: GTIOCA Output Enabled: True
      Output: GTIOCA Stop Level: Pin Level Low
      Output: GTIOCB Output Enabled: False
      Output: GTIOCB Stop Level: Pin Level Low
      Input: Count Up Source: 
      Input: Count Down Source: 
      Input: Start Source: 
      Input: Stop Source: 
      Input: Clear Source: 
      Input: Capture A Source: 
      Input: Capture B Source: 
      Input: Noise Filter A Sampling Clock Select: No Filter
      Input: Noise Filter B Sampling Clock Select: No Filter
      Interrupts: Callback: NULL
      Interrupts: Overflow/Crest Interrupt Priority: Disabled
      Interrupts: Capture/Compare match A Interrupt Priority: Disabled
      Interrupts: Capture/Compare match B Interrupt Priority: Disabled
      Interrupts: Underflow/Trough Interrupt Priority: Disabled
      Extra Features: Extra Features: Disabled
      Extra Features: Output Disable: POEG Link: POEG Channel 0
      Extra Features: Output Disable: Output Disable POEG Trigger: 
      Extra Features: ADC Trigger: Start Event Trigger (Channels with GTINTAD only): 
      Extra Features: ADC Trigger: ADC A Compare Match (Raw Counts): 0
      Extra Features: ADC Trigger: ADC B Compare Match (Raw Counts): 0
      Extra Features: Dead Time (Value range varies with Channel): Dead Time Count Up (Raw Counts): 0
      Extra Features: Dead Time (Value range varies with Channel): Dead Time Count Down (Raw Counts) (Channels with GTDVD only): 0
      Extra Features: Interrupt Skipping (Channels with GTITC only): Interrupt to Count: None
      Extra Features: Interrupt Skipping (Channels with GTITC only): Interrupt Skip Count: 0
      Extra Features: Interrupt Skipping (Channels with GTITC only): Skip ADC Events: None
      Extra Features: Output Disable: GTIOCA Disable Setting: Disable Prohibited
      Extra Features: Output Disable: GTIOCB Disable Setting: Disable Prohibited
      
    Instance "g_timer_ws Timer, General PWM (r_gpt)"
      General: Name: g_timer_ws
      General: Channel: 4
      General: Mode: Saw-wave PWM
      General: Period: 32
      General: Compare Match: Compare Match A: Status: Disabled
      General: Compare Match: Compare Match A: Compare match value: 0
      General: Compare Match: Compare Match B: Status: Disabled
      General: Compare Match: Compare Match B: Compare match value: 0
      General: Period Unit: Raw Counts
      Output: Custom Waveform: GTIOA: Initial Output Level: Pin Level Low
      Output: Custom Waveform: GTIOA: Cycle End Output Level: Pin Level Retain
      Output: Custom Waveform: GTIOA: Compare Match Output Level: Pin Level Retain
      Output: Custom Waveform: GTIOA: Retain Output Level at Count Stop: Disabled
      Output: Custom Waveform: GTIOB: Initial Output Level: Pin Level High
      Output: Custom Waveform: GTIOB: Cycle End Output Level: Pin Level Retain
      Output: Custom Waveform: GTIOB: Compare Match Output Level: Pin Level Toggle
      Output: Custom Waveform: GTIOB: Retain Output Level at Count Stop: Disabled
      Output: Custom Waveform: Custom Waveform Enable: Enabled
      Output: Duty Cycle Percent (only applicable in PWM mode): 50
      Output: GTIOCA Output Enabled: False
      Output: GTIOCA Stop Level: Pin Level Low
      Output: GTIOCB Output Enabled: True
      Output: GTIOCB Stop Level: Pin Level Low
      Input: Count Up Source: GPT1 COUNTER OVERFLOW (Overflow)
      Input: Count Down Source: 
      Input: Start Source: 
      Input: Stop Source: 
      Input: Clear Source: 
      Input: Capture A Source: 
      Input: Capture B Source: 
      Input: Noise Filter A Sampling Clock Select: No Filter
      Input: Noise Filter B Sampling Clock Select: No Filter
      Interrupts: Callback: NULL
      Interrupts: Overflow/Crest Interrupt Priority: Disabled
      Interrupts: Capture/Compare match A Interrupt Priority: Disabled
      Interrupts: Capture/Compare match B Interrupt Priority: Disabled
      Interrupts: Underflow/Trough Interrupt Priority: Disabled
      Extra Features: Extra Features: Disabled
      Extra Features: Output Disable: POEG Link: POEG Channel 0
      Extra Features: Output Disable: Output Disable POEG Trigger: 
      Extra Features: ADC Trigger: Start Event Trigger (Channels with GTINTAD only): 
      Extra Features: ADC Trigger: ADC A Compare Match (Raw Counts): 0
      Extra Features: ADC Trigger: ADC B Compare Match (Raw Counts): 0
      Extra Features: Dead Time (Value range varies with Channel): Dead Time Count Up (Raw Counts): 0
      Extra Features: Dead Time (Value range varies with Channel): Dead Time Count Down (Raw Counts) (Channels with GTDVD only): 0
      Extra Features: Interrupt Skipping (Channels with GTITC only): Interrupt to Count: None
      Extra Features: Interrupt Skipping (Channels with GTITC only): Interrupt Skip Count: 0
      Extra Features: Interrupt Skipping (Channels with GTITC only): Skip ADC Events: None
      Extra Features: Output Disable: GTIOCA Disable Setting: Disable Prohibited
      Extra Features: Output Disable: GTIOCB Disable Setting: Disable Prohibited
      
    Instance "g_elc Event Link Controller (r_elc)"
      Name: g_elc
      
    Instance "g_rai_data_shipper0 Data Shipper (rm_rai_data_shipper)"
      Name: g_rai_data_shipper0
      Frame Rate Divider: 0
      Callback: rai_data_shipper0_callback
      
      Instance "g_comms_uart0 UART Communication Device (rm_comms_uart)"
        Name: g_comms_uart0
        RTOS: Write Mutex: Use
        RTOS: Read Mutex: Use
        RTOS: Mutex Timeout: 0xFFFFFFFF
        RTOS: Write Semaphore: Use
        RTOS: Read Semaphore: Use
        RTOS: Semaphore Timeout: 0xFFFFFFFF
        Callback: NULL
        
        Instance "g_uart0 UART (r_sci_uart)"
          General: Name: g_uart0
          General: Channel: 4
          General: Data Bits: 8bits
          General: Parity: None
          General: Stop Bits: 1bit
          Baud: Baud Rate: 921600
          Baud: Baud Rate Modulation: Disabled
          Baud: Max Error (%): 5
          Flow Control: CTS/RTS Selection: Hardware RTS
          Flow Control: Software RTS Port: Disabled
          Flow Control: Software RTS Pin: Disabled
          Extra: Clock Source: Internal Clock
          Extra: Start bit detection: Falling Edge
          Extra: Noise Filter: Disable
          Extra: Receive FIFO Trigger Level: Max
          Extra: IrDA: Enable: Disabled
          Extra: IrDA: RXD Polarity Switching: Normal
          Extra: IrDA: TXD Polarity Switching: Normal
          Extra: RS-485: DE Pin: Disable
          Extra: RS-485: DE Pin Polarity: Active High
          Extra: RS-485: DE Port Number: Disabled
          Extra: RS-485: DE Pin Number: Disabled
          Interrupts: Callback: NULL
          Interrupts: Receive Interrupt Priority: Priority 12
          Interrupts: Transmit Data Empty Interrupt Priority: Priority 12
          Interrupts: Transmit End Interrupt Priority: Priority 12
          Interrupts: Error Interrupt Priority: Priority 12
          
      Instance "g_crc0 CRC (r_crc)"
        Name: g_crc0
        CRC Polynomial: CRC-8
        Bit Order: MSB
        Snoop Address: Not Supported
        
      Instance "g_rai_data_collector0 Data Collector (rm_rai_data_collector)"
        General: Name: g_rai_data_collector0
        General: ID: 0
        General: Frame Buffer Length: 4096
        General: Data Ready Callback: rai_data_collector0_callback
        General: Error Callback: rai_data_collector0_error_callback
        Data Feed Mode: Channels: 1
        Data Feed Mode: Channel 0: Name: dc0_data_feed_ch0
        Data Feed Mode: Channel 0: Data Type: 16-bit Signed
        Data Feed Mode: Channel 1: Name: dc0_data_feed_ch1
        Data Feed Mode: Channel 1: Data Type: 8-bit Unsigned
        Data Feed Mode: Channel 2: Name: dc0_data_feed_ch2
        Data Feed Mode: Channel 2: Data Type: 8-bit Unsigned
        Data Feed Mode: Channel 3: Name: dc0_data_feed_ch3
        Data Feed Mode: Channel 3: Data Type: 8-bit Unsigned
        Data Feed Mode: Channel 4: Name: dc0_data_feed_ch4
        Data Feed Mode: Channel 4: Data Type: 8-bit Unsigned
        Data Feed Mode: Channel 5: Name: dc0_data_feed_ch5
        Data Feed Mode: Channel 5: Data Type: 8-bit Unsigned
        Data Feed Mode: Channel 6: Name: dc0_data_feed_ch6
        Data Feed Mode: Channel 6: Data Type: 8-bit Unsigned
        Data Feed Mode: Channel 7: Name: dc0_data_feed_ch7
        Data Feed Mode: Channel 7: Data Type: 8-bit Unsigned
        Snapshot Mode: Channels: 0
        Snapshot Mode: DTC Transfer Count: 1
        Snapshot Mode: Channel 0: Name: dc0_snapshot_ch0
        Snapshot Mode: Channel 0: Data Type: 8-bit Unsigned
        Snapshot Mode: Channel 1: Name: dc0_snapshot_ch1
        Snapshot Mode: Channel 1: Data Type: 8-bit Unsigned
        Snapshot Mode: Channel 2: Name: dc0_snapshot_ch2
        Snapshot Mode: Channel 2: Data Type: 8-bit Unsigned
        Snapshot Mode: Channel 3: Name: dc0_snapshot_ch3
        Snapshot Mode: Channel 3: Data Type: 8-bit Unsigned
        Snapshot Mode: Channel 4: Name: dc0_snapshot_ch4
        Snapshot Mode: Channel 4: Data Type: 8-bit Unsigned
        Snapshot Mode: Channel 5: Name: dc0_snapshot_ch5
        Snapshot Mode: Channel 5: Data Type: 8-bit Unsigned
        Snapshot Mode: Channel 6: Name: dc0_snapshot_ch6
        Snapshot Mode: Channel 6: Data Type: 8-bit Unsigned
        Snapshot Mode: Channel 7: Name: dc0_snapshot_ch7
        Snapshot Mode: Channel 7: Data Type: 8-bit Unsigned
        
