T4ACC 000:001.384   SEGGER J-Link V7.98g Log File
T4ACC 000:001.663   DLL Compiled: Sep  5 2024 11:46:36
T4ACC 000:001.698   Logging started @ 2025-01-23 22:16
T4ACC 000:001.714   Process: C:\Users\a5137978\.eclipse\com.renesas.platform_15818172\DebugComp\RA\e2-server-gdb.exe
T4ACC 000:001.729 - 1.727ms
T4ACC 000:001.752 JLINK_GetDLLVersion()
T4ACC 000:001.766 - 0.014ms returns 79807
T4ACC 000:009.113 JLINK_OpenEx(...)
T4ACC 000:025.167   Firmware: J-Link OB-RA4M2 compiled Jul  3 2024 17:03:13
T4ACC 000:028.251   Firmware: J-Link OB-RA4M2 compiled Jul  3 2024 17:03:13
T4ACC 000:044.837   Hardware: V1.00
T4ACC 000:044.985   S/N: 1086136413
T4ACC 000:045.070   OEM: SEGGER
T4ACC 000:045.121   Feature(s): None
T4ACC 000:046.176   Bootloader: 2021 May 14
T4ACC 000:046.761   USB speed mode: Full speed (12 MBit/s)
T4ACC 000:047.337   TELNET listener socket opened on port 19021
T4ACC 000:047.743   WEBSRV WEBSRV_Init(): Starting webserver thread(s)
T4ACC 000:048.115   WEBSRV Webserver running on local port 19080
T4ACC 000:048.432   Looking for J-Link GUI Server exe at: C:\Users\a5137978\.eclipse\com.renesas.platform_15818172\DebugComp\RA\ARM\Segger_v7.98.7\JLinkGUIServer.exe
T4ACC 000:049.005   Looking for J-Link GUI Server exe at: \JLinkGUIServer.exe
T4ACC 000:357.274   Failed to connect to J-Link GUI Server.
T4ACC 000:357.645 - 348.476ms returns "O.K."
T4ACC 000:358.658 JLINK_ExecCommand("ProjectFile=C:\mywork\e2_studio_workspaces\e2_studio_tutorials\QC_Demos\Glass_Break_Detector_V1_1/Glass_Break_Detector_V1_1.elf.jlink", ...). 
T4ACC 000:390.960 - 32.308ms returns 0x00
T4ACC 000:392.057 JLINK_ExecCommand("device=R7FA6E10F", ...). 
T4ACC 000:392.990   Flash bank @ 0x0100A100: SFL: Parsing sectorization info from ELF file
T4ACC 000:393.036     FlashDevice.SectorInfo[0]: .SectorSize = 0x00000010, .SectorStartAddr = 0x00000000
T4ACC 000:393.068   FlashBank @0x0100A100: Sectorization info from SFL ELF file ignored because sectorization override from DLL / XML file is active.
T4ACC 000:393.394   Flash bank @ 0x60000000: SFL: Parsing sectorization info from ELF file
T4ACC 000:393.420     FlashDevice.SectorInfo[0]: .SectorSize = 0x00010000, .SectorStartAddr = 0x00000000
T4ACC 000:397.761   Device "R7FA6E10F" selected.
T4ACC 000:399.129 - 7.019ms returns 0x00
T4ACC 000:399.163 JLINK_TIF_GetAvailable(...)
T4ACC 000:399.567 - 0.404ms
T4ACC 000:399.618 JLINK_TIF_Select(JLINKARM_TIF_SWD)
T4ACC 000:400.916 - 1.297ms returns 0x00
T4ACC 000:400.958 JLINK_SetSpeed(4000)
T4ACC 000:401.174 - 0.219ms
T4ACC 000:401.223 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T4ACC 000:401.662   ConfigTargetSettings() start
T4ACC 000:401.735    J-Link Script File: Executing ConfigTargetSettings()
T4ACC 000:401.797   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T4ACC 000:434.320   ConfigTargetSettings() end - Took 32.5ms
T4ACC 000:434.388   InitTarget() start
T4ACC 000:434.419    J-Link Script File: Executing InitTarget()
T4ACC 000:434.443   SWD selected. Executing JTAG -> SWD switching sequence.
T4ACC 000:436.604   DAP initialized successfully.
T4ACC 000:436.686   Determining TrustZone configuration...
T4ACC 000:437.820     Secure Debug: Enabled (SSD)
T4ACC 000:437.874   Determining currently configured transfer type by reading the AHB-AP CSW register.
T4ACC 000:438.715     --> Correct transfer type configured. Done.
T4ACC 000:438.803   InitTarget() end - Took 4.38ms
T4ACC 000:439.520   Found SW-DP with ID 0x6BA02477
T4ACC 000:441.860   DPIDR: 0x6BA02477
T4ACC 000:441.918   CoreSight SoC-400 or earlier
T4ACC 000:441.939   Scanning AP map to find all available APs
T4ACC 000:443.024   AP[2]: Stopped AP scan as end of AP map has been reached
T4ACC 000:443.095   AP[0]: AHB-AP (IDR: 0x84770001, ADDR: 0x00000000)
T4ACC 000:443.124   AP[1]: APB-AP (IDR: 0x54770002, ADDR: 0x01000000)
T4ACC 000:443.146   Iterating through AP map to find AHB-AP to use
T4ACC 000:444.080   AP[0]: Core found
T4ACC 000:444.123   AP[0]: AHB-AP ROM base: 0xE00FE000
T4ACC 000:444.678   CPUID register: 0x410FD214. Implementer code: 0x41 (ARM)
T4ACC 000:444.794   Feature set: Mainline
T4ACC 000:445.147   Cache: No cache
T4ACC 000:445.196   Found Cortex-M33 r0p4, Little endian.
T4ACC 000:445.523   -- Max. mem block: 0x0001D648
T4ACC 000:446.105   CPU_ReadMem(4 bytes @ 0xE000EDF0)
T4ACC 000:446.748   CPU_ReadMem(4 bytes @ 0xE0002000)
T4ACC 000:447.180   FPUnit: 8 code (BP) slots and 0 literal slots
T4ACC 000:447.222   CPU_ReadMem(4 bytes @ 0xE000EDFC)
T4ACC 000:447.680   CPU_ReadMem(4 bytes @ 0xE0001000)
T4ACC 000:448.036   CPU_ReadMem(4 bytes @ 0xE0001000)
T4ACC 000:448.392   CPU_ReadMem(4 bytes @ 0xE0001028)
T4ACC 000:448.784   CPU_ReadMem(4 bytes @ 0xE0001038)
T4ACC 000:449.120   CPU_ReadMem(4 bytes @ 0xE0001048)
T4ACC 000:449.442   CPU_ReadMem(4 bytes @ 0xE0001058)
T4ACC 000:449.840   CPU_WriteMem(4 bytes @ 0xE0001000)
T4ACC 000:450.270   CPU_ReadMem(4 bytes @ 0xE000ED88)
T4ACC 000:450.692   CPU_WriteMem(4 bytes @ 0xE000ED88)
T4ACC 000:451.147   CPU_ReadMem(4 bytes @ 0xE000ED88)
T4ACC 000:451.563   CPU_WriteMem(4 bytes @ 0xE000ED88)
T4ACC 000:451.936   CPU_ReadMem(4 bytes @ 0xE000EFB8)
T4ACC 000:452.321   Security extension: implemented
T4ACC 000:452.370   Secure debug: enabled
T4ACC 000:452.394   CoreSight components:
T4ACC 000:452.415   ROMTbl[0] @ E00FE000
T4ACC 000:452.439   CPU_ReadMem(64 bytes @ 0xE00FE000)
T4ACC 000:453.234   CPU_ReadMem(32 bytes @ 0xE0044FE0)
T4ACC 000:453.817   CPU_ReadMem(4 bytes @ 0xE0044FBC)
T4ACC 000:454.278   CPU_ReadMem(4 bytes @ 0xE0044FCC)
T4ACC 000:454.787   [0][0]: E0044000 CID B105900D PID 005BB906 DEVARCH 00000000 DEVTYPE 14 CTI (?)
T4ACC 000:454.835   CPU_ReadMem(32 bytes @ 0xE0047FE0)
T4ACC 000:455.287   CPU_ReadMem(4 bytes @ 0xE0047FBC)
T4ACC 000:455.623   CPU_ReadMem(4 bytes @ 0xE0047FCC)
T4ACC 000:455.943   [0][1]: E0047000 CID B105900D PID 003BB908 DEVARCH 00000000 DEVTYPE 12 CSTF
T4ACC 000:455.992   CPU_ReadMem(32 bytes @ 0xE0048FE0)
T4ACC 000:456.461   CPU_ReadMem(4 bytes @ 0xE0048FBC)
T4ACC 000:456.795   CPU_ReadMem(4 bytes @ 0xE0048FCC)
T4ACC 000:457.143   [0][2]: E0048000 CID B105900D PID 001BB961 DEVARCH 00000000 DEVTYPE 21 ETB
T4ACC 000:457.203   CPU_ReadMem(32 bytes @ 0xE0049FE0)
T4ACC 000:457.694   [0][3]: E0049000 CID B105F00D PID 001BB101 TSG
T4ACC 000:457.756   CPU_ReadMem(32 bytes @ 0xE0040FE0)
T4ACC 000:458.222   CPU_ReadMem(4 bytes @ 0xE0040FBC)
T4ACC 000:458.669   CPU_ReadMem(4 bytes @ 0xE0040FCC)
T4ACC 000:459.078   [0][4]: E0040000 CID B105900D PID 000BBD21 DEVARCH 00000000 DEVTYPE 11 TPIU
T4ACC 000:459.154   CPU_ReadMem(32 bytes @ 0xE00FFFE0)
T4ACC 000:459.824   [0][5]: E00FF000 CID B105100D PID 000BB4C9 ROM Table
T4ACC 000:459.882   ROMTbl[1] @ E00FF000
T4ACC 000:459.904   CPU_ReadMem(64 bytes @ 0xE00FF000)
T4ACC 000:460.739   CPU_ReadMem(32 bytes @ 0xE000EFE0)
T4ACC 000:461.313   CPU_ReadMem(4 bytes @ 0xE000EFBC)
T4ACC 000:461.820   CPU_ReadMem(4 bytes @ 0xE000EFCC)
T4ACC 000:462.342   [1][0]: E000E000 CID B105900D PID 000BBD21 DEVARCH 47702A04 DEVTYPE 00 Cortex-M33
T4ACC 000:462.382   CPU_ReadMem(32 bytes @ 0xE0001FE0)
T4ACC 000:462.992   CPU_ReadMem(4 bytes @ 0xE0001FBC)
T4ACC 000:463.464   CPU_ReadMem(4 bytes @ 0xE0001FCC)
T4ACC 000:463.866   [1][1]: E0001000 CID B105900D PID 000BBD21 DEVARCH 47701A02 DEVTYPE 00 DWT
T4ACC 000:463.913   CPU_ReadMem(32 bytes @ 0xE0002FE0)
T4ACC 000:464.393   CPU_ReadMem(4 bytes @ 0xE0002FBC)
T4ACC 000:464.779   CPU_ReadMem(4 bytes @ 0xE0002FCC)
T4ACC 000:465.154   [1][2]: E0002000 CID B105900D PID 000BBD21 DEVARCH 47701A03 DEVTYPE 00 FPB
T4ACC 000:465.183   CPU_ReadMem(32 bytes @ 0xE0000FE0)
T4ACC 000:465.651   CPU_ReadMem(4 bytes @ 0xE0000FBC)
T4ACC 000:466.021   CPU_ReadMem(4 bytes @ 0xE0000FCC)
T4ACC 000:466.336   [1][3]: E0000000 CID B105900D PID 000BBD21 DEVARCH 47701A01 DEVTYPE 43 ITM
T4ACC 000:466.377   CPU_ReadMem(32 bytes @ 0xE0041FE0)
T4ACC 000:466.952   CPU_ReadMem(4 bytes @ 0xE0041FBC)
T4ACC 000:467.330   CPU_ReadMem(4 bytes @ 0xE0041FCC)
T4ACC 000:467.700   [1][5]: E0041000 CID B105900D PID 002BBD21 DEVARCH 47724A13 DEVTYPE 13 ETM
T4ACC 000:467.747   CPU_ReadMem(32 bytes @ 0xE0042FE0)
T4ACC 000:468.305   CPU_ReadMem(4 bytes @ 0xE0042FBC)
T4ACC 000:468.643   CPU_ReadMem(4 bytes @ 0xE0042FCC)
T4ACC 000:469.019   [1][6]: E0042000 CID B105900D PID 000BBD21 DEVARCH 47701A14 DEVTYPE 14 CSS600-CTI
T4ACC 000:469.092   CPU_ReadMem(4 bytes @ 0xE000EDF0)
T4ACC 000:469.432   Data:  03 00 13 00
T4ACC 000:469.471   Debug reg: DHCSR
T4ACC 000:469.493 - 68.269ms returns 0
T4ACC 000:469.520 JLINK_ReadMem(0x400E002C, 0x4 Bytes, ...)
T4ACC 000:469.539   CPU_ReadMem(4 bytes @ 0x400E002C)
T4ACC 000:469.866   Data:  02 00 00 00
T4ACC 000:469.905 - 0.385ms returns 0
T4ACC 000:470.720 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T4ACC 000:470.758   CPU_ReadMem(4 bytes @ 0xE000EDF0)
T4ACC 000:471.117   Data:  03 00 13 00
T4ACC 000:471.156   Debug reg: DHCSR
T4ACC 000:471.178 - 0.459ms returns 0
T4ACC 000:471.222 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T4ACC 000:471.242   CPU_ReadMem(4 bytes @ 0xE000EDF0)
T4ACC 000:471.549   Data:  03 00 13 00
T4ACC 000:471.607   Debug reg: DHCSR
T4ACC 000:471.635 - 0.413ms returns 0
T4ACC 000:471.659 JLINK_ReadMem(0x400E001C, 0x4 Bytes, ...)
T4ACC 000:471.682   CPU_ReadMem(4 bytes @ 0x400E001C)
T4ACC 000:472.158   Data:  00 EC 00 00
T4ACC 000:472.271 - 0.611ms returns 0
T4ACC 000:472.344 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T4ACC 000:472.401   CPU_ReadMem(4 bytes @ 0xE000EDF0)
T4ACC 000:472.869   Data:  03 00 13 00
T4ACC 000:472.909   Debug reg: DHCSR
T4ACC 000:472.931 - 0.587ms returns 0
T4ACC 000:472.949 JLINK_ReadMem(0x400E0018, 0x4 Bytes, ...)
T4ACC 000:472.967   CPU_ReadMem(4 bytes @ 0x400E0018)
T4ACC 000:473.442   Data:  00 00 01 00
T4ACC 000:473.485 - 0.536ms returns 0
T4ACC 000:473.505 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T4ACC 000:473.524   CPU_ReadMem(4 bytes @ 0xE000EDF0)
T4ACC 000:473.959   Data:  03 00 13 00
T4ACC 000:473.998   Debug reg: DHCSR
T4ACC 000:474.020 - 0.514ms returns 0
T4ACC 000:474.038 JLINK_ReadMem(0x400E0020, 0x4 Bytes, ...)
T4ACC 000:474.056   CPU_ReadMem(4 bytes @ 0x400E0020)
T4ACC 000:474.466   Data:  00 00 00 00
T4ACC 000:474.508 - 0.470ms returns 0
T4ACC 000:474.529 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T4ACC 000:474.549   CPU_ReadMem(4 bytes @ 0xE000EDF0)
T4ACC 000:475.043   Data:  03 00 13 00
T4ACC 000:475.085   Debug reg: DHCSR
T4ACC 000:475.107 - 0.577ms returns 0
T4ACC 000:475.125 JLINK_ReadMem(0x400E0028, 0x4 Bytes, ...)
T4ACC 000:475.143   CPU_ReadMem(4 bytes @ 0x400E0028)
T4ACC 000:475.588   Data:  00 F0 01 00
T4ACC 000:475.633 - 0.508ms returns 0
T4ACC 000:475.657 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T4ACC 000:475.678   CPU_ReadMem(4 bytes @ 0xE000EDF0)
T4ACC 000:476.163   Data:  03 00 13 00
T4ACC 000:476.208   Debug reg: DHCSR
T4ACC 000:476.233 - 0.576ms returns 0
T4ACC 000:476.253 JLINK_ReadMem(0x400E0024, 0x4 Bytes, ...)
T4ACC 000:476.275   CPU_ReadMem(4 bytes @ 0x400E0024)
T4ACC 000:476.718   Data:  00 00 02 00
T4ACC 000:476.762 - 0.508ms returns 0
T4ACC 000:476.785 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T4ACC 000:476.806   CPU_ReadMem(4 bytes @ 0xE000EDF0)
T4ACC 000:477.250   Data:  03 00 13 00
T4ACC 000:477.294   Debug reg: DHCSR
T4ACC 000:477.319 - 0.533ms returns 0
T4ACC 000:477.339 JLINK_ReadMem(0x400E002C, 0x4 Bytes, ...)
T4ACC 000:477.359   CPU_ReadMem(4 bytes @ 0x400E002C)
T4ACC 000:477.840   Data:  02 00 00 00
T4ACC 000:477.883 - 0.545ms returns 0
T4ACC 000:477.906 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T4ACC 000:477.927   CPU_ReadMem(4 bytes @ 0xE000EDF0)
T4ACC 000:478.375   Data:  03 00 13 00
T4ACC 000:478.418   Debug reg: DHCSR
T4ACC 000:478.442 - 0.536ms returns 0
T4ACC 000:478.462 JLINK_ReadMem(0x400E002C, 0x4 Bytes, ...)
T4ACC 000:478.482   CPU_ReadMem(4 bytes @ 0x400E002C)
T4ACC 000:478.875   Data:  02 00 00 00
T4ACC 000:478.928 - 0.465ms returns 0
T4ACC 000:486.448 JLINK_Close()
T4ACC 000:507.179 - 20.729ms
T4ACC 000:507.264   
T4ACC 000:507.292   Closed
