FSP Configuration
  Board "RA8|RA8P1|EK-RA8P1"
  R7KA8P1KFLCAC
    part_number: R7KA8P1KFLCAC
    rom_size_bytes: 1048576
    ram_size_bytes: 2097152
    data_flash_size_bytes: 0
    package_style: LFBGA
    package_pins: 289
    number of cores: 2
    
  RA8P1
    series: 8
    
  RA8P1 Family
    Enable inline BSP IRQ functions: Enabled
    SDRAM: SDRAM Support: Disabled
    SDRAM: Timings: tRAS (cycles): 6 cycles
    SDRAM: Timings: tRCD (cycles): 3 cycles
    SDRAM: Timings: tRP (cycles): 3 cycles
    SDRAM: Timings: tWR (cycles): 2 cycles
    SDRAM: Timings: tCL (cycles): 3 cycles
    SDRAM: Timings: tRFC (cycles): 937
    SDRAM: Timings: tREFW (cycles): 8 cycles
    SDRAM: Initialization: Auto-Refresh Interval (ARFI): 10 cycles
    SDRAM: Initialization: Auto-Refresh Count (ARFC): 8 times
    SDRAM: Initialization: Precharge Cycle Count (PRC): 3 cycles
    SDRAM: Address Multiplex Shift: 9-bit shift
    SDRAM: Endian Mode: Little Endian
    SDRAM: Continuous Access Mode: Enabled
    SDRAM: Bus Width: 32-bit
    Security: Exceptions: Exception Response: Non-Maskable Interrupt
    Security: Exceptions: BusFault, HardFault, and NMI Target: Secure State
    Security: System Reset Request Accessibility: Secure State
    Security: Exceptions: Prioritize Secure Exceptions: Disabled
    Security: System Reset Status Accessibility: Both Secure and Non-Secure State
    Security: Battery Backup Accessibility: Both Secure and Non-Secure State
    Security: SRAM Accessibility: SRAM0 Protection: Both Secure and Non-Secure State
    Security: SRAM Accessibility: SRAM1 Protection: Both Secure and Non-Secure State
    Security: SRAM Accessibility: SRAM2 Protection: Both Secure and Non-Secure State
    Security: SRAM Accessibility: SRAM3 Protection: Both Secure and Non-Secure State
    Security: BUS Accessibility: Bus Security Attribution Register A: Both Secure and Non-Secure State
    Security: BUS Accessibility: Bus Security Attribution Register B: Both Secure and Non-Secure State
    Security: BUS Accessibility: Bus Security Attribution Register C: Both Secure and Non-Secure State
    Security: IPC: IPC Semaphore Group Security Attribution (0 to 7): Secure State
    Security: IPC: IPC Semaphore Group Security Attribution (8 to 15): Secure State
    Security: IPC: IPC NMI0 Security Attribution: Secure State
    Security: IPC: IPC NMI1 Security Attribution: Secure State
    Security: Graphics Power Domain Security Attribution: Secure State
    Security: Uninitialized Non-Secure Application Fallback: Enable Uninitialized Non-Secure Application Fallback
    Clocks: HOCO FLL Function: Disabled
    Clocks: Clock Settling Delay: Enabled
    Clocks: Sleep Mode Entry and Exit Delays: Enabled
    Clocks: RTOS Sleep Mode Entry and Exit Delays: Enabled
    Clocks: MSTP Change Delays: Enabled
    Clocks: Settling Delay (us): 150
    Main Oscillator Wait Time: 8163 cycles
    Cache settings: Data cache: Disabled
    
  RA8P1 Device Options
    OFS Registers: OFS0 (Option Function Select Register 0) Settings: Disabled
    OFS Registers: OFS0 (Option Function Select Register 0) Settings: Independent WDT: Start Mode: IWDT is stopped after a reset (Register-start mode)
    OFS Registers: OFS0 (Option Function Select Register 0) Settings: Independent WDT: Timeout Period: 2048 cycles
    OFS Registers: OFS0 (Option Function Select Register 0) Settings: Independent WDT: Dedicated Clock Frequency Divisor: 128
    OFS Registers: OFS0 (Option Function Select Register 0) Settings: Independent WDT: Window End Position:  0% (no window end position)
    OFS Registers: OFS0 (Option Function Select Register 0) Settings: Independent WDT: Window Start Position: 100% (no window start position)
    OFS Registers: OFS0 (Option Function Select Register 0) Settings: Independent WDT: Reset Interrupt Request Select: Reset is enabled
    OFS Registers: OFS0 (Option Function Select Register 0) Settings: Independent WDT: Stop Control: Stop counting when in Sleep,Deep SleepSnooze modec, or Software Standby
    OFS Registers: OFS0 (Option Function Select Register 0) Settings: WDT0: Start Mode Select: Stop WDT after a reset (register-start mode)
    OFS Registers: OFS0 (Option Function Select Register 0) Settings: WDT0: Timeout Period: 16384 cycles
    OFS Registers: OFS0 (Option Function Select Register 0) Settings: WDT0: Clock Frequency Division Ratio: 128
    OFS Registers: OFS0 (Option Function Select Register 0) Settings: WDT0: Window End Position:  0% (no window end position)
    OFS Registers: OFS0 (Option Function Select Register 0) Settings: WDT0: Window Start Position: 100% (no window start position)
    OFS Registers: OFS0 (Option Function Select Register 0) Settings: WDT0: Reset Interrupt Request: Reset
    OFS Registers: OFS0 (Option Function Select Register 0) Settings: WDT0: Stop Control: Stop counting when entering Sleep mode
    OFS Registers: OFS2 (Option Function Select Register 2) Settings: Disabled
    OFS Registers: OFS2 (Option Function Select Register 2) Settings: DCDC: Enabled
    OFS Registers: OFS1 (Option Function Select Register 1) Settings: Disabled
    OFS Registers: OFS1 (Option Function Select Register 1) Settings: Voltage Detection 0 Circuit Start: Voltage monitor 0 reset is disabled after reset
    OFS Registers: OFS1 (Option Function Select Register 1) Settings: Voltage Detection 0 Level: 1.60 V
    OFS Registers: OFS1 (Option Function Select Register 1) Settings: HOCO Oscillation Enable: HOCO oscillation is disabled after reset
    OFS Registers: OFS1 (Option Function Select Register 1) Settings: Voltage Detection 0 Low Power Consumption: Voltage monitor 0 Low Power Consumption Disabled
    OFS Registers: OFS1 (Option Function Select Register 1) Settings: WDT/IWDT Software Debug Control: Disabled (WDT and IWDT continue operating while the CPU is in the debug state)
    OFS Registers: OFS1 (Option Function Select Register 1) Settings: Tightly Coupled Memory (TCM)/Cache ECC: Disable ECC function for TCM and Cache
    OFS Registers: OFS1_SEC (Option Function Select Register 1 Secure) Settings: Disabled
    OFS Registers: OFS1_SEC (Option Function Select Register 1 Secure) Settings: Voltage Detection 0 Circuit Start: Voltage monitor 0 reset is disabled after reset
    OFS Registers: OFS1_SEC (Option Function Select Register 1 Secure) Settings: Voltage Detection 0 Level: 1.60 V
    OFS Registers: OFS1_SEC (Option Function Select Register 1 Secure) Settings: HOCO Oscillation Enable: HOCO oscillation is disabled after reset
    OFS Registers: OFS1_SEC (Option Function Select Register 1 Secure) Settings: Voltage Detection 0 Low Power Consumption: Voltage monitor 0 Low Power Consumption Disabled
    OFS Registers: OFS1_SEC (Option Function Select Register 1 Secure) Settings: WDT/IWDT Software Debug Control: Disabled (WDT and IWDT continue operating while the CPU is in the debug state)
    OFS Registers: OFS1_SEC (Option Function Select Register 1 Secure) Settings: Tightly Coupled Memory (TCM)/Cache ECC: Disable ECC function for TCM and Cache
    OFS Registers: OFS1_SEL (OFS1 Register Select) Settings: Disabled
    OFS Registers: OFS1_SEL (OFS1 Register Select) Settings: Voltage Detection 0 Level Security Attribution: VDSEL setting loads from OFS1_SEC
    OFS Registers: OFS1_SEL (OFS1 Register Select) Settings: Voltage Detection 0 Circuit Start Security Attribution: PVDAS setting loads from OFS1_SEC
    OFS Registers: OFS1_SEL (OFS1 Register Select) Settings: Voltage Detection 0 Low Power Consumption Security Attribution: PVDLPSEL setting loads from OFS1_SEC
    OFS Registers: OFS1_SEL (OFS1 Register Select) Settings: WDT/IWDT Software Debug Control Security Attribution: SWDBG setting loads from OFS1_SEC
    OFS Registers: OFS1_SEL (OFS1 Register Select) Settings: Tightly Coupled Memory (TCM)/Cache ECC Security Attribution: INITECCEN setting loads from OFS1_SEC
    OFS Registers: OFS3 (Option Function Select Register 3) Settings: Disabled
    OFS Registers: OFS3 (Option Function Select Register 3) Settings: WDT1: Start Mode: Stop WDT after a reset (register start mode)
    OFS Registers: OFS3 (Option Function Select Register 3) Settings: WDT1: Timeout Period: 16384 cycles
    OFS Registers: OFS3 (Option Function Select Register 3) Settings: WDT1: Clock Frequency Division Ratio: 128
    OFS Registers: OFS3 (Option Function Select Register 3) Settings: WDT1: Window End Position: 0% (no window end position)
    OFS Registers: OFS3 (Option Function Select Register 3) Settings: WDT1: Window Start Position: 100% (no window start position)
    OFS Registers: OFS3 (Option Function Select Register 3) Settings: WDT1: Reset Interrupt Request: Reset
    OFS Registers: OFS3 (Option Function Select Register 3) Settings: WDT1: Stop Control: Stop counting when entering Sleep or Deep Sleep mode
    OFS Registers: OFS3_SEC (Option Function Select Register 3 Secure) Settings: Disabled
    OFS Registers: OFS3_SEC (Option Function Select Register 3 Secure) Settings: WDT1: Start Mode: Stop WDT after a reset (register start mode)
    OFS Registers: OFS3_SEC (Option Function Select Register 3 Secure) Settings: WDT1: Timeout Period: 16384 cycles
    OFS Registers: OFS3_SEC (Option Function Select Register 3 Secure) Settings: WDT1: Clock Frequency Division Ratio: 128
    OFS Registers: OFS3_SEC (Option Function Select Register 3 Secure) Settings: WDT1: Window End Position: 0% (no window end position)
    OFS Registers: OFS3_SEC (Option Function Select Register 3 Secure) Settings: WDT1: Window Start Position: 100% (no window start position)
    OFS Registers: OFS3_SEC (Option Function Select Register 3 Secure) Settings: WDT1: Reset Interrupt Request: Reset
    OFS Registers: OFS3_SEC (Option Function Select Register 3 Secure) Settings: WDT1: Stop Control: Stop counting when entering Sleep or Deep Sleep mode
    OFS Registers: OFS3_SEL (OFS3 Register Select) Settings: Disabled
    OFS Registers: OFS3_SEL (OFS3 Register Select) Settings: WDT1: Start Mode: WDT1STRT setting loads from OFS3_SEC
    OFS Registers: OFS3_SEL (OFS3 Register Select) Settings: WDT1: Timeout Period: WDT1TOPS setting loads from OFS3_SEC
    OFS Registers: OFS3_SEL (OFS3 Register Select) Settings: WDT1: Clock Frequency Division Ratio: WDT1CKS setting loads from OFS3_SEC
    OFS Registers: OFS3_SEL (OFS3 Register Select) Settings: WDT1: Window End Position: WDT1RPES setting loads from OFS3_SEC
    OFS Registers: OFS3_SEL (OFS3 Register Select) Settings: WDT1: Window Start Position: WDT1RPSS setting loads from OFS3_SEC
    OFS Registers: OFS3_SEL (OFS3 Register Select) Settings: WDT1: Reset Interrupt Request Select: WDT1RSTIRQS setting loads from OFS3_SEC
    OFS Registers: OFS3_SEL (OFS3 Register Select) Settings: WDT1: Stop Control: WDT1STPCTL setting loads from OFS3_SEC
    OFS Registers: BPS (Block Protect Setting Register) Settings: Disabled
    OFS Registers: BPS (Block Protect Setting Register) Settings: BPS0: 
    OFS Registers: BPS (Block Protect Setting Register) Settings: BPS1: 
    OFS Registers: BPS (Block Protect Setting Register) Settings: BPS2: 
    OFS Registers: BPS (Block Protect Setting Register) Settings: BPS3: 
    OFS Registers: BPS (Block Protect Setting Register) Settings: BPS4: 
    OFS Registers: BPS (Block Protect Setting Register) Settings: BPS5: 
    OFS Registers: BPS (Block Protect Setting Register) Settings: BPS6: 
    OFS Registers: BPS (Block Protect Setting Register) Settings: BPS7: 
    OFS Registers: BPS (Block Protect Setting Register) Settings: BPS8: 
    OFS Registers: BPS (Block Protect Setting Register) Settings: BPS9: 
    OFS Registers: BPS (Block Protect Setting Register) Settings: BPS10: 
    OFS Registers: BPS (Block Protect Setting Register) Settings: BPS11: 
    OFS Registers: BPS (Block Protect Setting Register) Settings: BPS12: 
    OFS Registers: BPS (Block Protect Setting Register) Settings: BPS13: 
    OFS Registers: BPS (Block Protect Setting Register) Settings: BPS14: 
    OFS Registers: BPS (Block Protect Setting Register) Settings: BPS15: 
    OFS Registers: BPS (Block Protect Setting Register) Settings: BPS16: 
    OFS Registers: BPS_SEC (Block Protect Setting Register Secure) Settings: Disabled
    OFS Registers: BPS_SEC (Block Protect Setting Register Secure) Settings: BPS_SEC0: 
    OFS Registers: BPS_SEC (Block Protect Setting Register Secure) Settings: BPS_SEC1: 
    OFS Registers: BPS_SEC (Block Protect Setting Register Secure) Settings: BPS_SEC2: 
    OFS Registers: BPS_SEC (Block Protect Setting Register Secure) Settings: BPS_SEC3: 
    OFS Registers: BPS_SEC (Block Protect Setting Register Secure) Settings: BPS_SEC4: 
    OFS Registers: BPS_SEC (Block Protect Setting Register Secure) Settings: BPS_SEC5: 
    OFS Registers: BPS_SEC (Block Protect Setting Register Secure) Settings: BPS_SEC6: 
    OFS Registers: BPS_SEC (Block Protect Setting Register Secure) Settings: BPS_SEC7: 
    OFS Registers: BPS_SEC (Block Protect Setting Register Secure) Settings: BPS_SEC8: 
    OFS Registers: BPS_SEC (Block Protect Setting Register Secure) Settings: BPS_SEC9: 
    OFS Registers: BPS_SEC (Block Protect Setting Register Secure) Settings: BPS_SEC10: 
    OFS Registers: BPS_SEC (Block Protect Setting Register Secure) Settings: BPS_SEC11: 
    OFS Registers: BPS_SEC (Block Protect Setting Register Secure) Settings: BPS_SEC12: 
    OFS Registers: BPS_SEC (Block Protect Setting Register Secure) Settings: BPS_SEC13: 
    OFS Registers: BPS_SEC (Block Protect Setting Register Secure) Settings: BPS_SEC14: 
    OFS Registers: BPS_SEC (Block Protect Setting Register Secure) Settings: BPS_SEC15: 
    OFS Registers: BPS_SEC (Block Protect Setting Register Secure) Settings: BPS_SEC16: 
    OFS Registers: PBPS_SEC (Permanent Block Protect Setting Register Secure) Settings: Disabled
    OFS Registers: PBPS_SEC (Permanent Block Protect Setting Register Secure) Settings: PBPS_SEC0: 
    OFS Registers: PBPS_SEC (Permanent Block Protect Setting Register Secure) Settings: PBPS_SEC1: 
    OFS Registers: PBPS_SEC (Permanent Block Protect Setting Register Secure) Settings: PBPS_SEC2: 
    OFS Registers: PBPS_SEC (Permanent Block Protect Setting Register Secure) Settings: PBPS_SEC3: 
    OFS Registers: PBPS_SEC (Permanent Block Protect Setting Register Secure) Settings: PBPS_SEC4: 
    OFS Registers: PBPS_SEC (Permanent Block Protect Setting Register Secure) Settings: PBPS_SEC5: 
    OFS Registers: PBPS_SEC (Permanent Block Protect Setting Register Secure) Settings: PBPS_SEC6: 
    OFS Registers: PBPS_SEC (Permanent Block Protect Setting Register Secure) Settings: PBPS_SEC7: 
    OFS Registers: PBPS_SEC (Permanent Block Protect Setting Register Secure) Settings: PBPS_SEC8: 
    OFS Registers: PBPS_SEC (Permanent Block Protect Setting Register Secure) Settings: PBPS_SEC9: 
    OFS Registers: PBPS_SEC (Permanent Block Protect Setting Register Secure) Settings: PBPS_SEC10: 
    OFS Registers: PBPS_SEC (Permanent Block Protect Setting Register Secure) Settings: PBPS_SEC11: 
    OFS Registers: PBPS_SEC (Permanent Block Protect Setting Register Secure) Settings: PBPS_SEC12: 
    OFS Registers: PBPS_SEC (Permanent Block Protect Setting Register Secure) Settings: PBPS_SEC13: 
    OFS Registers: PBPS_SEC (Permanent Block Protect Setting Register Secure) Settings: PBPS_SEC14: 
    OFS Registers: PBPS_SEC (Permanent Block Protect Setting Register Secure) Settings: PBPS_SEC15: 
    OFS Registers: PBPS_SEC (Permanent Block Protect Setting Register Secure) Settings: PBPS_SEC16: 
    OFS Registers: PBPS (Permanent Block Protect Setting Register) Settings: Disabled
    OFS Registers: PBPS (Permanent Block Protect Setting Register) Settings: PBPS0: 
    OFS Registers: PBPS (Permanent Block Protect Setting Register) Settings: PBPS1: 
    OFS Registers: PBPS (Permanent Block Protect Setting Register) Settings: PBPS2: 
    OFS Registers: PBPS (Permanent Block Protect Setting Register) Settings: PBPS3: 
    OFS Registers: PBPS (Permanent Block Protect Setting Register) Settings: PBPS4: 
    OFS Registers: PBPS (Permanent Block Protect Setting Register) Settings: PBPS5: 
    OFS Registers: PBPS (Permanent Block Protect Setting Register) Settings: PBPS6: 
    OFS Registers: PBPS (Permanent Block Protect Setting Register) Settings: PBPS7: 
    OFS Registers: PBPS (Permanent Block Protect Setting Register) Settings: PBPS8: 
    OFS Registers: PBPS (Permanent Block Protect Setting Register) Settings: PBPS9: 
    OFS Registers: PBPS (Permanent Block Protect Setting Register) Settings: PBPS10: 
    OFS Registers: PBPS (Permanent Block Protect Setting Register) Settings: PBPS11: 
    OFS Registers: PBPS (Permanent Block Protect Setting Register) Settings: PBPS12: 
    OFS Registers: PBPS (Permanent Block Protect Setting Register) Settings: PBPS13: 
    OFS Registers: PBPS (Permanent Block Protect Setting Register) Settings: PBPS14: 
    OFS Registers: PBPS (Permanent Block Protect Setting Register) Settings: PBPS15: 
    OFS Registers: PBPS (Permanent Block Protect Setting Register) Settings: PBPS16: 
    
  RA8P1 Core 0 Options
  RA8P1 event data
  RA Common
    Main stack size (bytes): 0x30000
    Heap size (bytes): 0x10000
    Bootloader Secondary XIP: Disabled
    MCU Vcc (mV): 3300
    Parameter checking: Disabled
    Assert Failures: Return FSP_ERR_ASSERTION
    Clock Registers not Reset Values during Startup: Disabled
    Main Oscillator Populated: Populated
    PFS Protect: Enabled
    C Runtime Initialization : Enabled
    Early BSP Initialization : Disabled
    Main Oscillator Clock Source: Crystal or Resonator
    Subclock Populated: Populated
    Subclock Drive (Drive capacitance availability varies by MCU): Standard/Normal mode
    Subclock Stabilization Time (ms): 1000
    
  Clocks
    XTAL 24000000Hz
    HOCO 48MHz
    PLL Src: XTAL
    PLL Div /3
    PLL Mul x200-219|Mul x200|PLL Mul x200.00
    PLL1P Div /2
    PLL1Q Div /2
    PLL1R Div /2
    PLL2 Src: XTAL
    PLL2 Div /1
    PLL2 Mul x40-59|Mul x48|PLL2 Mul x48.00
    PLL2P Div /3
    PLL2Q Div /2
    PLL2R Div /2
    Clock Src: PLL1P
    CPUCLK Div /1
    CPUCLK1 Div /4
    NPUCLK Div /2
    MRICLK Div /4
    MRPCLK Div /32
    ICLK Div /4
    PCLKA Div /8
    PCLKB Div /16
    PCLKC Div /8
    PCLKD Div /4
    PCLKE Div /4
    BCLK Div /8
    BCLKA Src: PLL2Q
    BCLKA Div /6
    SDCLK Enabled
    EBCLK Src: BCLK (Synchronous)
    EBCLK Div /2
    CLKOUT Src: HOCO
    CLKOUT Div /1
    SCICLK Src: PLL2R
    SCICLK Div /4
    SPICLK Src: PLL1Q
    SPICLK Div /4
    CANFDCLK Src: PLL2R
    CANFDCLK Div /10
    GPTCLK Src: PLL2P
    GPTCLK Div /4
    GPT Src: GPTCLK
    LCDCLK Src: PLL2R
    LCDCLK Div /4
    I3CCLK Src: PLL2Q
    I3CCLK Div /5
    USBCLK Src: PLL2R
    USBCLK Div /5
    USB60CLK Src: PLL2R
    USB60CLK Div /5
    OCTACLK Src: PLL1Q
    OCTACLK Div /4
    ADCCLK Src: PLL2R
    ADCCLK Div /4
    ESWCLK Src: PLL1P
    ESWCLK Div /4
    ESWPHYCLK Src: PLL1P
    ESWPHYCLK Div /2
    ETHPHYCLK Src: PLL2Q
    ETHPHYCLK Div /32
    
  Pin Configurations
    RA8P1 EK -> g_bsp_pin_cfg
      AVCC0 R9 CGC_AVCC0 - - - - - - - - IO "Read only" - 
      AVCC_MIPI T4 CGC_AVCC_MIPI - - - - - - - - IO "Read only" - 
      AVCC_USBHS K15 CGC_AVCC_USBHS - - - - - - - - IO "Read only" - 
      AVSS0 R10 CGC_AVSS0 - - - - - - - - IO "Read only" - 
      MIPI_CLN U2 CGC_MIPI_CLN - - - - - - - - IO "Read only" - 
      MIPI_CLP T2 CGC_MIPI_CLP - - - - - - - - IO "Read only" - 
      MIPI_DL0N U1 CGC_MIPI_DL0N - - - - - - - - IO "Read only" - 
      MIPI_DL0P T1 CGC_MIPI_DL0P - - - - - - - - IO "Read only" - 
      MIPI_DL1N U3 CGC_MIPI_DL1N - - - - - - - - IO "Read only" - 
      MIPI_DL1P T3 CGC_MIPI_DL1P - - - - - - - - IO "Read only" - 
      P000 U13 - S4_INT - - Disabled - - "ACMPHS: IVCMP2; ADC0: AN000; IRQ: IRQ6-DS" - None - - 
      P001 T13 - ARDUINO_A0 - - Disabled - - "ACMPHS: IVCMP3; ADC0: AN001; IRQ: IRQ7-DS" - None - - 
      P002 U14 - GROVE2_2_AN - - Disabled - - "ACMPHS: IVCMP2; ADC0: AN002; IRQ: IRQ8-DS" - None - - 
      P003 R12 - ARDUINO_A2 - - Disabled - - "ACMPHS: IVCMP3; ADC0: AN003; IRQ: IRQ29" - None - - 
      P004 T11 - ARDUINO_A3_MIKROBUS_AN - - Disabled - - "ACMPHS: IVCMP2; ADC0: AN004; IRQ: IRQ9-DS" - None - - 
      P005 R11 - GROVE2_1_AN - - Disabled - - "ACMPHS: IVCMP3; ADC0: AN005; IRQ: IRQ10-DS" - None - - 
      P006 U12 - PMOD1_7_INT - - Disabled - - "ACMPHS: IVCMP2; ADC1: AN006; IRQ: IRQ11-DS" - None - - 
      P007 T12 - ARDUINO_A1 - - Disabled - - "ACMPHS: IVCMP3; ADC1: AN007; IRQ: IRQ28" - None - - 
      P008 U11 - USER_S2 - - Disabled - - "ACMPHS: IVREF0; ADC1: AN008; IRQ: IRQ12-DS" - None - - 
      P009 P11 - USER_S1 - - Disabled - - "ACMPHS: IVREF1; ADC1: AN009; IRQ: IRQ13-DS" - None - - 
      P010 P10 - CAM_INT - - Disabled - - "ADC1: AN010; IRQ: IRQ14" - None - - 
      P011 N10 - ARDUINO_D2 - - Disabled - - "ADC1: AN011; IRQ: IRQ16" - None - - 
      P012 P9 - PMOD2_7_IRQ15 - - Disabled - - "ADC0: AN012; IRQ: IRQ15" - None - - 
      P013 N9 - I2C_SCL0_PULLUP - - Disabled - - "ADC1: AN013; IRQ: IRQ14" - None - - 
      P014 T8 - ARDUINO_A4 - - Disabled - - "ACMPHS: IVCMP0; ADC0: AN014; DAC120: DA0; IRQ: IRQ27" - None - - 
      P015 U8 - ARDUINO_A5 - - Disabled - - "ACMPHS: IVCMP0; ADC1: AN015; DAC121: DA1; IRQ: IRQ13" - None - - 
      P100 U6 - OSPI_DQ0_ARDUINO_D12_MISOB_MIKROBUS_MISOB - - Disabled - - "AGT0: AGTIO0; ESWM_GMII/MII: GPTP1_MATCH; ESWM_RGMII1: GPTP1_MATCH; ESWM_RMII1: GPTP1_MATCH; GPT8: GTIOC8B; GPT_POEGA: GTETRGA; IRQ: IRQ2; OSPI0: OM_0_SIO0; SCI9: DE9; SCI9: SCK9; SPI1: MISO1" - None - - 
      P101 R5 - OSPI_DQ3_ARDUINO_D11_MOSIB_MIKROBUS_MOSIB - - Disabled - - "AGT0: AGTEE0; ESWM_GMII/MII: GPTP1_CAPTURE; ESWM_RGMII1: GPTP1_CAPTURE; ESWM_RMII1: GPTP1_CAPTURE; GPT8: GTIOC8A; GPT_POEGB: GTETRGB; IRQ: IRQ1; OSPI0: OM_0_SIO3; SCI9: RXD9; SPI1: MOSI1" - None - - 
      P102 P5 - OSPI_DQ4_ARDUINO_D13_RSPCKB_MIKROBUS_RSPCKB - - Disabled - - "ADC0(Digital): ADTRG0; AGT0: AGTO0; CANFD0: CRX0; GPT2: GTIOC2B; GPT_OPS: GTOWLO; IRQ: IRQ17; OSPI0: OM_0_SIO4; SCI9: TXD9; SPI1: RSPCK1" - None - - 
      P103 R4 - OSPI_DQ2_ARDUINO_D10_SSLB_MIKROBUS_SSLB - - Disabled - - "ADC1(Digital): AD1FLAG1; CANFD0: CTX0; ESWM_GMII/MII: GPTP0_PPS; ESWM_RGMII0: GPTP0_PPS; ESWM_RMII0: GPTP0_PPS; GPT2: GTIOC2A; GPT_OPS: GTOWUP; IRQ: IRQ16; OSPI0: OM_0_SIO2; SCI9: CTS_RTS9; SCI9: DE9; SPI1: SSLB0" - None - - 
      P104 M6 - OSPI_CS_ARDUINO_D5 - - Disabled - - "ADC0(Digital): AD0FLAG1; ESWM_GMII/MII: GPTP0_MATCH; ESWM_RGMII0: GPTP0_MATCH; ESWM_RMII0: GPTP0_MATCH; GPT1: GTIOC1B; GPT_POEGB: GTETRGB; IRQ: IRQ1; OSPI0: OM_0_CS1; SCI9: CTS9; SPI1: SSLB1" - None - - 
      P105 N7 - OSPI_INT_ARDUINO_D6 - - Disabled - - "ADC(Digital): ADSYNC; ESWM_GMII/MII: GPTP0_CAPTURE; ESWM_RGMII0: GPTP0_CAPTURE; ESWM_RMII0: GPTP0_CAPTURE; GPT1: GTIOC1A; IRQ: IRQ0; OSPI0: OM_0_ECSINT1; SCI8: CTS_RTS8; SCI8: DE8; SPI1: SSLB2; ULPT1: ULPTO1-DS" - None - - 
      P106 N6 - OSPI_RES - - Disabled - - "ADC1(Digital): ADST1; AGT0: AGTOB0; ESWM_GMII/MII: ET1_LINKSTA; ESWM_RGMII1: ET1_LINKSTA; ESWM_RMII1: ET1_LINKSTA; GPT8: GTIOC8B; GPT_OPS: GTOWLO; IRQ: IRQ16; OSPI0: OM_0_RESET; SCI8: CTS8; SPI1: SSLB3; ULPT1: ULPTEE1-DS" - None - - 
      P107 N5 - ETH_MDINT - - Disabled - - "ADC0(Digital): ADST0; AGT0: AGTOA0; ESWM_GMII/MII: ET1_INT; ESWM_RGMII1: ET1_INT; ESWM_RMII1: ET1_INT; GPT8: GTIOC8A; GPT_OPS: GTOWUP; IRQ: IRQ31; OSPI0: OM_0_CS0; SCI4: CTS4" - None - - 
      P108 D8 - - - - Disabled - - "GPT10: GTIOC10B; IRQ: IRQ24; SDHI0: SD0DAT6" - None - - 
      P109 D7 - I2C_SDA0_PULLUP - - Disabled - - "GPT10: GTIOC10A; IRQ: IRQ23; SDHI0: SD0DAT5" - None - - 
      P110 C8 - ARDUINO_D9 - - Disabled - - "GPT9: GTIOC9B; IRQ: IRQ20; SDHI0: SD0DAT4" - None - - 
      P111 E8 - LCD_INT_MIPI_IRQ19 - - Disabled - - "GPT9: GTIOC9A; IRQ: IRQ19; SDHI0: SD0DAT3" - None - - 
      P112 A4 - SDRAM_DQ3 - - Disabled - - "ADC0(Digital): ADST0; BUS: D3; GLCDC: LCD_DATA10; GPT3: GTIOC3B; GPT_POEGA: GTETRGA; IRQ: IRQ27; SCI0: TXD0; SDHI0: SD0DAT4; SDRAM: DQ3; SPI0: SSLA2; SSIE0: SSIBCK0; ULPT0: ULPTOB0-DS" - None - - 
      P113 A2 - SDRAM_DQ4 - - Disabled - - "ADC1(Digital): ADST1; BUS: D4; GLCDC: LCD_DATA9; GPT2: GTIOC2A; GPT_POEGB: GTETRGB; IRQ: IRQ28; SCI0: RXD0; SDHI0: SD0DAT5; SDRAM: DQ4; SPI0: SSLA1; SSIE0: SSILRCK0; ULPT0: ULPTOA0-DS" - None - - 
      P114 B3 - SDRAM_DQ5 - - Disabled - - "ADC(Digital): ADSYNC; BUS: D5; GLCDC: LCD_DATA8; GPT2: GTIOC2B; GPT_POEGC: GTETRGC; IRQ: IRQ30-DS; SCI0: CTS_RTS0; SCI0: DE0; SDHI0: SD0DAT6; SDRAM: DQ5; SPI0: SSLA0; SSIE0: SSIRXD0" - None - - 
      P115 A3 - SDRAM_DQ6 - - Disabled - - "ADC0(Digital): AD0FLAG1; BUS: D6; GLCDC: LCD_DATA7; GPT5: GTIOC5A; GPT_POEGD: GTETRGD; IRQ: IRQ31-DS; SCI0: CTS0; SDHI0: SD0DAT7; SDRAM: DQ6; SPI0: MOSI0; SSIE0: SSITXD0" - None - - 
      P200 C5 - NMI - - Disabled - - "IRQ: NMI" - None - - 
      P201 E6 - MD_MIKROBUS_RES - - Disabled - - "CGC: MD; IRQ: IRQ4" - None - - 
      P206 B15 - ENET_RX_CTL - - Disabled - - "BUS: CS7; CEU: VIO_D0; CLKOUT: CLKOUT; ESWM_GMII/MII1: ET1_RX_DV; ESWM_RGMII1: RGMII1_RX_CTL; ESWM_RMII1: RMII1_CRS_DV; GPT0: GTCPPO0; GPT_OPS: GTIU; IRQ: IRQ0-DS; SDHI0: SD0DAT7; SSIE1: SSIDATA1; ULPT1: ULPTOB1; USB FS: USB_VBUSEN" - None - - 
      P207 A17 - LCD_D9 - - Disabled - - "ESWM_GMII/MII1: ET1_RXD5; GLCDC: LCD_DATA9; GPT3: GTCPPO3; IRQ: IRQ25" - None - - 
      P208 C7 - DEBUG_TDI - - Disabled - - "CANFD1: CRX1; CMPOUT: VCOUT; GPT1: GTIOC1B; GPT_OPS: GTOVLO; IRQ: IRQ3; JTAG/SWD: TDI; SCI9: RXD9" - None - - 
      P209 E7 - DEBUG_TDO_SWO - - Disabled - - "CANFD1: CTX1; CLKOUT: CLKOUT; GPT1: GTIOC1A; GPT_OPS: GTOVUP; IRQ: IRQ25; JTAG/SWD: TDO; SCI9: TXD9; TRACE: SWO" - None - - 
      P210 C6 JTAG/SWD_SWDIO DEBUG_TMS_SWDIO L None "Peripheral mode" - - "GPT0: GTIOC0B; GPT_OPS: GTOULO; IRQ: IRQ24; JTAG/SWD: SWDIO; JTAG/SWD: TMS; SCI9: CTS_RTS9; SCI9: DE9" - IO - - 
      P211 D6 JTAG/SWD_SWCLK DEBUG_TCLK_SWCLK L None "Peripheral mode" - - "GPT0: GTIOC0A; GPT_OPS: GTOUUP; IRQ: IRQ23; JTAG/SWD: SWCLK; JTAG/SWD: TCK; SCI9: DE9; SCI9: SCK9" - IO - - 
      P212 K17 - EXTAL - - Disabled - - "AGT1: AGTEE1; CGC: EXTAL; GPT0: GTIOC0B; GPT_POEGD: GTETRGD; IRQ: IRQ3; SCI1: RXD1" - None - - 
      P213 K16 - XTAL - - Disabled - - "ADC1(Digital): ADTRG1; CGC: XTAL; GPT0: GTIOC0A; GPT_POEGC: GTETRGC; IRQ: IRQ2; SCI1: TXD1; ULPT0: ULPTEE0" - None - - 
      P214 L16 - XCOUT - - Disabled - - "CGC: XCOUT; IRQ: IRQ21" - None - - 
      P215 L17 - XCIN - - Disabled - - "CGC: EXCIN; CGC: XCIN; IRQ: IRQ20" - None - - 
      P300 B5 - SDRAM_DQ2 - - Disabled - - "BUS: D2; GLCDC: LCD_DATA11; GPT3: GTIOC3A; IRQ: IRQ4; SCI0: DE0; SCI0: SCK0; SDHI0: SD0DAT3; SDRAM: DQ2; SPI0: SSLA3; ULPT0: ULPTEVI0-DS" - None - - 
      P301 C4 - SDRAM_DQ1 - - Disabled - - "AGT0: AGTIO0; BUS: D1; GLCDC: LCD_DATA12; GPT4: GTIOC4B; GPT_OPS: GTOULO; IRQ: IRQ6; SCI6: TXD6; SDHI0: SD0DAT2; SDRAM: DQ1; ULPT0: ULPTEE0-DS" - None - - 
      P302 A5 - SDRAM_DQ0 - - Disabled - - "BUS: D0; GLCDC: LCD_DATA13; GPT4: GTIOC4A; GPT_OPS: GTOUUP; IRQ: IRQ5; SCI6: RXD6; SDHI0: SD0DAT1; SDRAM: DQ0; ULPT0: ULPTO0-DS" - None - - 
      P303 B6 - USER_LED2_GREEN - - Disabled - - "GLCDC: LCD_DATA14; GPT7: GTIOC7B; IRQ: IRQ29-DS; SCI6: DE6; SCI6: SCK6" - None - - 
      P304 D10 - ETH_TXD3_TRACE_TDATA3 - - Disabled - - "CEU: VIO_D15; ESWM_GMII/MII1: ET1_TXD3; ESWM_RGMII1: RGMII1_TXD3; GPT7: GTIOC7A; GPT_OPS: GTOVLO; IRQ: IRQ9; SDHI0: SD0DAT0; TRACE: TDATA3; ULPT1: ULPTO1" - None - - 
      P305 C10 - ETH_TXD2_TRACE_TDATA2 - - Disabled - - "CEU: VIO_D14; ESWM_GMII/MII1: ET1_TXD2; ESWM_RGMII1: RGMII1_TXD2; GPT12: GTCPPO12; GPT_OPS: GTOVUP; IRQ: IRQ8; SDHI0: SD0WP; TRACE: TDATA2; ULPT1: ULPTEE1" - None - - 
      P306 D11 - ETH_TXD1_TRACE_TDATA1 - - Disabled - - "CEU: VIO_D13; ESWM_GMII/MII1: ET1_TXD1; ESWM_RGMII1: RGMII1_TXD1; ESWM_RMII1: RMII1_TXD1; GPT11: GTCPPO11; GPT_OPS: GTIW; IRQ: IRQ28-DS; SDHI0: SD0CD; TRACE: TDATA1; ULPT1: ULPTEVI1" - None - - 
      P307 C11 - ETH_TXD0_TRACE_TDATA0 - - Disabled - - "CEU: VIO_D12; ESWM_GMII/MII1: ET1_TXD0; ESWM_RGMII1: RGMII1_TXD0; ESWM_RMII1: RMII1_TXD0; GPT10: GTCPPO10; GPT_OPS: GTIV; IRQ: IRQ27-DS; SCI6: CTS_RTS6; SCI6: DE6; SDHI0: SD0CMD; TRACE: TDATA0; ULPT1: ULPTOA1" - None - - 
      P308 C9 - TRACE_TCLK - - Disabled - - "CEU: VIO_D11; ESWM_GMII/MII1: ET1_TX_ER; ETHPHYCLK: ETHPHYCLK; GPT9: GTCPPO9; GPT_OPS: GTIU; IRQ: IRQ26-DS; SCI3: CTS3; SDHI0: SD0CLK; TRACE: TCLK; ULPT1: ULPTOB1" - None - - 
      P309 A12 - ETH_TX_CLK - - Disabled - - "CEU: VIO_D10; CMPOUT: VCOUT; ESWM_GMII/MII1: ET1_GTX_CLK; ESWM_RGMII1: RGMII1_TXC; GLCDC: LCD_DATA15; GPT8: GTCPPO8; IRQ: IRQ25-DS; SCI9: CTS9" - None - - 
      P310 E10 - ETH_TX_CTL - - Disabled - - "AGT1: AGTEE1; CEU: VIO_D9; ESWM_GMII/MII1: ET1_TX_EN; ESWM_RGMII1: RGMII1_TX_CTL; ESWM_RMII1: RMII1_TX_EN; GLCDC: LCD_DATA16; GPT7: GTCPPO7; IRQ: IRQ24-DS; SCI3: TXD3" - None - - 
      P311 B12 - CAM_D8 - - Disabled - - "AGT1: AGTOB1; CANFD0: CRX0; CEU: VIO_D8; ESWM_GMII/MII1: ET1_TX_CLK; GLCDC: LCD_DATA17; GPT: GTADSM1; GPT6: GTCPPO6; IRQ: IRQ23-DS; SCI3: DE3; SCI3: SCK3" - None - - 
      P312 C13 - ARDUINO_D7 - - Disabled - - "AGT1: AGTOA1; CANFD0: CTX0; CEU: VIO_D7; ESWM_GMII/MII1: ET1_RX_ER; ESWM_RMII1: RMII1_RX_ER; GLCDC: LCD_DATA18; GPT: GTADSM0; GPT5: GTCPPO5; IRQ: IRQ22-DS; PDM2: PDMDAT2; SCI3: CTS_RTS3; SCI3: DE3" - None - - 
      P400 P17 - CAM_D0_ARDUINO_GROVE1_SCL0 - - Disabled - - "ADC1(Digital): ADTRG1; AGT1: AGTIO1; CEU: VIO_D0; GPT6: GTIOC6A; I3C0: I3C_SCL0; IRQ: IRQ0; SCI1: TXD1; SDHI1: SD1CLK; SSIE: AUDIO_CLK" - None - - 
      P401 N17 - ARDUINO_GROVE1_SDA0 - - Disabled - - "CANFD0: CTX0; CEU: VIO_D1; GPT6: GTIOC6B; GPT_POEGA: GTETRGA; I3C0: I3C_SDA0; IRQ: IRQ5-DS; SCI1: RXD1; SDHI1: SD1CMD" - None - - 
      P402 L14 - PMOD1_8_GPIO_RST - - Disabled - - "CAC: CACREF; CANFD0: CRX0; ESWM_GMII/MII: ET0_LINKSTA; ESWM_RGMII0: ET0_LINKSTA; ESWM_RMII0: ET0_LINKSTA; IRQ: IRQ4-DS; RTC: RTCIC0; SCI1: DE1; SCI1: SCK1; SDHI1: SD1DAT0; SSIE: AUDIO_CLK" - None - - 
      P403 H13 - AUDIO_BCLK - - Disabled - - "ADC0(Digital): AD0FLAG1; ESWM_GMII/MII: ET1_WOL; ESWM_RGMII1: ET1_WOL; ESWM_RMII1: ET1_WOL; GPT3: GTIOC3A; IRQ: IRQ14-DS; RTC: RTCIC1; SCI1: CTS_RTS1; SCI1: DE1; SDHI1: SD1DAT1; SSIE0: SSIBCK0" - None - - 
      P404 J13 - AUDIO_WCLK - - Disabled - - "ADC1(Digital): AD1FLAG1; ESWM_GMII/MII: ET0_WOL; ESWM_RGMII0: ET0_WOL; ESWM_RMII0: ET0_WOL; GPT3: GTIOC3B; IRQ: IRQ15-DS; RTC: RTCIC2; SCI1: CTS1; SDHI1: SD1DAT2; SSIE0: SSILRCK0" - None - - 
      P405 G12 - CAM_D2_AUDIO_DATIN - - Disabled - - "AGT1: AGTIO1; CEU: VIO_D2; ESWM_GMII/MII0: ET0_RX_DV; ESWM_RGMII0: RGMII0_RX_CTL; ESWM_RMII0: RMII0_CRS_DV; GPT1: GTIOC1A; IRQ: IRQ30; SCI2: DE2; SCI2: SCK2; SDHI1: SD1DAT3; SSIE0: SSITXD0" - None - - 
      P406 F14 - CAM_D3_AUDIO_DOUT - - Disabled - - "CEU: VIO_D3; ESWM_GMII/MII0: ET0_RXD3; ESWM_RGMII0: RGMII0_RXD3; GPT1: GTIOC1B; IRQ: IRQ31; SCI2: TXD2; SDHI1: SD1CD; SPI0: SSLA3; SSIE0: SSIRXD0" - None - - 
      P407 R17 - USBFS_VBUS - - Disabled - - "ADC0(Digital): ADTRG0; AGT0: AGTIO0; BUS: CS6; ESWM_GMII/MII: GPTP_PTPOUT3; ESWM_RGMII: GPTP_PTPOUT3; ESWM_RMII: GPTP_PTPOUT3; GPT10: GTIOC10B; IIC0: SDA0; IRQ: IRQ22; RTC: RTCOUT; SCI1: DE1; SCI1: SCK1; USB FS: USB_VBUS; USB HS: USBHS_VBUSEN" - None - - 
      P408 M15 - USBHS_VBUS - - Disabled - - "ADC(Digital): ADSYNC; BUS: A17; ESWM_GMII/MII: GPTP_PTPOUT2; ESWM_RGMII: GPTP_PTPOUT2; ESWM_RMII: GPTP_PTPOUT2; GPT10: GTIOC10A; GPT_OPS: GTOWLO; IIC0: SCL0; IRQ: IRQ7; SCI3: RXD3; ULPT0: ULPTOB0; USB FS: USB_VBUSEN; USB HS: USBHS_VBUS" - None - - 
      P409 R16 - PMOD2_9_GPIO - - Disabled - - "ADC1(Digital): ADST1; BUS: A18; ESWM_GMII/MII: GPTP0_CAPTURE; ESWM_RGMII0: GPTP0_CAPTURE; ESWM_RMII0: GPTP0_CAPTURE; GPT_OPS: GTOWUP; IIC0: SDA0; IRQ: IRQ6; SCI3: TXD3; ULPT0: ULPTOA0; USB FS: USB_OVRCURA-DS; USB HS: USBHS_OVRCURA" - None - - 
      P410 K13 - PMOD2_8_GPIO_RST - - Disabled - - "ADC0(Digital): ADST0; AGT1: AGTOB1; BUS: A19; ESWM_GMII/MII: GPTP0_MATCH; ESWM_RGMII0: GPTP0_MATCH; ESWM_RMII0: GPTP0_MATCH; GPT9: GTIOC9B; GPT_OPS: GTOVLO; IIC0: SCL0; IRQ: IRQ5; SCI3: DE3; SCI3: SCK3; USB FS: USB_OVRCURB-DS; USB HS: USBHS_OVRCURB" - None - - 
      P411 M14 - DSI_TE - - Disabled - - "AGT1: AGTOA1; BUS: A20; CAC: CACREF; ESWM_GMII/MII: GPTP_PTPOUT1; ESWM_RGMII: GPTP_PTPOUT1; ESWM_RMII: GPTP_PTPOUT1; GPT9: GTIOC9A; GPT_OPS: GTOVUP; IRQ: IRQ4; MIPI: DSI_TE; SCI3: CTS_RTS3; SCI3: DE3; USB FS: USB_ID; USB HS: USBHS_ID" - None - - 
      P412 M12 - PMOD1_9_GPIO - - Disabled - - "AGT1: AGTEE1; BUS: A21; ESWM_GMII/MII: GPTP_PTPOUT0; ESWM_RGMII: GPTP_PTPOUT0; ESWM_RMII: GPTP_PTPOUT0; GPT8: GTCPPO8; GPT_OPS: GTOULO; IRQ: IRQ20-DS; SCI3: CTS3; USB FS: USB_EXICEN; USB HS: USBHS_EXICEN" - None - - 
      P413 P14 - PMOD1_10_GPIO - - Disabled - - "BUS: A22; ESWM_GMII/MII: ET_TAS_STA3; ESWM_RGMII: ET_TAS_STA3; ESWM_RMII: ET_TAS_STA3; GPT7: GTCPPO7; GPT_OPS: GTOUUP; IRQ: IRQ18; ULPT1: ULPTEE1" - None - - 
      P414 L13 - ETH_MDIO - - Disabled - - "BUS: A23; CANFD1: CRX1; CEU: VIO_CLK; ESWM_GMII/MII: ET1_MDIO; ESWM_RGMII1: ET1_MDIO; ESWM_RMII1: ET1_MDIO; GPT0: GTIOC0B; IRQ: IRQ9; SCI4: RXD4; SPI1: SSLB0" - None - - 
      P415 R15 - ETH_MDC - - Disabled - - "BUS: WAIT; CANFD1: CTX1; CEU: VIO_HD; ESWM_GMII/MII: ET1_MDC; ESWM_RGMII1: ET1_MDC; ESWM_RMII1: ET1_MDC; GPT0: GTIOC0A; IRQ: IRQ8; SCI4: TXD4; SPI1: RSPCK1" - None - - 
      P500 U7 - USBFS_VBUSEN - - Disabled - - "ADC0: AN021; ADC1: AN021; CAC: CACREF; GPT11: GTIOC11B; IRQ: IRQ24; PDM0: PDMDAT0; SCI8: RXD8; SDHI1: SD1DAT5; USB FS: USB_VBUSEN" - None - - 
      P501 R8 - CAM_XCLK - - Disabled - - "ADC0: AN020; ADC1: AN020; GPT12: GTIOC12A; IRQ: IRQ25; PDM1: PDMDAT1; SCI8: TXD8; SDHI1: SD1DAT6; USB FS: USB_OVRCURA" - None - - 
      P502 T7 PDM2_PDMDAT2 MEMS_MIC_DATA L None "Peripheral mode" - - "ADC0: AN019; ADC1: AN019; GPT12: GTIOC12B; IRQ: IRQ26; PDM2: PDMDAT2; SCI8: DE8; SCI8: SCK8; SDHI1: SD1DAT7; USB FS: USB_OVRCURB" - I - - 
      P503 H2 - SDRAM_A4 - - Disabled - - "BUS: A6; CEU: VIO_D4; GPT6: GTCPPO6; GPT_OPS: GTOUUP; IRQ: IRQ6; SDHI0: SD0CD; SDRAM: A6" - None - - 
      P504 H1 - SDRAM_A5 - - Disabled - - "BUS: A7; CEU: VIO_D3; GPT1: GTCPPO1; GPT_OPS: GTOULO; IRQ: IRQ7; SDHI0: SD0WP; SDRAM: A7" - None - - 
      P505 H3 - SDRAM_A6 - - Disabled - - "BUS: A8; CEU: VIO_D2; GPT2: GTCPPO2; GPT_OPS: GTOWUP; IRQ: IRQ8; SDHI0: SD0CLK; SDRAM: A8" - None - - 
      P506 J1 - SDRAM_A7 - - Disabled - - "BUS: A9; CEU: VIO_D1; GPT3: GTCPPO3; GPT_OPS: GTOWLO; IRQ: IRQ9; SDHI0: SD0CMD; SDRAM: A9" - None - - 
      P507 J2 - SDRAM_A8 - - Disabled - - "BUS: A10; CEU: VIO_D0; ESWM_GMII/MII: ET_TAS_STA0; ESWM_RGMII: ET_TAS_STA0; ESWM_RMII: ET_TAS_STA0; GLCDC: LCD_EXTCLK; GPT: GTADSM0; GPT0: GTIOC0A; IRQ: IRQ10; SCI7: CTS_RTS7; SCI7: DE7; SDRAM: A10" - None - - 
      P508 J3 - SDRAM_A9 - - Disabled - - "BUS: A11; CEU: VIO_VD; ESWM_GMII/MII: ET_TAS_STA1; ESWM_RGMII: ET_TAS_STA1; ESWM_RMII: ET_TAS_STA1; GPT: GTADSM1; GPT0: GTIOC0B; IRQ: IRQ1; SCI5: CTS5; SDRAM: A11" - None - - 
      P509 J4 - SDRAM_A10 - - Disabled - - "BUS: A12; CEU: VIO_HD; ESWM_GMII/MII: ET_TAS_STA2; ESWM_RGMII: ET_TAS_STA2; ESWM_RMII: ET_TAS_STA2; GPT1: GTIOC1A; IRQ: IRQ2; SCI5: CTS_RTS5; SCI5: DE5; SDRAM: A12; ULPT1: ULPTEVI1" - None - - 
      P510 K3 - SDRAM_A11 - - Disabled - - "BUS: A13; CEU: VIO_CLK; ESWM_GMII/MII: ET_TAS_STA3; ESWM_RGMII: ET_TAS_STA3; ESWM_RMII: ET_TAS_STA3; GPT1: GTIOC1B; IRQ: IRQ3; SCI5: RXD5; SDRAM: A13; ULPT0: ULPTEVI0" - None - - 
      P511 U15 - IIC_SYSTEM_SDA1 - - Disabled - - "CANFD1: CRX1; ESWM_GMII/MII: ET1_LINKSTA; ESWM_RGMII1: ET1_LINKSTA; ESWM_RMII1: ET1_LINKSTA; GPT0: GTIOC0B; IIC1: SDA1; IRQ: IRQ15; SCI8: CTS_RTS8; SCI8: DE8" - None - - 
      P512 P13 - IIC_SYSTEM_SCL1 - - Disabled - - "CANFD1: CTX1; ESWM_GMII/MII: ET1_INT; ESWM_RGMII1: ET1_INT; ESWM_RMII1: ET1_INT; GPT0: GTIOC0A; IIC1: SCL1; IRQ: IRQ14; SCI8: CTS8" - None - - 
      P513 R13 - LCD_TCON3 - - Disabled - - "ACMPHS: IVCMP0; ADC0: AN016; ADC1: AN016; CEU: VIO_FLD; ESWM_GMII/MII: ET0_INT; ESWM_RGMII0: ET0_INT; ESWM_RMII0: ET0_INT; GLCDC: LCD_TCON3; GPT13: GTIOC13B; IRQ: IRQ31; SCI8: DE8; SCI8: SCK8" - None - - 
      P514 R14 - ETH_RST - - Disabled - - "ESWM_GMII/MII: ET_TAS_STA1; ESWM_RGMII: ET_TAS_STA1; ESWM_RMII: ET_TAS_STA1; GLCDC: LCD_EXTCLK; GPT13: GTIOC13B; IIC2: SDA2; IRQ: IRQ13; SCI4: DE4; SCI4: SCK4" - None - - 
      P515 P15 - LCD_CLK - - Disabled - - "ESWM_GMII/MII: ET_TAS_STA0; ESWM_RGMII: ET_TAS_STA0; ESWM_RMII: ET_TAS_STA0; GLCDC: LCD_CLK; GPT13: GTIOC13A; IIC2: SCL2; IRQ: IRQ12; SCI4: CTS_RTS4; SCI4: DE4" - None - - 
      P600 P3 - USER_LED1_BLUE - - Disabled - - "CAC: CACREF; ESWM_GMII/MII: ET1_WOL; ESWM_RGMII1: ET1_WOL; ESWM_RMII1: ET1_WOL; GPT6: GTIOC6B; IRQ: IRQ30; OSPI0: OM_0_RSTO1; ULPT1: ULPTEVI1-DS" - None - - 
      P601 P4 - PMOD2_4_RSPCKB - - Disabled - - "GPT6: GTIOC6A; IRQ: IRQ29; OSPI0: OM_0_WP1; RTC: RTCOUT; SCI0: DE0; SCI0: SCK0; ULPT0: ULPTEVI0" - None - - 
      P602 P2 - PMOD2_3_MISOB_RXD0 - - Disabled - - "GPT7: GTIOC7B; IRQ: IRQ28; OSPI1: OM_1_SCLKN; SCI0: RXD0; ULPT0: ULPTEE0" - None - - 
      P603 P1 - PMOD2_2_MOSIB_TXD0 - - Disabled - - "GPT7: GTIOC7A; IRQ: IRQ27; OSPI1: OM_1_SCLK; SCI0: TXD0; ULPT0: ULPTO0" - None - - 
      P604 N2 - PMOD2_1_SSLB0_CTS_RTS0 - - Disabled - - "GPT8: GTIOC8B; IRQ: IRQ26; OSPI1: OM_1_SIO7; SCI0: CTS_RTS0; SCI0: DE0" - None - - 
      P605 N1 - PMOD2_1_CTS0 - - Disabled - - "GPT8: GTIOC8A; IRQ: IRQ25; OSPI1: OM_1_SIO1; SCI0: CTS0" - None - - 
      P606 N3 - LCD_RST - - Disabled - - "BUS: BC3; BUS: WR3; IRQ: IRQ24; OSPI1: OM_1_SIO6" - None - - 
      P607 M2 - SDRAM_DQ31 - - Disabled - - "BUS: D31; IRQ: IRQ23; OSPI1: OM_1_DQS; SDRAM: DQ31" - None - - 
      P608 K2 - SDRAM_A12 - - Disabled - - "BUS: A14; CAC: CACREF; CEU: VIO_FLD; GPT4: GTCPPO4; GPT_OPS: GTOWUP; IRQ: IRQ22; SCI5: TXD5; SDRAM: A14" - None - - 
      P609 A1 - SDRAM_DQ7 - - Disabled - - "ADC1(Digital): AD1FLAG1; BUS: D7; CANFD1: CTX1; GLCDC: LCD_DATA6; GPT5: GTIOC5B; GPT_OPS: GTIU; IRQ: IRQ29; SCI0: TXD0; SDRAM: DQ7; SPI0: MISO0; ULPT1: ULPTOA1-DS" - None - - 
      P610 D3 - SDRAM_DQ12 - - Disabled - - "BUS: D12; CANFD1: CRX1; GLCDC: LCD_DATA5; GPT4: GTIOC4A; GPT_OPS: GTOUUP; IRQ: IRQ16; SCI0: RXD0; SDRAM: DQ12; SPI0: RSPCK0; ULPT1: ULPTOB1-DS" - None - - 
      P611 D2 - SDRAM_DQ13 - - Disabled - - "BUS: D13; CAC: CACREF; CLKOUT: CLKOUT; GLCDC: LCD_DATA4; GPT4: GTIOC4B; GPT_OPS: GTOULO; IRQ: IRQ17; SCI0: DE0; SCI0: SCK0; SDRAM: DQ13; SPI0: MOSI0; USB HS: USBHS_VBUSEN" - None - - 
      P612 E4 - SDRAM_DQ14 - - Disabled - - "BUS: D14; GLCDC: LCD_DATA3; GPT9: GTIOC9A; IRQ: IRQ18; SCI0: CTS_RTS0; SCI0: DE0; SDRAM: DQ14; SPI0: SSLA0; USB HS: USBHS_OVRCURA" - None - - 
      P613 C2 - SDRAM_DQ15 - - Disabled - - "AGT1: AGTO1; BUS: D15; GLCDC: LCD_DATA2; GPT9: GTIOC9B; GPT_POEGA: GTETRGA; IRQ: IRQ19; SCI0: CTS0; SDRAM: DQ15; USB HS: USBHS_OVRCURB" - None - - 
      P614 E3 - SDRAM_DQM0 - - Disabled - - "AGT0: AGTO0; BUS: WR; BUS: WR0; GLCDC: LCD_DATA1; GPT9: GTCPPO9; GPT_POEGB: GTETRGB; IRQ: IRQ20; SCI7: RXD7; SDRAM: DQM0; USB HS: USBHS_ID" - None - - 
      P615 E2 - SDRAM_DQM2 - - Disabled - - "BUS: BC2; BUS: WR2; GLCDC: LCD_DATA0; GPT10: GTCPPO10; GPT_POEGC: GTETRGC; IRQ: IRQ7; SCI7: TXD7; SDRAM: DQM2; USB HS: USBHS_EXICEN" - None - - 
      P700 F12 - CAM_D4 - - Disabled - - "CEU: VIO_D4; ESWM_GMII/MII0: ET0_RXD2; ESWM_RGMII0: RGMII0_RXD2; GPT5: GTIOC5A; IRQ: IRQ16-DS; SCI2: RXD2; SDHI1: SD1WP; SPI0: MISO0; SSIE1: SSIDATA1" - None - - 
      P701 F15 - CAM_D5 - - Disabled - - "CEU: VIO_D5; ESWM_GMII/MII0: ET0_RXD1; ESWM_RGMII0: RGMII0_RXD1; ESWM_RMII0: RMII0_RXD1; GPT5: GTIOC5B; IRQ: IRQ17-DS; SCI2: CTS_RTS2; SCI2: DE2; SDHI1: SD1DAT4; SPI0: MOSI0; SSIE1: SSILRCK1; ULPT1: ULPTO1" - None - - 
      P702 F13 - CAM_D6 - - Disabled - - "CEU: VIO_D6; ESWM_GMII/MII0: ET0_RXD0; ESWM_RGMII0: RGMII0_RXD0; ESWM_RMII0: RMII0_RXD0; GPT6: GTIOC6A; IRQ: IRQ18-DS; SCI2: CTS2; SDHI1: SD1DAT5; SPI0: RSPCK0; SSIE1: SSIBCK1; ULPT0: ULPTO0" - None - - 
      P703 G14 - CAM_D7 - - Disabled - - "AGT1: AGTO1; CEU: VIO_D7; CMPOUT: VCOUT; ESWM_GMII/MII0: ET0_RX_CLK; ESWM_RGMII0: RGMII0_RXC; ESWM_RMII0: RMII0_REF50CK; GPT6: GTIOC6B; IRQ: IRQ19-DS; PDM0: PDMCLK0; SDHI1: SD1DAT6; SPI0: SSLA0" - None - - 
      P704 G13 - PMOD2_10_GPIO - - Disabled - - "AGT0: AGTO0; CANFD0: CTX0; CEU: VIO_D8; ESWM_GMII/MII0: ET0_RX_ER; ESWM_RMII0: RMII0_RX_ER; GPT: GTADSM0; GPT0: GTCPPO0; IRQ: IRQ26; PDM1: PDMCLK1; SDHI1: SD1DAT7; SPI0: SSLA1" - None - - 
      P705 F17 - CAM_D9 - - Disabled - - "AGT0: AGTIO0; CANFD0: CRX0; CEU: VIO_D9; ESWM_GMII/MII0: ET0_TX_EN; ESWM_RGMII0: RGMII0_TX_CTL; ESWM_RMII0: RMII0_TX_EN; GPT: GTADSM1; GPT1: GTCPPO1; IRQ: IRQ19; PDM2: PDMCLK2; SCI1: CTS1; SPI0: SSLA2" - None - - 
      P706 E17 - CAM_D10 - - Disabled - - "AGT0: AGTIO0; CEU: VIO_D10; ESWM_GMII/MII0: ET0_GTX_CLK; ESWM_RGMII0: RGMII0_TXC; ETHPHYCLK: ETHPHYCLK; GPT2: GTCPPO2; IRQ: IRQ7; PDM0: PDMDAT0; SCI1: RXD1; USB HS: USBHS_OVRCURB-DS" - None - - 
      P707 F16 - LCD_D18_CAM_D11 - - Disabled - - "CEU: VIO_D11; ESWM_GMII/MII0: ET0_TX_ER; ETHPHYCLK: ETHPHYCLK; GLCDC: LCD_DATA18; GPT3: GTCPPO3; IRQ: IRQ8; PDM1: PDMDAT1; SCI1: TXD1; USB HS: USBHS_OVRCURA-DS" - None - - 
      P708 N12 - LCD_BLEN - - Disabled - - "BUS: BC1; BUS: WR1; CAC: CACREF; CEU: VIO_VD; ESWM_GMII/MII: ET0_MDC; ESWM_RGMII0: ET0_MDC; ESWM_RMII0: ET0_MDC; GPT6: GTCPPO6; IIC2: SDA2; IRQ: IRQ11; SCI4: DE4; SCI4: SCK4; SPI1: MOSI1; SSIE: AUDIO_CLK" - None - - 
      P709 P16 - CAM_RST - - Disabled - - "BUS: CS4; CEU: VIO_D13; ESWM_GMII/MII: ET0_MDIO; ESWM_RGMII0: ET0_MDIO; ESWM_RMII0: ET0_MDIO; GPT5: GTCPPO5; IIC2: SCL2; IRQ: IRQ10; SCI4: CTS_RTS4; SCI4: DE4; SPI1: MISO1" - None - - 
      P710 M13 - LCD_EXTCLK - - Disabled - - "BUS: CS5; CEU: VIO_D12; ESWM_GMII/MII: ET0_LINKSTA; ESWM_RGMII0: ET0_LINKSTA; ESWM_RMII0: ET0_LINKSTA; GLCDC: LCD_EXTCLK; GPT11: GTIOC11B; IRQ: IRQ17; SCI4: CTS4; SPI1: SSLB3" - None - - 
      P711 N15 - LCD_D19 - - Disabled - - "AGT0: AGTEE0; ESWM_GMII/MII: GPTP0_PPS; ESWM_RGMII0: GPTP0_PPS; ESWM_RMII0: GPTP0_PPS; GLCDC: LCD_DATA19; GPT11: GTIOC11A; IRQ: IRQ3; SCI1: CTS_RTS1; SCI1: DE1; SPI1: SSLB2" - None - - 
      P712 N13 - LCD_D20 - - Disabled - - "AGT0: AGTOB0; ESWM_GMII/MII: GPTP1_CAPTURE; ESWM_RGMII1: GPTP1_CAPTURE; ESWM_RMII1: GPTP1_CAPTURE; GLCDC: LCD_DATA20; GPT2: GTIOC2B; IRQ: IRQ2; SCI1: CTS1; SPI1: SSLB1" - None - - 
      P713 N16 - LCD_D21 - - Disabled - - "AGT0: AGTOA0; ESWM_GMII/MII: GPTP1_MATCH; ESWM_RGMII1: GPTP1_MATCH; ESWM_RMII1: GPTP1_MATCH; GLCDC: LCD_DATA21; GPT2: GTIOC2A; IRQ: IRQ14; SCI4: CTS4" - None - - 
      P714 N14 - LCD_D22 - - Disabled - - "ESWM_GMII/MII: GPTP1_PPS; ESWM_RGMII1: GPTP1_PPS; ESWM_RMII1: GPTP1_PPS; GLCDC: LCD_DATA22; GPT12: GTIOC12B; IRQ: IRQ13; MIPI: DSI_TE; SCI4: TXD4" - None - - 
      P715 T15 - LCD_D23 - - Disabled - - "ESWM_GMII/MII: ET_TAS_STA2; ESWM_RGMII: ET_TAS_STA2; ESWM_RMII: ET_TAS_STA2; GLCDC: LCD_DATA23; GPT12: GTIOC12A; IRQ: IRQ12; SCI4: RXD4" - None - - 
      P800 T6 - OSPI_DQ5_PMOD1_1_CTS2 - - Disabled - - "AGT0: AGTOA0; GPT11: GTIOC11A; GPT_OPS: GTIU; IRQ: IRQ11; OSPI0: OM_0_SIO5; SCI2: CTS2" - None - - 
      P801 P6 SCI2_TXD2 OSPI_DS L None "Peripheral mode" - - "AGT0: AGTOB0; ESWM_GMII/MII: GPTP1_PPS; ESWM_RGMII1: GPTP1_PPS; ESWM_RMII1: GPTP1_PPS; GPT11: GTIOC11B; GPT_OPS: GTIV; IRQ: IRQ12; OSPI0: OM_0_DQS; SCI2: TXD2" - O - - 
      P802 R6 - OSPI_DQ6 - - Disabled - - "GPT12: GTIOC12A; GPT_OPS: GTIW; IRQ: IRQ18; OSPI0: OM_0_SIO6; SCI2: RXD2" - None - - 
      P803 P7 - OSPI_DQ1 - - Disabled - - "GPT12: GTIOC12B; GPT_POEGC: GTETRGC; IRQ: IRQ19; OSPI0: OM_0_SIO1; SCI2: DE2; SCI2: SCK2" - None - - 
      P804 R7 - OSPI_DQ7 - - Disabled - - "GPT13: GTIOC13A; GPT_POEGD: GTETRGD; IRQ: IRQ14; MIPI: DSI_TE; OSPI0: OM_0_SIO7; SCI2: CTS_RTS2; SCI2: DE2" - None - - 
      P805 P12 - LCD_HSYNC_TCON1 - - Disabled - - "ACMPHS: IVCMP0; ADC0: AN017; ADC1: AN017; CEU: VIO_D15; ESWM_GMII/MII: ET1_MDIO; ESWM_RGMII1: ET1_MDIO; ESWM_RMII1: ET1_MDIO; GLCDC: LCD_TCON1; IRQ: IRQ30; SCI8: TXD8" - None - - 
      P806 T14 - LCD_VSYNC_TCON0 - - Disabled - - "ADC0: AN018; ADC1: AN018; CEU: VIO_D14; ESWM_GMII/MII: ET1_MDC; ESWM_RGMII1: ET1_MDC; ESWM_RMII1: ET1_MDC; GLCDC: LCD_TCON0; IRQ: IRQ0; SCI8: RXD8" - None - - 
      P807 N11 - LCD_DE_TCON2 - - Disabled - - "GLCDC: LCD_TCON2; GPT13: GTIOC13A; IRQ: IRQ11" - None - - 
      P808 U5 - OSPI_SCLK_ARDUINO_D0_RXD_MIKROBUS_RXD - - Disabled - - "GPT13: GTIOC13B; IRQ: IRQ15; OSPI0: OM_0_SCLK; SCI7: RXD7" - None - - 
      P809 T5 - ARDUINO_D1_TXD_MIKROBUS_TXD - - Disabled - - "IRQ: IRQ20; OSPI0: OM_0_SCLKN; SCI7: TXD7" - None - - 
      P810 M9 - ARDUINO_D4_MIKROBUS_1_PWM - - Disabled - - "GPT10: GTIOC10A; IRQ: IRQ21; PDM0: PDMCLK0; SCI7: DE7; SCI7: SCK7; SDHI1: SD1DAT2; ULPT0: ULPTOA0" - None - - 
      P811 N8 - ARDUINO_D3 - - Disabled - - "GPT10: GTIOC10B; IRQ: IRQ22; PDM1: PDMCLK1; SCI7: CTS7; SDHI1: SD1DAT3; ULPT0: ULPTOB0; USB FS: USB_ID" - None - - 
      P812 P8 PDM2_PDMCLK2 MEMS_MIC_CLK L None "Peripheral mode" - - "ADC0: AN022; ADC1: AN022; GPT11: GTIOC11A; IRQ: IRQ23; PDM2: PDMCLK2; SCI7: CTS_RTS7; SCI7: DE7; SDHI1: SD1DAT4; USB FS: USB_EXICEN" - O - - 
      P813 B1 - SDRAM_CS - - Disabled - - "CEU: VIO_D13; GPT7: GTIOC7B; GPT_POEGA: GTETRGA; IRQ: IRQ15; PDM2: PDMCLK2; SCI7: DE7; SCI7: SCK7; SDRAM: SDCS" - None - - 
      P814 U16 - USBFS_DP - - Disabled - - "CANFD0: CRX0; GPT8: GTIOC8B; IRQ: IRQ16; USB FS: USB_DP" - None - - 
      P815 T16 - USBFS_DN - - Disabled - - "CANFD0: CTX0; GPT8: GTIOC8A; IRQ: IRQ15; USB FS: USB_DM" - None - - 
      P902 E9 - CAM_D1_LCD_D3 - - Disabled - - "BUS: ALE; CEU: VIO_D1; ETHPHYCLK: ETHPHYCLK; GLCDC: LCD_DATA3; GPT13: GTCPPO13; IRQ: IRQ0; SSIE: AUDIO_CLK" - None - - 
      P903 D9 - LCD_D2 - - Disabled - - "GLCDC: LCD_DATA2; GPT11: GTIOC11A; IRQ: IRQ1" - None - - 
      P904 A16 - LCD_D8 - - Disabled - - "ESWM_GMII/MII1: ET1_RXD4; GLCDC: LCD_DATA8; GPT11: GTIOC11B; IRQ: IRQ2" - None - - 
      P905 A14 - ETH_RX_CLK - - Disabled - - "ADC1(Digital): AD1FLAG1; CEU: VIO_D6; ESWM_GMII/MII1: ET1_RX_CLK; ESWM_RGMII1: RGMII1_RXC; ESWM_RMII1: RMII1_REF50CK; GLCDC: LCD_DATA19; GPT13: GTCPPO13; IRQ: IRQ8; PDM1: PDMDAT1; SCI3: RXD3" - None - - 
      P906 A13 - ETH_RXD0 - - Disabled - - "ADC0(Digital): AD0FLAG1; CEU: VIO_D5; ESWM_GMII/MII1: ET1_RXD0; ESWM_RGMII1: RGMII1_RXD0; ESWM_RMII1: RMII1_RXD0; GLCDC: LCD_DATA20; GPT13: GTIOC13B; IRQ: IRQ9; PDM0: PDMDAT0; SCI6: CTS6; SSIE1: SSILRCK1; ULPT1: ULPTO1; USB FS: USB_ID" - None - - 
      P907 A15 - ETH_RXD1 - - Disabled - - "ADC(Digital): ADSYNC; CEU: VIO_D4; ESWM_GMII/MII1: ET1_RXD1; ESWM_RGMII1: RGMII1_RXD1; ESWM_RMII1: RMII1_RXD1; GLCDC: LCD_DATA21; GPT13: GTIOC13A; IRQ: IRQ10; PDM2: PDMCLK2; SCI6: DE6; SCI6: SCK6; SSIE1: SSIBCK1; ULPT1: ULPTEE1; USB FS: USB_EXICEN" - None - - 
      P908 B13 - ETH_RXD2 - - Disabled - - "ADC1(Digital): ADST1; CANFD1: CRX1; CEU: VIO_D3; ESWM_GMII/MII1: ET1_RXD2; ESWM_RGMII1: RGMII1_RXD2; GLCDC: LCD_DATA22; GPT12: GTIOC12B; IRQ: IRQ11; PDM1: PDMCLK1; SCI6: TXD6; ULPT1: ULPTEVI1; USB FS: USB_OVRCURB; USB HS: USBHS_ID" - None - - 
      P909 B14 - ETH_RXD3 - - Disabled - - "ADC0(Digital): ADST0; CANFD1: CTX1; CEU: VIO_D2; ESWM_GMII/MII1: ET1_RXD3; ESWM_RGMII1: RGMII1_RXD3; GLCDC: LCD_DATA23; GPT12: GTIOC12A; IRQ: IRQ21-DS; PDM0: PDMCLK0; SCI6: RXD6; ULPT1: ULPTOA1; USB FS: USB_OVRCURA; USB HS: USBHS_EXICEN" - None - - 
      P910 E11 - LCD_D4 - - Disabled - - "ESWM_GMII/MII1: ET1_TXD4; GLCDC: LCD_DATA4; GPT12: GTCPPO12; IRQ: IRQ7" - None - - 
      P911 C12 - LCD_D5 - - Disabled - - "ESWM_GMII/MII1: ET1_TXD5; GLCDC: LCD_DATA5; GPT3: GTIOC3B; IRQ: IRQ6" - None - - 
      P912 D12 - LCD_D6 - - Disabled - - "ESWM_GMII/MII1: ET1_TXD6; GLCDC: LCD_DATA6; GPT3: GTIOC3A; IRQ: IRQ5" - None - - 
      P913 E12 - LCD_D7 - - Disabled - - "CLKOUT: CLKOUT; ESWM_GMII/MII1: ET1_TXD7; GLCDC: LCD_DATA7; GPT11: GTCPPO11; IRQ: IRQ3" - None - - 
      P914 E5 - LCD_D0 - - Disabled - - "GLCDC: LCD_DATA0; GPT5: GTIOC5B; IRQ: IRQ9; SCI6: CTS_RTS6; SCI6: DE6" - None - - 
      P915 A6 - LCD_D1 - - Disabled - - "GLCDC: LCD_DATA1; GPT5: GTIOC5A; IRQ: IRQ8; SCI6: CTS6" - None - - 
      PA00 G1 - SDRAM_A3 - - Disabled - - "ADC1(Digital): AD1FLAG1; BUS: A5; CEU: VIO_D5; GLCDC: LCD_CLK; GPT7: GTCPPO7; GPT_OPS: GTOVLO; IRQ: IRQ22; SCI5: CTS_RTS5; SCI5: DE5; SDHI0: SD0DAT7; SDRAM: A5" - None - - 
      PA01 H4 - SDRAM_A2 - - Disabled - - "ADC0(Digital): AD0FLAG1; BUS: A4; CEU: VIO_D6; GLCDC: LCD_TCON0; GPT8: GTCPPO8; GPT_OPS: GTOVUP; IRQ: IRQ21; SCI5: CTS5; SDHI0: SD0DAT6; SDRAM: A4" - None - - 
      PA02 F1 SCI2_RXD2 SDRAM_A1 L None "Peripheral mode" - - "ADC(Digital): ADSYNC; BUS: A3; CEU: VIO_D7; GPT9: GTCPPO9; GPT_OPS: GTIW; IRQ: IRQ31; SCI2: RXD2; SDHI0: SD0DAT5; SDRAM: A3" - I - - 
      PA03 G2 - SDRAM_A0 - - Disabled - - "ADC1(Digital): ADST1; BUS: A2; CEU: VIO_D8; GPT10: GTCPPO10; GPT_OPS: GTIV; IRQ: IRQ20; SCI2: TXD2; SDHI0: SD0DAT4; SDRAM: A2" - None - - 
      PA04 D1 - SDRAM_DQM3 - - Disabled - - "ADC0(Digital): ADST0; BUS: A1; CEU: VIO_D9; GPT4: GTIOC4B; GPT_OPS: GTIU; IRQ: IRQ19; SCI2: DE2; SCI2: SCK2; SDHI0: SD0DAT3; SDRAM: A1; SDRAM: DQM3" - None - - 
      PA05 G3 - SDRAM_DQM1 - - Disabled - - "BUS: A0; BUS: BC0; CEU: VIO_D10; GPT4: GTIOC4A; GPT_POEGD: GTETRGD; IRQ: IRQ18; PDM2: PDMDAT2; SCI2: CTS_RTS2; SCI2: DE2; SDHI0: SD0DAT2; SDRAM: A0; SDRAM: DQM1" - None - - 
      PA06 C1 - SDRAM_CKE - - Disabled - - "BUS: CS1; CEU: VIO_D11; GPT7: GTIOC7B; GPT_POEGC: GTETRGC; IRQ: IRQ17; PDM1: PDMDAT1; SCI2: CTS2; SDHI0: SD0DAT1; SDRAM: CKE" - None - - 
      PA07 G4 - USER_LED3_RED - - Disabled - - "BUS: RD; CEU: VIO_D12; CMPOUT: VCOUT; GPT7: GTIOC7A; GPT_POEGB: GTETRGB; IRQ: IRQ16; PDM0: PDMDAT0; SCI7: CTS7; SDHI0: SD0DAT0" - None - - 
      PA08 F3 - SDRAM_WE - - Disabled - - "BUS: CS0; GLCDC: LCD_TCON3; GPT11: GTCPPO11; GPT_POEGD: GTETRGD; IRQ: IRQ6; SCI5: RXD5; SDRAM: WE" - None - - 
      PA09 F4 - SDRAM_CAS - - Disabled - - "BUS: CS3; GLCDC: LCD_TCON2; GPT12: GTCPPO12; IRQ: IRQ5; SCI5: TXD5; SDRAM: CAS" - None - - 
      PA10 F2 - SDRAM_RAS - - Disabled - - "BUS: CS2; CEU: VIO_D15; GLCDC: LCD_TCON1; GPT13: GTCPPO13; IRQ: IRQ4; PDM0: PDMCLK0; SCI5: DE5; SCI5: SCK5; SDRAM: RAS" - None - - 
      PA11 B4 - SDRAM_DQ8 - - Disabled - - "BUS: D8; GPT6: GTIOC6A; GPT_OPS: GTIV; IRQ: IRQ10; SCI9: DE9; SCI9: SCK9; SDRAM: DQ8" - None - - 
      PA12 B2 - SDRAM_DQ9 - - Disabled - - "BUS: D9; GPT6: GTIOC6B; GPT_OPS: GTIW; IRQ: IRQ11; SCI9: RXD9; SDRAM: DQ9" - None - - 
      PA13 C3 - SDRAM_DQ10 - - Disabled - - "BUS: D10; GPT10: GTIOC10A; GPT_OPS: GTOVUP; IRQ: IRQ12; SCI9: CTS_RTS9; SCI9: DE9; SDRAM: DQ10" - None - - 
      PA14 D4 - SDRAM_DQ11 - - Disabled - - "BUS: D11; GPT10: GTIOC10B; GPT_OPS: GTOVLO; IRQ: IRQ13; SCI9: TXD9; SDRAM: DQ11" - None - - 
      PA15 E1 - SDRAM_CLK - - Disabled - - "BUS: EBCLK; CEU: VIO_D14; GPT7: GTIOC7A; IRQ: IRQ14; PDM1: PDMCLK1; SCI9: CTS9; SDRAM: SDCLK" - None - - 
      PB00 E16 - LCD_D17 - - Disabled - - "ADC0(Digital): ADST0; ESWM_GMII/MII0: ET0_TXD0; ESWM_RGMII0: RGMII0_TXD0; ESWM_RMII0: RMII0_TXD0; GLCDC: LCD_DATA17; GPT4: GTCPPO4; IRQ: IRQ10; PDM2: PDMDAT2; SCI1: DE1; SCI1: SCK1; USB HS: USBHS_VBUSEN" - None - - 
      PB01 D17 - LCD_D13 - - Disabled - - "ADC1(Digital): AD1FLAG1; BUS: ALE; CEU: VIO_FLD; ESWM_GMII/MII0: ET0_TX_CLK; GLCDC: LCD_DATA13; GPT2: GTCPPO2; IRQ: IRQ12; SCI1: CTS_RTS1; SCI1: DE1" - None - - 
      PB02 E13 - CAM_VSYNC_LCD_D16 - - Disabled - - "ADC1(Digital): ADST1; CEU: VIO_VD; ESWM_GMII/MII0: ET0_TXD1; ESWM_RGMII0: RGMII0_TXD1; ESWM_RMII0: RMII0_TXD1; GLCDC: LCD_DATA16; GPT0: GTCPPO0; IRQ: IRQ11; SCI5: RXD5" - None - - 
      PB03 D16 - CAM_HSYNC_LCD_D15 - - Disabled - - "ADC(Digital): ADSYNC; CEU: VIO_HD; ESWM_GMII/MII0: ET0_TXD2; ESWM_RGMII0: RGMII0_TXD2; GLCDC: LCD_DATA15; GPT1: GTCPPO1; IRQ: IRQ13; SCI5: TXD5" - None - - 
      PB04 D13 - CAM_PCLK_LCD_D14 - - Disabled - - "ADC0(Digital): AD0FLAG1; CEU: VIO_CLK; ESWM_GMII/MII0: ET0_TXD3; ESWM_RGMII0: RGMII0_TXD3; GLCDC: LCD_DATA14; GPT3: GTCPPO3; IRQ: IRQ9; SCI5: DE5; SCI5: SCK5" - None - - 
      PB05 D15 - LCD_D12 - - Disabled - - "ESWM_GMII/MII0: ET0_TXD7; GLCDC: LCD_DATA12; GPT4: GTCPPO4; IRQ: IRQ15; SCI5: CTS5" - None - - 
      PB06 E14 - LCD_D11 - - Disabled - - "ESWM_GMII/MII0: ET0_TXD6; GLCDC: LCD_DATA11; GPT9: GTIOC9A; IRQ: IRQ0; SCI5: CTS_RTS5; SCI5: DE5" - None - - 
      PB07 D14 - LCD_D10 - - Disabled - - "ESWM_GMII/MII0: ET0_TXD5; GLCDC: LCD_DATA10; GPT9: GTIOC9B; IRQ: IRQ1" - None - - 
      PC00 M1 - SDRAM_DQ30 - - Disabled - - "BUS: D30; GPT7: GTCPPO7; IRQ: IRQ28; OSPI1: OM_1_SIO5; SCI7: CTS_RTS7; SCI7: DE7; SDRAM: DQ30" - None - - 
      PC01 M3 - SDRAM_DQ29 - - Disabled - - "BUS: D29; GPT6: GTCPPO6; IRQ: IRQ27; OSPI1: OM_1_SIO0; SCI7: CTS7; SDRAM: DQ29" - None - - 
      PC02 L2 - SDRAM_DQ28 - - Disabled - - "BUS: D28; GPT5: GTCPPO5; IRQ: IRQ26; OSPI1: OM_1_SIO3; SCI7: DE7; SCI7: SCK7; SDRAM: DQ28" - None - - 
      PC03 L1 - SDRAM_DQ27 - - Disabled - - "BUS: D27; GPT4: GTCPPO4; IRQ: IRQ25; OSPI1: OM_1_SIO4; SCI7: TXD7; SDRAM: DQ27" - None - - 
      PC04 L3 - SDRAM_DQ26 - - Disabled - - "BUS: D26; GPT3: GTCPPO3; IRQ: IRQ24; OSPI1: OM_1_SIO2; SCI7: RXD7; SDRAM: DQ26" - None - - 
      PC05 L5 - SDRAM_DQ25 - - Disabled - - "BUS: D25; GPT2: GTCPPO2; IRQ: IRQ23; OSPI1: OM_1_CS1; SDRAM: DQ25" - None - - 
      PC06 N4 - SDRAM_DQ24 - - Disabled - - "BUS: D24; GPT1: GTCPPO1; IRQ: IRQ22; OSPI1: OM_1_ECSINT1; SDRAM: DQ24" - None - - 
      PC07 K5 - SDRAM_DQ23 - - Disabled - - "BUS: D23; GPT0: GTCPPO0; IRQ: IRQ21; OSPI1: OM_1_RESET; SDRAM: DQ23" - None - - 
      PC08 M4 - SDRAM_DQ22 - - Disabled - - "BUS: D22; GPT8: GTCPPO8; IRQ: IRQ29; OSPI1: OM_1_CS0; SDRAM: DQ22" - None - - 
      PC09 L4 - SDRAM_DQ21 - - Disabled - - "BUS: D21; IRQ: IRQ5; OSPI1: OM_1_RSTO1; SDRAM: DQ21" - None - - 
      PC10 M5 - SDRAM_DQ20 - - Disabled - - "BUS: D20; GPT13: GTCPPO13; IRQ: IRQ4; OSPI1: OM_1_WP1; SDRAM: DQ20" - None - - 
      PC11 H5 - SDRAM_DQ19 - - Disabled - - "BUS: D19; ESWM_GMII/MII: ET0_MDC; ESWM_RGMII0: ET0_MDC; ESWM_RMII0: ET0_MDC; GPT12: GTCPPO12; IRQ: IRQ3; SCI6: CTS_RTS6; SCI6: DE6; SDRAM: DQ19" - None - - 
      PC12 G5 - SDRAM_DQ18 - - Disabled - - "BUS: D18; ESWM_GMII/MII: ET0_MDIO; ESWM_RGMII0: ET0_MDIO; ESWM_RMII0: ET0_MDIO; GPT11: GTCPPO11; IRQ: IRQ2; SCI6: DE6; SCI6: SCK6; SDRAM: DQ18" - None - - 
      PC13 J5 - SDRAM_DQ17 - - Disabled - - "BUS: D17; ESWM_GMII/MII: ET0_INT; ESWM_RGMII0: ET0_INT; ESWM_RMII0: ET0_INT; GPT10: GTCPPO10; IRQ: IRQ1; SCI6: RXD6; SDRAM: DQ17" - None - - 
      PC14 F5 - SDRAM_DQ16 - - Disabled - - "BUS: D16; ESWM_GMII/MII: ET0_WOL; ESWM_RGMII0: ET0_WOL; ESWM_RMII0: ET0_WOL; GPT: GTADSM1; GPT9: GTCPPO9; IRQ: IRQ0; SCI6: TXD6; SDRAM: DQ16" - None - - 
      PC15 K1 - SDRAM_BA1 - - Disabled - - "BUS: A16; CANFD1: CRX1; GPT: GTADSM0; IRQ: IRQ30; SCI6: CTS6; SDRAM: A16" - None - - 
      PD00 K4 - SDRAM_BA0 - - Disabled - - "BUS: A15; CANFD1: CTX1; GPT5: GTCPPO5; GPT_OPS: GTOWLO; IRQ: IRQ23; SCI5: DE5; SCI5: SCK5; SDRAM: A15" - None - - 
      PD01 B16 - ARDUINO_D8_MIKROBUS_INT - - Disabled - - "ESWM_GMII/MII1: ET1_RXD6; GPT2: GTCPPO2; IRQ: IRQ22; SCI8: DE8; SCI8: SCK8; SDHI0: SD0DAT2" - None - - 
      PD02 B17 SCI8_TXD8 JLINK_VCOM_TX L None "Peripheral mode" - - "ESWM_GMII/MII1: ET1_RXD7; GPT1: GTCPPO1; IRQ: IRQ21; SCI8: TXD8; SDHI0: SD0DAT1" - O - - 
      PD03 C15 SCI8_RXD8 JLINK_VCOM_RXD L None "Peripheral mode" - - "ESWM_GMII/MII0: ET0_RXD4; GPT3: GTIOC3B; IRQ: IRQ21; SCI8: RXD8; SDHI0: SD0DAT0; USB HS: USBHS_EXICEN" - I - - 
      PD04 C14 - JLINK_VCOM_CTS_RTS - - Disabled - - "ESWM_GMII/MII0: ET0_RXD5; GPT3: GTIOC3A; IRQ: IRQ20; SCI8: CTS_RTS8; SCI8: DE8; SDHI0: SD0CMD; USB HS: USBHS_ID" - None - - 
      PD05 C16 - JLINK_VCOM_CTS - - Disabled - - "ESWM_GMII/MII0: ET0_RXD6; GPT2: GTIOC2B; IRQ: IRQ19; SCI8: CTS8; SDHI0: SD0CLK; USB HS: USBHS_OVRCURB" - None - - 
      PD06 C17 - AUDIO_MCLK - - Disabled - - "ESWM_GMII/MII0: ET0_RXD7; GPT2: GTIOC2A; IRQ: IRQ18; SDHI0: SD0WP; USB HS: USBHS_OVRCURA" - None - - 
      PD07 E15 - USB_HS_VBUS_SEL - - Disabled - - "ESWM_GMII/MII0: ET0_TXD4; GPT0: GTCPPO0; IRQ: IRQ17; SDHI0: SD0CD; USB HS: USBHS_VBUSEN" - None - - 
      RES D5 CGC_RES - - - - - - - - IO "Read only" - 
      USBHS_DM H17 CGC_USBHS_DM - - - - - - - - IO "Read only" - 
      USBHS_DP H16 CGC_USBHS_DP - - - - - - - - IO "Read only" - 
      USBHS_RREF J15 CGC_USBHS_RREF - - - - - - - - IO "Read only" - 
      VBATT M16 CGC_VBATT - - - - - - - - IO "Read only" - 
      VCC H11 CGC_VCC - - - - - - - - IO "Read only" - 
      VCC H14 CGC_VCC - - - - - - - - IO "Read only" - 
      VCC G11 CGC_VCC - - - - - - - - IO "Read only" - 
      VCC G16 CGC_VCC - - - - - - - - IO "Read only" - 
      VCC F6 CGC_VCC - - - - - - - - IO "Read only" - 
      VCC G6 CGC_VCC - - - - - - - - IO "Read only" - 
      VCC F11 CGC_VCC - - - - - - - - IO "Read only" - 
      VCC H6 CGC_VCC - - - - - - - - IO "Read only" - 
      VCC L15 CGC_VCC - - - - - - - - IO "Read only" - 
      VCC K14 CGC_VCC - - - - - - - - IO "Read only" - 
      VCC18_MIPI R2 CGC_VCC18_MIPI - - - - - - - - IO "Read only" - 
      VCC2 R1 CGC_VCC2 - - - - - - - - IO "Read only" - 
      VCC2 J6 CGC_VCC2 - - - - - - - - IO "Read only" - 
      VCC2 L6 CGC_VCC2 - - - - - - - - IO "Read only" - 
      VCC2 M7 CGC_VCC2 - - - - - - - - IO "Read only" - 
      VCC2 M8 CGC_VCC2 - - - - - - - - IO "Read only" - 
      VCC_DCDC A10 CGC_VCC_DCDC - - - - - - - - IO "Read only" - 
      VCC_DCDC A11 CGC_VCC_DCDC - - - - - - - - IO "Read only" - 
      VCC_DCDC B10 CGC_VCC_DCDC - - - - - - - - IO "Read only" - 
      VCC_DCDC B11 CGC_VCC_DCDC - - - - - - - - IO "Read only" - 
      VCC_USB U17 CGC_VCC_USB - - - - - - - - IO "Read only" - 
      VCC_USBHS H15 CGC_VCC_USBHS - - - - - - - - IO "Read only" - 
      VCL F9 CGC_VCL - - - - - - - - IO "Read only" - 
      VCL G9 CGC_VCL - - - - - - - - IO "Read only" - 
      VCL H9 CGC_VCL - - - - - - - - IO "Read only" - 
      VCL M11 CGC_VCL - - - - - - - - IO "Read only" - 
      VCL J8 CGC_VCL - - - - - - - - IO "Read only" - 
      VCL J9 CGC_VCL - - - - - - - - IO "Read only" - 
      VCL K8 CGC_VCL - - - - - - - - IO "Read only" - 
      VCL K9 CGC_VCL - - - - - - - - IO "Read only" - 
      VCL L10 CGC_VCL - - - - - - - - IO "Read only" - 
      VCL L11 CGC_VCL - - - - - - - - IO "Read only" - 
      VCL K11 CGC_VCL - - - - - - - - IO "Read only" - 
      VCL J11 CGC_VCL - - - - - - - - IO "Read only" - 
      VLO A7 CGC_VLO - - - - - - - - IO "Read only" - 
      VLO A8 CGC_VLO - - - - - - - - IO "Read only" - 
      VLO B7 CGC_VLO - - - - - - - - IO "Read only" - 
      VLO B8 CGC_VLO - - - - - - - - IO "Read only" - 
      VREFH U9 CGC_VREFH - - - - - - - - IO "Read only" - 
      VREFH0 U10 CGC_VREFH0 - - - - - - - - IO "Read only" - 
      VREFL T9 CGC_VREFL - - - - - - - - IO "Read only" - 
      VREFL0 T10 CGC_VREFL0 - - - - - - - - IO "Read only" - 
      VSS A9 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS B9 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS H10 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS H12 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS U4 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS G10 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS G15 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS G17 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS F7 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS F8 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS G7 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS G8 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS F10 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS H7 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS H8 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS M10 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS J7 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS M17 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS K6 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS K7 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS L7 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS L8 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS L12 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS L9 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS K10 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS K12 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS J10 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS J12 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS J14 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS1_USBHS J17 CGC_VSS1_USBHS - - - - - - - - IO "Read only" - 
      VSS2_USBHS J16 CGC_VSS2_USBHS - - - - - - - - IO "Read only" - 
      VSS_MIPI R3 CGC_VSS_MIPI - - - - - - - - IO "Read only" - 
      VSS_USB T17 CGC_VSS_USB - - - - - - - - IO "Read only" - 
    R7KA8P1KFLCAC.pincfg -> 
      AVCC0 R9 CGC_AVCC0 - - - - - - - - IO "Read only" - 
      AVCC_MIPI T4 CGC_AVCC_MIPI - - - - - - - - IO "Read only" - 
      AVCC_USBHS K15 CGC_AVCC_USBHS - - - - - - - - IO "Read only" - 
      AVSS0 R10 CGC_AVSS0 - - - - - - - - IO "Read only" - 
      MIPI_CLN U2 CGC_MIPI_CLN - - - - - - - - IO "Read only" - 
      MIPI_CLP T2 CGC_MIPI_CLP - - - - - - - - IO "Read only" - 
      MIPI_DL0N U1 CGC_MIPI_DL0N - - - - - - - - IO "Read only" - 
      MIPI_DL0P T1 CGC_MIPI_DL0P - - - - - - - - IO "Read only" - 
      MIPI_DL1N U3 CGC_MIPI_DL1N - - - - - - - - IO "Read only" - 
      MIPI_DL1P T3 CGC_MIPI_DL1P - - - - - - - - IO "Read only" - 
      P000 U13 - S4_INT - - Disabled - - "ACMPHS: IVCMP2; ADC0: AN000; IRQ: IRQ6-DS" - None - - 
      P001 T13 - ARDUINO_A0 - - Disabled - - "ACMPHS: IVCMP3; ADC0: AN001; IRQ: IRQ7-DS" - None - - 
      P002 U14 - GROVE2_2_AN - - Disabled - - "ACMPHS: IVCMP2; ADC0: AN002; IRQ: IRQ8-DS" - None - - 
      P003 R12 - ARDUINO_A2 - - Disabled - - "ACMPHS: IVCMP3; ADC0: AN003; IRQ: IRQ29" - None - - 
      P004 T11 - ARDUINO_A3_MIKROBUS_AN - - Disabled - - "ACMPHS: IVCMP2; ADC0: AN004; IRQ: IRQ9-DS" - None - - 
      P005 R11 - GROVE2_1_AN - - Disabled - - "ACMPHS: IVCMP3; ADC0: AN005; IRQ: IRQ10-DS" - None - - 
      P006 U12 - PMOD1_7_INT - - Disabled - - "ACMPHS: IVCMP2; ADC1: AN006; IRQ: IRQ11-DS" - None - - 
      P007 T12 - ARDUINO_A1 - - Disabled - - "ACMPHS: IVCMP3; ADC1: AN007; IRQ: IRQ28" - None - - 
      P008 U11 - USER_S2 - - Disabled - - "ACMPHS: IVREF0; ADC1: AN008; IRQ: IRQ12-DS" - None - - 
      P009 P11 - USER_S1 - - Disabled - - "ACMPHS: IVREF1; ADC1: AN009; IRQ: IRQ13-DS" - None - - 
      P010 P10 - CAM_INT - - Disabled - - "ADC1: AN010; IRQ: IRQ14" - None - - 
      P011 N10 - ARDUINO_D2 - - Disabled - - "ADC1: AN011; IRQ: IRQ16" - None - - 
      P012 P9 - PMOD2_7_IRQ15 - - Disabled - - "ADC0: AN012; IRQ: IRQ15" - None - - 
      P013 N9 - I2C_SCL0_PULLUP - - Disabled - - "ADC1: AN013; IRQ: IRQ14" - None - - 
      P014 T8 - ARDUINO_A4 - - Disabled - - "ACMPHS: IVCMP0; ADC0: AN014; DAC120: DA0; IRQ: IRQ27" - None - - 
      P015 U8 - ARDUINO_A5 - - Disabled - - "ACMPHS: IVCMP0; ADC1: AN015; DAC121: DA1; IRQ: IRQ13" - None - - 
      P100 U6 - OSPI_DQ0_ARDUINO_D12_MISOB_MIKROBUS_MISOB - - Disabled - - "AGT0: AGTIO0; ESWM_GMII/MII: GPTP1_MATCH; ESWM_RGMII1: GPTP1_MATCH; ESWM_RMII1: GPTP1_MATCH; GPT8: GTIOC8B; GPT_POEGA: GTETRGA; IRQ: IRQ2; OSPI0: OM_0_SIO0; SCI9: DE9; SCI9: SCK9; SPI1: MISO1" - None - - 
      P101 R5 - OSPI_DQ3_ARDUINO_D11_MOSIB_MIKROBUS_MOSIB - - Disabled - - "AGT0: AGTEE0; ESWM_GMII/MII: GPTP1_CAPTURE; ESWM_RGMII1: GPTP1_CAPTURE; ESWM_RMII1: GPTP1_CAPTURE; GPT8: GTIOC8A; GPT_POEGB: GTETRGB; IRQ: IRQ1; OSPI0: OM_0_SIO3; SCI9: RXD9; SPI1: MOSI1" - None - - 
      P102 P5 - OSPI_DQ4_ARDUINO_D13_RSPCKB_MIKROBUS_RSPCKB - - Disabled - - "ADC0(Digital): ADTRG0; AGT0: AGTO0; CANFD0: CRX0; GPT2: GTIOC2B; GPT_OPS: GTOWLO; IRQ: IRQ17; OSPI0: OM_0_SIO4; SCI9: TXD9; SPI1: RSPCK1" - None - - 
      P103 R4 - OSPI_DQ2_ARDUINO_D10_SSLB_MIKROBUS_SSLB - - Disabled - - "ADC1(Digital): AD1FLAG1; CANFD0: CTX0; ESWM_GMII/MII: GPTP0_PPS; ESWM_RGMII0: GPTP0_PPS; ESWM_RMII0: GPTP0_PPS; GPT2: GTIOC2A; GPT_OPS: GTOWUP; IRQ: IRQ16; OSPI0: OM_0_SIO2; SCI9: CTS_RTS9; SCI9: DE9; SPI1: SSLB0" - None - - 
      P104 M6 - OSPI_CS_ARDUINO_D5 - - Disabled - - "ADC0(Digital): AD0FLAG1; ESWM_GMII/MII: GPTP0_MATCH; ESWM_RGMII0: GPTP0_MATCH; ESWM_RMII0: GPTP0_MATCH; GPT1: GTIOC1B; GPT_POEGB: GTETRGB; IRQ: IRQ1; OSPI0: OM_0_CS1; SCI9: CTS9; SPI1: SSLB1" - None - - 
      P105 N7 - OSPI_INT_ARDUINO_D6 - - Disabled - - "ADC(Digital): ADSYNC; ESWM_GMII/MII: GPTP0_CAPTURE; ESWM_RGMII0: GPTP0_CAPTURE; ESWM_RMII0: GPTP0_CAPTURE; GPT1: GTIOC1A; IRQ: IRQ0; OSPI0: OM_0_ECSINT1; SCI8: CTS_RTS8; SCI8: DE8; SPI1: SSLB2; ULPT1: ULPTO1-DS" - None - - 
      P106 N6 - OSPI_RES - - Disabled - - "ADC1(Digital): ADST1; AGT0: AGTOB0; ESWM_GMII/MII: ET1_LINKSTA; ESWM_RGMII1: ET1_LINKSTA; ESWM_RMII1: ET1_LINKSTA; GPT8: GTIOC8B; GPT_OPS: GTOWLO; IRQ: IRQ16; OSPI0: OM_0_RESET; SCI8: CTS8; SPI1: SSLB3; ULPT1: ULPTEE1-DS" - None - - 
      P107 N5 - ETH_MDINT - - Disabled - - "ADC0(Digital): ADST0; AGT0: AGTOA0; ESWM_GMII/MII: ET1_INT; ESWM_RGMII1: ET1_INT; ESWM_RMII1: ET1_INT; GPT8: GTIOC8A; GPT_OPS: GTOWUP; IRQ: IRQ31; OSPI0: OM_0_CS0; SCI4: CTS4" - None - - 
      P108 D8 - - - - Disabled - - "GPT10: GTIOC10B; IRQ: IRQ24; SDHI0: SD0DAT6" - None - - 
      P109 D7 - I2C_SDA0_PULLUP - - Disabled - - "GPT10: GTIOC10A; IRQ: IRQ23; SDHI0: SD0DAT5" - None - - 
      P110 C8 - ARDUINO_D9 - - Disabled - - "GPT9: GTIOC9B; IRQ: IRQ20; SDHI0: SD0DAT4" - None - - 
      P111 E8 - LCD_INT_MIPI_IRQ19 - - Disabled - - "GPT9: GTIOC9A; IRQ: IRQ19; SDHI0: SD0DAT3" - None - - 
      P112 A4 - SDRAM_DQ3 - - Disabled - - "ADC0(Digital): ADST0; BUS: D3; GLCDC: LCD_DATA10; GPT3: GTIOC3B; GPT_POEGA: GTETRGA; IRQ: IRQ27; SCI0: TXD0; SDHI0: SD0DAT4; SDRAM: DQ3; SPI0: SSLA2; SSIE0: SSIBCK0; ULPT0: ULPTOB0-DS" - None - - 
      P113 A2 - SDRAM_DQ4 - - Disabled - - "ADC1(Digital): ADST1; BUS: D4; GLCDC: LCD_DATA9; GPT2: GTIOC2A; GPT_POEGB: GTETRGB; IRQ: IRQ28; SCI0: RXD0; SDHI0: SD0DAT5; SDRAM: DQ4; SPI0: SSLA1; SSIE0: SSILRCK0; ULPT0: ULPTOA0-DS" - None - - 
      P114 B3 - SDRAM_DQ5 - - Disabled - - "ADC(Digital): ADSYNC; BUS: D5; GLCDC: LCD_DATA8; GPT2: GTIOC2B; GPT_POEGC: GTETRGC; IRQ: IRQ30-DS; SCI0: CTS_RTS0; SCI0: DE0; SDHI0: SD0DAT6; SDRAM: DQ5; SPI0: SSLA0; SSIE0: SSIRXD0" - None - - 
      P115 A3 - SDRAM_DQ6 - - Disabled - - "ADC0(Digital): AD0FLAG1; BUS: D6; GLCDC: LCD_DATA7; GPT5: GTIOC5A; GPT_POEGD: GTETRGD; IRQ: IRQ31-DS; SCI0: CTS0; SDHI0: SD0DAT7; SDRAM: DQ6; SPI0: MOSI0; SSIE0: SSITXD0" - None - - 
      P200 C5 - NMI - - Disabled - - "IRQ: NMI" - None - - 
      P201 E6 - MD_MIKROBUS_RES - - Disabled - - "CGC: MD; IRQ: IRQ4" - None - - 
      P206 B15 - ENET_RX_CTL - - Disabled - - "BUS: CS7; CEU: VIO_D0; CLKOUT: CLKOUT; ESWM_GMII/MII1: ET1_RX_DV; ESWM_RGMII1: RGMII1_RX_CTL; ESWM_RMII1: RMII1_CRS_DV; GPT0: GTCPPO0; GPT_OPS: GTIU; IRQ: IRQ0-DS; SDHI0: SD0DAT7; SSIE1: SSIDATA1; ULPT1: ULPTOB1; USB FS: USB_VBUSEN" - None - - 
      P207 A17 - LCD_D9 - - Disabled - - "ESWM_GMII/MII1: ET1_RXD5; GLCDC: LCD_DATA9; GPT3: GTCPPO3; IRQ: IRQ25" - None - - 
      P208 C7 - DEBUG_TDI - - Disabled - - "CANFD1: CRX1; CMPOUT: VCOUT; GPT1: GTIOC1B; GPT_OPS: GTOVLO; IRQ: IRQ3; JTAG/SWD: TDI; SCI9: RXD9" - None - - 
      P209 E7 - DEBUG_TDO_SWO - - Disabled - - "CANFD1: CTX1; CLKOUT: CLKOUT; GPT1: GTIOC1A; GPT_OPS: GTOVUP; IRQ: IRQ25; JTAG/SWD: TDO; SCI9: TXD9; TRACE: SWO" - None - - 
      P210 C6 - DEBUG_TMS_SWDIO L None Disabled - - "GPT0: GTIOC0B; GPT_OPS: GTOULO; IRQ: IRQ24; JTAG/SWD: SWDIO; JTAG/SWD: TMS; SCI9: CTS_RTS9; SCI9: DE9" - IO - - 
      P211 D6 - DEBUG_TCLK_SWCLK L None Disabled - - "GPT0: GTIOC0A; GPT_OPS: GTOUUP; IRQ: IRQ23; JTAG/SWD: SWCLK; JTAG/SWD: TCK; SCI9: DE9; SCI9: SCK9" - IO - - 
      P212 K17 - EXTAL - - Disabled - - "AGT1: AGTEE1; CGC: EXTAL; GPT0: GTIOC0B; GPT_POEGD: GTETRGD; IRQ: IRQ3; SCI1: RXD1" - None - - 
      P213 K16 - XTAL - - Disabled - - "ADC1(Digital): ADTRG1; CGC: XTAL; GPT0: GTIOC0A; GPT_POEGC: GTETRGC; IRQ: IRQ2; SCI1: TXD1; ULPT0: ULPTEE0" - None - - 
      P214 L16 - XCOUT - - Disabled - - "CGC: XCOUT; IRQ: IRQ21" - None - - 
      P215 L17 - XCIN - - Disabled - - "CGC: EXCIN; CGC: XCIN; IRQ: IRQ20" - None - - 
      P300 B5 - SDRAM_DQ2 - - Disabled - - "BUS: D2; GLCDC: LCD_DATA11; GPT3: GTIOC3A; IRQ: IRQ4; SCI0: DE0; SCI0: SCK0; SDHI0: SD0DAT3; SDRAM: DQ2; SPI0: SSLA3; ULPT0: ULPTEVI0-DS" - None - - 
      P301 C4 - SDRAM_DQ1 - - Disabled - - "AGT0: AGTIO0; BUS: D1; GLCDC: LCD_DATA12; GPT4: GTIOC4B; GPT_OPS: GTOULO; IRQ: IRQ6; SCI6: TXD6; SDHI0: SD0DAT2; SDRAM: DQ1; ULPT0: ULPTEE0-DS" - None - - 
      P302 A5 - SDRAM_DQ0 - - Disabled - - "BUS: D0; GLCDC: LCD_DATA13; GPT4: GTIOC4A; GPT_OPS: GTOUUP; IRQ: IRQ5; SCI6: RXD6; SDHI0: SD0DAT1; SDRAM: DQ0; ULPT0: ULPTO0-DS" - None - - 
      P303 B6 - USER_LED2_GREEN - - Disabled - - "GLCDC: LCD_DATA14; GPT7: GTIOC7B; IRQ: IRQ29-DS; SCI6: DE6; SCI6: SCK6" - None - - 
      P304 D10 - ETH_TXD3_TRACE_TDATA3 - - Disabled - - "CEU: VIO_D15; ESWM_GMII/MII1: ET1_TXD3; ESWM_RGMII1: RGMII1_TXD3; GPT7: GTIOC7A; GPT_OPS: GTOVLO; IRQ: IRQ9; SDHI0: SD0DAT0; TRACE: TDATA3; ULPT1: ULPTO1" - None - - 
      P305 C10 - ETH_TXD2_TRACE_TDATA2 - - Disabled - - "CEU: VIO_D14; ESWM_GMII/MII1: ET1_TXD2; ESWM_RGMII1: RGMII1_TXD2; GPT12: GTCPPO12; GPT_OPS: GTOVUP; IRQ: IRQ8; SDHI0: SD0WP; TRACE: TDATA2; ULPT1: ULPTEE1" - None - - 
      P306 D11 - ETH_TXD1_TRACE_TDATA1 - - Disabled - - "CEU: VIO_D13; ESWM_GMII/MII1: ET1_TXD1; ESWM_RGMII1: RGMII1_TXD1; ESWM_RMII1: RMII1_TXD1; GPT11: GTCPPO11; GPT_OPS: GTIW; IRQ: IRQ28-DS; SDHI0: SD0CD; TRACE: TDATA1; ULPT1: ULPTEVI1" - None - - 
      P307 C11 - ETH_TXD0_TRACE_TDATA0 - - Disabled - - "CEU: VIO_D12; ESWM_GMII/MII1: ET1_TXD0; ESWM_RGMII1: RGMII1_TXD0; ESWM_RMII1: RMII1_TXD0; GPT10: GTCPPO10; GPT_OPS: GTIV; IRQ: IRQ27-DS; SCI6: CTS_RTS6; SCI6: DE6; SDHI0: SD0CMD; TRACE: TDATA0; ULPT1: ULPTOA1" - None - - 
      P308 C9 - TRACE_TCLK - - Disabled - - "CEU: VIO_D11; ESWM_GMII/MII1: ET1_TX_ER; ETHPHYCLK: ETHPHYCLK; GPT9: GTCPPO9; GPT_OPS: GTIU; IRQ: IRQ26-DS; SCI3: CTS3; SDHI0: SD0CLK; TRACE: TCLK; ULPT1: ULPTOB1" - None - - 
      P309 A12 - ETH_TX_CLK - - Disabled - - "CEU: VIO_D10; CMPOUT: VCOUT; ESWM_GMII/MII1: ET1_GTX_CLK; ESWM_RGMII1: RGMII1_TXC; GLCDC: LCD_DATA15; GPT8: GTCPPO8; IRQ: IRQ25-DS; SCI9: CTS9" - None - - 
      P310 E10 - ETH_TX_CTL - - Disabled - - "AGT1: AGTEE1; CEU: VIO_D9; ESWM_GMII/MII1: ET1_TX_EN; ESWM_RGMII1: RGMII1_TX_CTL; ESWM_RMII1: RMII1_TX_EN; GLCDC: LCD_DATA16; GPT7: GTCPPO7; IRQ: IRQ24-DS; SCI3: TXD3" - None - - 
      P311 B12 - CAM_D8 - - Disabled - - "AGT1: AGTOB1; CANFD0: CRX0; CEU: VIO_D8; ESWM_GMII/MII1: ET1_TX_CLK; GLCDC: LCD_DATA17; GPT: GTADSM1; GPT6: GTCPPO6; IRQ: IRQ23-DS; SCI3: DE3; SCI3: SCK3" - None - - 
      P312 C13 - ARDUINO_D7 - - Disabled - - "AGT1: AGTOA1; CANFD0: CTX0; CEU: VIO_D7; ESWM_GMII/MII1: ET1_RX_ER; ESWM_RMII1: RMII1_RX_ER; GLCDC: LCD_DATA18; GPT: GTADSM0; GPT5: GTCPPO5; IRQ: IRQ22-DS; PDM2: PDMDAT2; SCI3: CTS_RTS3; SCI3: DE3" - None - - 
      P400 P17 - CAM_D0_ARDUINO_GROVE1_SCL0 - - Disabled - - "ADC1(Digital): ADTRG1; AGT1: AGTIO1; CEU: VIO_D0; GPT6: GTIOC6A; I3C0: I3C_SCL0; IRQ: IRQ0; SCI1: TXD1; SDHI1: SD1CLK; SSIE: AUDIO_CLK" - None - - 
      P401 N17 - ARDUINO_GROVE1_SDA0 - - Disabled - - "CANFD0: CTX0; CEU: VIO_D1; GPT6: GTIOC6B; GPT_POEGA: GTETRGA; I3C0: I3C_SDA0; IRQ: IRQ5-DS; SCI1: RXD1; SDHI1: SD1CMD" - None - - 
      P402 L14 - PMOD1_8_GPIO_RST - - Disabled - - "CAC: CACREF; CANFD0: CRX0; ESWM_GMII/MII: ET0_LINKSTA; ESWM_RGMII0: ET0_LINKSTA; ESWM_RMII0: ET0_LINKSTA; IRQ: IRQ4-DS; RTC: RTCIC0; SCI1: DE1; SCI1: SCK1; SDHI1: SD1DAT0; SSIE: AUDIO_CLK" - None - - 
      P403 H13 - AUDIO_BCLK - - Disabled - - "ADC0(Digital): AD0FLAG1; ESWM_GMII/MII: ET1_WOL; ESWM_RGMII1: ET1_WOL; ESWM_RMII1: ET1_WOL; GPT3: GTIOC3A; IRQ: IRQ14-DS; RTC: RTCIC1; SCI1: CTS_RTS1; SCI1: DE1; SDHI1: SD1DAT1; SSIE0: SSIBCK0" - None - - 
      P404 J13 - AUDIO_WCLK - - Disabled - - "ADC1(Digital): AD1FLAG1; ESWM_GMII/MII: ET0_WOL; ESWM_RGMII0: ET0_WOL; ESWM_RMII0: ET0_WOL; GPT3: GTIOC3B; IRQ: IRQ15-DS; RTC: RTCIC2; SCI1: CTS1; SDHI1: SD1DAT2; SSIE0: SSILRCK0" - None - - 
      P405 G12 - CAM_D2_AUDIO_DATIN - - Disabled - - "AGT1: AGTIO1; CEU: VIO_D2; ESWM_GMII/MII0: ET0_RX_DV; ESWM_RGMII0: RGMII0_RX_CTL; ESWM_RMII0: RMII0_CRS_DV; GPT1: GTIOC1A; IRQ: IRQ30; SCI2: DE2; SCI2: SCK2; SDHI1: SD1DAT3; SSIE0: SSITXD0" - None - - 
      P406 F14 - CAM_D3_AUDIO_DOUT - - Disabled - - "CEU: VIO_D3; ESWM_GMII/MII0: ET0_RXD3; ESWM_RGMII0: RGMII0_RXD3; GPT1: GTIOC1B; IRQ: IRQ31; SCI2: TXD2; SDHI1: SD1CD; SPI0: SSLA3; SSIE0: SSIRXD0" - None - - 
      P407 R17 - USBFS_VBUS - - Disabled - - "ADC0(Digital): ADTRG0; AGT0: AGTIO0; BUS: CS6; ESWM_GMII/MII: GPTP_PTPOUT3; ESWM_RGMII: GPTP_PTPOUT3; ESWM_RMII: GPTP_PTPOUT3; GPT10: GTIOC10B; IIC0: SDA0; IRQ: IRQ22; RTC: RTCOUT; SCI1: DE1; SCI1: SCK1; USB FS: USB_VBUS; USB HS: USBHS_VBUSEN" - None - - 
      P408 M15 - USBHS_VBUS - - Disabled - - "ADC(Digital): ADSYNC; BUS: A17; ESWM_GMII/MII: GPTP_PTPOUT2; ESWM_RGMII: GPTP_PTPOUT2; ESWM_RMII: GPTP_PTPOUT2; GPT10: GTIOC10A; GPT_OPS: GTOWLO; IIC0: SCL0; IRQ: IRQ7; SCI3: RXD3; ULPT0: ULPTOB0; USB FS: USB_VBUSEN; USB HS: USBHS_VBUS" - None - - 
      P409 R16 - PMOD2_9_GPIO - - Disabled - - "ADC1(Digital): ADST1; BUS: A18; ESWM_GMII/MII: GPTP0_CAPTURE; ESWM_RGMII0: GPTP0_CAPTURE; ESWM_RMII0: GPTP0_CAPTURE; GPT_OPS: GTOWUP; IIC0: SDA0; IRQ: IRQ6; SCI3: TXD3; ULPT0: ULPTOA0; USB FS: USB_OVRCURA-DS; USB HS: USBHS_OVRCURA" - None - - 
      P410 K13 - PMOD2_8_GPIO_RST - - Disabled - - "ADC0(Digital): ADST0; AGT1: AGTOB1; BUS: A19; ESWM_GMII/MII: GPTP0_MATCH; ESWM_RGMII0: GPTP0_MATCH; ESWM_RMII0: GPTP0_MATCH; GPT9: GTIOC9B; GPT_OPS: GTOVLO; IIC0: SCL0; IRQ: IRQ5; SCI3: DE3; SCI3: SCK3; USB FS: USB_OVRCURB-DS; USB HS: USBHS_OVRCURB" - None - - 
      P411 M14 - DSI_TE - - Disabled - - "AGT1: AGTOA1; BUS: A20; CAC: CACREF; ESWM_GMII/MII: GPTP_PTPOUT1; ESWM_RGMII: GPTP_PTPOUT1; ESWM_RMII: GPTP_PTPOUT1; GPT9: GTIOC9A; GPT_OPS: GTOVUP; IRQ: IRQ4; MIPI: DSI_TE; SCI3: CTS_RTS3; SCI3: DE3; USB FS: USB_ID; USB HS: USBHS_ID" - None - - 
      P412 M12 - PMOD1_9_GPIO - - Disabled - - "AGT1: AGTEE1; BUS: A21; ESWM_GMII/MII: GPTP_PTPOUT0; ESWM_RGMII: GPTP_PTPOUT0; ESWM_RMII: GPTP_PTPOUT0; GPT8: GTCPPO8; GPT_OPS: GTOULO; IRQ: IRQ20-DS; SCI3: CTS3; USB FS: USB_EXICEN; USB HS: USBHS_EXICEN" - None - - 
      P413 P14 - PMOD1_10_GPIO - - Disabled - - "BUS: A22; ESWM_GMII/MII: ET_TAS_STA3; ESWM_RGMII: ET_TAS_STA3; ESWM_RMII: ET_TAS_STA3; GPT7: GTCPPO7; GPT_OPS: GTOUUP; IRQ: IRQ18; ULPT1: ULPTEE1" - None - - 
      P414 L13 - ETH_MDIO - - Disabled - - "BUS: A23; CANFD1: CRX1; CEU: VIO_CLK; ESWM_GMII/MII: ET1_MDIO; ESWM_RGMII1: ET1_MDIO; ESWM_RMII1: ET1_MDIO; GPT0: GTIOC0B; IRQ: IRQ9; SCI4: RXD4; SPI1: SSLB0" - None - - 
      P415 R15 - ETH_MDC - - Disabled - - "BUS: WAIT; CANFD1: CTX1; CEU: VIO_HD; ESWM_GMII/MII: ET1_MDC; ESWM_RGMII1: ET1_MDC; ESWM_RMII1: ET1_MDC; GPT0: GTIOC0A; IRQ: IRQ8; SCI4: TXD4; SPI1: RSPCK1" - None - - 
      P500 U7 - USBFS_VBUSEN - - Disabled - - "ADC0: AN021; ADC1: AN021; CAC: CACREF; GPT11: GTIOC11B; IRQ: IRQ24; PDM0: PDMDAT0; SCI8: RXD8; SDHI1: SD1DAT5; USB FS: USB_VBUSEN" - None - - 
      P501 R8 - CAM_XCLK - - Disabled - - "ADC0: AN020; ADC1: AN020; GPT12: GTIOC12A; IRQ: IRQ25; PDM1: PDMDAT1; SCI8: TXD8; SDHI1: SD1DAT6; USB FS: USB_OVRCURA" - None - - 
      P502 T7 - MEMS_MIC_DATA L None Disabled - - "ADC0: AN019; ADC1: AN019; GPT12: GTIOC12B; IRQ: IRQ26; PDM2: PDMDAT2; SCI8: DE8; SCI8: SCK8; SDHI1: SD1DAT7; USB FS: USB_OVRCURB" - I - - 
      P503 H2 - SDRAM_A4 - - Disabled - - "BUS: A6; CEU: VIO_D4; GPT6: GTCPPO6; GPT_OPS: GTOUUP; IRQ: IRQ6; SDHI0: SD0CD; SDRAM: A6" - None - - 
      P504 H1 - SDRAM_A5 - - Disabled - - "BUS: A7; CEU: VIO_D3; GPT1: GTCPPO1; GPT_OPS: GTOULO; IRQ: IRQ7; SDHI0: SD0WP; SDRAM: A7" - None - - 
      P505 H3 - SDRAM_A6 - - Disabled - - "BUS: A8; CEU: VIO_D2; GPT2: GTCPPO2; GPT_OPS: GTOWUP; IRQ: IRQ8; SDHI0: SD0CLK; SDRAM: A8" - None - - 
      P506 J1 - SDRAM_A7 - - Disabled - - "BUS: A9; CEU: VIO_D1; GPT3: GTCPPO3; GPT_OPS: GTOWLO; IRQ: IRQ9; SDHI0: SD0CMD; SDRAM: A9" - None - - 
      P507 J2 - SDRAM_A8 - - Disabled - - "BUS: A10; CEU: VIO_D0; ESWM_GMII/MII: ET_TAS_STA0; ESWM_RGMII: ET_TAS_STA0; ESWM_RMII: ET_TAS_STA0; GLCDC: LCD_EXTCLK; GPT: GTADSM0; GPT0: GTIOC0A; IRQ: IRQ10; SCI7: CTS_RTS7; SCI7: DE7; SDRAM: A10" - None - - 
      P508 J3 - SDRAM_A9 - - Disabled - - "BUS: A11; CEU: VIO_VD; ESWM_GMII/MII: ET_TAS_STA1; ESWM_RGMII: ET_TAS_STA1; ESWM_RMII: ET_TAS_STA1; GPT: GTADSM1; GPT0: GTIOC0B; IRQ: IRQ1; SCI5: CTS5; SDRAM: A11" - None - - 
      P509 J4 - SDRAM_A10 - - Disabled - - "BUS: A12; CEU: VIO_HD; ESWM_GMII/MII: ET_TAS_STA2; ESWM_RGMII: ET_TAS_STA2; ESWM_RMII: ET_TAS_STA2; GPT1: GTIOC1A; IRQ: IRQ2; SCI5: CTS_RTS5; SCI5: DE5; SDRAM: A12; ULPT1: ULPTEVI1" - None - - 
      P510 K3 - SDRAM_A11 - - Disabled - - "BUS: A13; CEU: VIO_CLK; ESWM_GMII/MII: ET_TAS_STA3; ESWM_RGMII: ET_TAS_STA3; ESWM_RMII: ET_TAS_STA3; GPT1: GTIOC1B; IRQ: IRQ3; SCI5: RXD5; SDRAM: A13; ULPT0: ULPTEVI0" - None - - 
      P511 U15 - IIC_SYSTEM_SDA1 - - Disabled - - "CANFD1: CRX1; ESWM_GMII/MII: ET1_LINKSTA; ESWM_RGMII1: ET1_LINKSTA; ESWM_RMII1: ET1_LINKSTA; GPT0: GTIOC0B; IIC1: SDA1; IRQ: IRQ15; SCI8: CTS_RTS8; SCI8: DE8" - None - - 
      P512 P13 - IIC_SYSTEM_SCL1 - - Disabled - - "CANFD1: CTX1; ESWM_GMII/MII: ET1_INT; ESWM_RGMII1: ET1_INT; ESWM_RMII1: ET1_INT; GPT0: GTIOC0A; IIC1: SCL1; IRQ: IRQ14; SCI8: CTS8" - None - - 
      P513 R13 - LCD_TCON3 - - Disabled - - "ACMPHS: IVCMP0; ADC0: AN016; ADC1: AN016; CEU: VIO_FLD; ESWM_GMII/MII: ET0_INT; ESWM_RGMII0: ET0_INT; ESWM_RMII0: ET0_INT; GLCDC: LCD_TCON3; GPT13: GTIOC13B; IRQ: IRQ31; SCI8: DE8; SCI8: SCK8" - None - - 
      P514 R14 - ETH_RST - - Disabled - - "ESWM_GMII/MII: ET_TAS_STA1; ESWM_RGMII: ET_TAS_STA1; ESWM_RMII: ET_TAS_STA1; GLCDC: LCD_EXTCLK; GPT13: GTIOC13B; IIC2: SDA2; IRQ: IRQ13; SCI4: DE4; SCI4: SCK4" - None - - 
      P515 P15 - LCD_CLK - - Disabled - - "ESWM_GMII/MII: ET_TAS_STA0; ESWM_RGMII: ET_TAS_STA0; ESWM_RMII: ET_TAS_STA0; GLCDC: LCD_CLK; GPT13: GTIOC13A; IIC2: SCL2; IRQ: IRQ12; SCI4: CTS_RTS4; SCI4: DE4" - None - - 
      P600 P3 - USER_LED1_BLUE - - Disabled - - "CAC: CACREF; ESWM_GMII/MII: ET1_WOL; ESWM_RGMII1: ET1_WOL; ESWM_RMII1: ET1_WOL; GPT6: GTIOC6B; IRQ: IRQ30; OSPI0: OM_0_RSTO1; ULPT1: ULPTEVI1-DS" - None - - 
      P601 P4 - PMOD2_4_RSPCKB - - Disabled - - "GPT6: GTIOC6A; IRQ: IRQ29; OSPI0: OM_0_WP1; RTC: RTCOUT; SCI0: DE0; SCI0: SCK0; ULPT0: ULPTEVI0" - None - - 
      P602 P2 - PMOD2_3_MISOB_RXD0 - - Disabled - - "GPT7: GTIOC7B; IRQ: IRQ28; OSPI1: OM_1_SCLKN; SCI0: RXD0; ULPT0: ULPTEE0" - None - - 
      P603 P1 - PMOD2_2_MOSIB_TXD0 - - Disabled - - "GPT7: GTIOC7A; IRQ: IRQ27; OSPI1: OM_1_SCLK; SCI0: TXD0; ULPT0: ULPTO0" - None - - 
      P604 N2 - PMOD2_1_SSLB0_CTS_RTS0 - - Disabled - - "GPT8: GTIOC8B; IRQ: IRQ26; OSPI1: OM_1_SIO7; SCI0: CTS_RTS0; SCI0: DE0" - None - - 
      P605 N1 - PMOD2_1_CTS0 - - Disabled - - "GPT8: GTIOC8A; IRQ: IRQ25; OSPI1: OM_1_SIO1; SCI0: CTS0" - None - - 
      P606 N3 - LCD_RST - - Disabled - - "BUS: BC3; BUS: WR3; IRQ: IRQ24; OSPI1: OM_1_SIO6" - None - - 
      P607 M2 - SDRAM_DQ31 - - Disabled - - "BUS: D31; IRQ: IRQ23; OSPI1: OM_1_DQS; SDRAM: DQ31" - None - - 
      P608 K2 - SDRAM_A12 - - Disabled - - "BUS: A14; CAC: CACREF; CEU: VIO_FLD; GPT4: GTCPPO4; GPT_OPS: GTOWUP; IRQ: IRQ22; SCI5: TXD5; SDRAM: A14" - None - - 
      P609 A1 - SDRAM_DQ7 - - Disabled - - "ADC1(Digital): AD1FLAG1; BUS: D7; CANFD1: CTX1; GLCDC: LCD_DATA6; GPT5: GTIOC5B; GPT_OPS: GTIU; IRQ: IRQ29; SCI0: TXD0; SDRAM: DQ7; SPI0: MISO0; ULPT1: ULPTOA1-DS" - None - - 
      P610 D3 - SDRAM_DQ12 - - Disabled - - "BUS: D12; CANFD1: CRX1; GLCDC: LCD_DATA5; GPT4: GTIOC4A; GPT_OPS: GTOUUP; IRQ: IRQ16; SCI0: RXD0; SDRAM: DQ12; SPI0: RSPCK0; ULPT1: ULPTOB1-DS" - None - - 
      P611 D2 - SDRAM_DQ13 - - Disabled - - "BUS: D13; CAC: CACREF; CLKOUT: CLKOUT; GLCDC: LCD_DATA4; GPT4: GTIOC4B; GPT_OPS: GTOULO; IRQ: IRQ17; SCI0: DE0; SCI0: SCK0; SDRAM: DQ13; SPI0: MOSI0; USB HS: USBHS_VBUSEN" - None - - 
      P612 E4 - SDRAM_DQ14 - - Disabled - - "BUS: D14; GLCDC: LCD_DATA3; GPT9: GTIOC9A; IRQ: IRQ18; SCI0: CTS_RTS0; SCI0: DE0; SDRAM: DQ14; SPI0: SSLA0; USB HS: USBHS_OVRCURA" - None - - 
      P613 C2 - SDRAM_DQ15 - - Disabled - - "AGT1: AGTO1; BUS: D15; GLCDC: LCD_DATA2; GPT9: GTIOC9B; GPT_POEGA: GTETRGA; IRQ: IRQ19; SCI0: CTS0; SDRAM: DQ15; USB HS: USBHS_OVRCURB" - None - - 
      P614 E3 - SDRAM_DQM0 - - Disabled - - "AGT0: AGTO0; BUS: WR; BUS: WR0; GLCDC: LCD_DATA1; GPT9: GTCPPO9; GPT_POEGB: GTETRGB; IRQ: IRQ20; SCI7: RXD7; SDRAM: DQM0; USB HS: USBHS_ID" - None - - 
      P615 E2 - SDRAM_DQM2 - - Disabled - - "BUS: BC2; BUS: WR2; GLCDC: LCD_DATA0; GPT10: GTCPPO10; GPT_POEGC: GTETRGC; IRQ: IRQ7; SCI7: TXD7; SDRAM: DQM2; USB HS: USBHS_EXICEN" - None - - 
      P700 F12 - CAM_D4 - - Disabled - - "CEU: VIO_D4; ESWM_GMII/MII0: ET0_RXD2; ESWM_RGMII0: RGMII0_RXD2; GPT5: GTIOC5A; IRQ: IRQ16-DS; SCI2: RXD2; SDHI1: SD1WP; SPI0: MISO0; SSIE1: SSIDATA1" - None - - 
      P701 F15 - CAM_D5 - - Disabled - - "CEU: VIO_D5; ESWM_GMII/MII0: ET0_RXD1; ESWM_RGMII0: RGMII0_RXD1; ESWM_RMII0: RMII0_RXD1; GPT5: GTIOC5B; IRQ: IRQ17-DS; SCI2: CTS_RTS2; SCI2: DE2; SDHI1: SD1DAT4; SPI0: MOSI0; SSIE1: SSILRCK1; ULPT1: ULPTO1" - None - - 
      P702 F13 - CAM_D6 - - Disabled - - "CEU: VIO_D6; ESWM_GMII/MII0: ET0_RXD0; ESWM_RGMII0: RGMII0_RXD0; ESWM_RMII0: RMII0_RXD0; GPT6: GTIOC6A; IRQ: IRQ18-DS; SCI2: CTS2; SDHI1: SD1DAT5; SPI0: RSPCK0; SSIE1: SSIBCK1; ULPT0: ULPTO0" - None - - 
      P703 G14 - CAM_D7 - - Disabled - - "AGT1: AGTO1; CEU: VIO_D7; CMPOUT: VCOUT; ESWM_GMII/MII0: ET0_RX_CLK; ESWM_RGMII0: RGMII0_RXC; ESWM_RMII0: RMII0_REF50CK; GPT6: GTIOC6B; IRQ: IRQ19-DS; PDM0: PDMCLK0; SDHI1: SD1DAT6; SPI0: SSLA0" - None - - 
      P704 G13 - PMOD2_10_GPIO - - Disabled - - "AGT0: AGTO0; CANFD0: CTX0; CEU: VIO_D8; ESWM_GMII/MII0: ET0_RX_ER; ESWM_RMII0: RMII0_RX_ER; GPT: GTADSM0; GPT0: GTCPPO0; IRQ: IRQ26; PDM1: PDMCLK1; SDHI1: SD1DAT7; SPI0: SSLA1" - None - - 
      P705 F17 - CAM_D9 - - Disabled - - "AGT0: AGTIO0; CANFD0: CRX0; CEU: VIO_D9; ESWM_GMII/MII0: ET0_TX_EN; ESWM_RGMII0: RGMII0_TX_CTL; ESWM_RMII0: RMII0_TX_EN; GPT: GTADSM1; GPT1: GTCPPO1; IRQ: IRQ19; PDM2: PDMCLK2; SCI1: CTS1; SPI0: SSLA2" - None - - 
      P706 E17 - CAM_D10 - - Disabled - - "AGT0: AGTIO0; CEU: VIO_D10; ESWM_GMII/MII0: ET0_GTX_CLK; ESWM_RGMII0: RGMII0_TXC; ETHPHYCLK: ETHPHYCLK; GPT2: GTCPPO2; IRQ: IRQ7; PDM0: PDMDAT0; SCI1: RXD1; USB HS: USBHS_OVRCURB-DS" - None - - 
      P707 F16 - LCD_D18_CAM_D11 - - Disabled - - "CEU: VIO_D11; ESWM_GMII/MII0: ET0_TX_ER; ETHPHYCLK: ETHPHYCLK; GLCDC: LCD_DATA18; GPT3: GTCPPO3; IRQ: IRQ8; PDM1: PDMDAT1; SCI1: TXD1; USB HS: USBHS_OVRCURA-DS" - None - - 
      P708 N12 - LCD_BLEN - - Disabled - - "BUS: BC1; BUS: WR1; CAC: CACREF; CEU: VIO_VD; ESWM_GMII/MII: ET0_MDC; ESWM_RGMII0: ET0_MDC; ESWM_RMII0: ET0_MDC; GPT6: GTCPPO6; IIC2: SDA2; IRQ: IRQ11; SCI4: DE4; SCI4: SCK4; SPI1: MOSI1; SSIE: AUDIO_CLK" - None - - 
      P709 P16 - CAM_RST - - Disabled - - "BUS: CS4; CEU: VIO_D13; ESWM_GMII/MII: ET0_MDIO; ESWM_RGMII0: ET0_MDIO; ESWM_RMII0: ET0_MDIO; GPT5: GTCPPO5; IIC2: SCL2; IRQ: IRQ10; SCI4: CTS_RTS4; SCI4: DE4; SPI1: MISO1" - None - - 
      P710 M13 - LCD_EXTCLK - - Disabled - - "BUS: CS5; CEU: VIO_D12; ESWM_GMII/MII: ET0_LINKSTA; ESWM_RGMII0: ET0_LINKSTA; ESWM_RMII0: ET0_LINKSTA; GLCDC: LCD_EXTCLK; GPT11: GTIOC11B; IRQ: IRQ17; SCI4: CTS4; SPI1: SSLB3" - None - - 
      P711 N15 - LCD_D19 - - Disabled - - "AGT0: AGTEE0; ESWM_GMII/MII: GPTP0_PPS; ESWM_RGMII0: GPTP0_PPS; ESWM_RMII0: GPTP0_PPS; GLCDC: LCD_DATA19; GPT11: GTIOC11A; IRQ: IRQ3; SCI1: CTS_RTS1; SCI1: DE1; SPI1: SSLB2" - None - - 
      P712 N13 - LCD_D20 - - Disabled - - "AGT0: AGTOB0; ESWM_GMII/MII: GPTP1_CAPTURE; ESWM_RGMII1: GPTP1_CAPTURE; ESWM_RMII1: GPTP1_CAPTURE; GLCDC: LCD_DATA20; GPT2: GTIOC2B; IRQ: IRQ2; SCI1: CTS1; SPI1: SSLB1" - None - - 
      P713 N16 - LCD_D21 - - Disabled - - "AGT0: AGTOA0; ESWM_GMII/MII: GPTP1_MATCH; ESWM_RGMII1: GPTP1_MATCH; ESWM_RMII1: GPTP1_MATCH; GLCDC: LCD_DATA21; GPT2: GTIOC2A; IRQ: IRQ14; SCI4: CTS4" - None - - 
      P714 N14 - LCD_D22 - - Disabled - - "ESWM_GMII/MII: GPTP1_PPS; ESWM_RGMII1: GPTP1_PPS; ESWM_RMII1: GPTP1_PPS; GLCDC: LCD_DATA22; GPT12: GTIOC12B; IRQ: IRQ13; MIPI: DSI_TE; SCI4: TXD4" - None - - 
      P715 T15 - LCD_D23 - - Disabled - - "ESWM_GMII/MII: ET_TAS_STA2; ESWM_RGMII: ET_TAS_STA2; ESWM_RMII: ET_TAS_STA2; GLCDC: LCD_DATA23; GPT12: GTIOC12A; IRQ: IRQ12; SCI4: RXD4" - None - - 
      P800 T6 - OSPI_DQ5_PMOD1_1_CTS2 - - Disabled - - "AGT0: AGTOA0; GPT11: GTIOC11A; GPT_OPS: GTIU; IRQ: IRQ11; OSPI0: OM_0_SIO5; SCI2: CTS2" - None - - 
      P801 P6 - OSPI_DS L None Disabled - - "AGT0: AGTOB0; ESWM_GMII/MII: GPTP1_PPS; ESWM_RGMII1: GPTP1_PPS; ESWM_RMII1: GPTP1_PPS; GPT11: GTIOC11B; GPT_OPS: GTIV; IRQ: IRQ12; OSPI0: OM_0_DQS; SCI2: TXD2" - O - - 
      P802 R6 - OSPI_DQ6 - - Disabled - - "GPT12: GTIOC12A; GPT_OPS: GTIW; IRQ: IRQ18; OSPI0: OM_0_SIO6; SCI2: RXD2" - None - - 
      P803 P7 - OSPI_DQ1 - - Disabled - - "GPT12: GTIOC12B; GPT_POEGC: GTETRGC; IRQ: IRQ19; OSPI0: OM_0_SIO1; SCI2: DE2; SCI2: SCK2" - None - - 
      P804 R7 - OSPI_DQ7 - - Disabled - - "GPT13: GTIOC13A; GPT_POEGD: GTETRGD; IRQ: IRQ14; MIPI: DSI_TE; OSPI0: OM_0_SIO7; SCI2: CTS_RTS2; SCI2: DE2" - None - - 
      P805 P12 - LCD_HSYNC_TCON1 - - Disabled - - "ACMPHS: IVCMP0; ADC0: AN017; ADC1: AN017; CEU: VIO_D15; ESWM_GMII/MII: ET1_MDIO; ESWM_RGMII1: ET1_MDIO; ESWM_RMII1: ET1_MDIO; GLCDC: LCD_TCON1; IRQ: IRQ30; SCI8: TXD8" - None - - 
      P806 T14 - LCD_VSYNC_TCON0 - - Disabled - - "ADC0: AN018; ADC1: AN018; CEU: VIO_D14; ESWM_GMII/MII: ET1_MDC; ESWM_RGMII1: ET1_MDC; ESWM_RMII1: ET1_MDC; GLCDC: LCD_TCON0; IRQ: IRQ0; SCI8: RXD8" - None - - 
      P807 N11 - LCD_DE_TCON2 - - Disabled - - "GLCDC: LCD_TCON2; GPT13: GTIOC13A; IRQ: IRQ11" - None - - 
      P808 U5 - OSPI_SCLK_ARDUINO_D0_RXD_MIKROBUS_RXD - - Disabled - - "GPT13: GTIOC13B; IRQ: IRQ15; OSPI0: OM_0_SCLK; SCI7: RXD7" - None - - 
      P809 T5 - ARDUINO_D1_TXD_MIKROBUS_TXD - - Disabled - - "IRQ: IRQ20; OSPI0: OM_0_SCLKN; SCI7: TXD7" - None - - 
      P810 M9 - ARDUINO_D4_MIKROBUS_1_PWM - - Disabled - - "GPT10: GTIOC10A; IRQ: IRQ21; PDM0: PDMCLK0; SCI7: DE7; SCI7: SCK7; SDHI1: SD1DAT2; ULPT0: ULPTOA0" - None - - 
      P811 N8 - ARDUINO_D3 - - Disabled - - "GPT10: GTIOC10B; IRQ: IRQ22; PDM1: PDMCLK1; SCI7: CTS7; SDHI1: SD1DAT3; ULPT0: ULPTOB0; USB FS: USB_ID" - None - - 
      P812 P8 - MEMS_MIC_CLK L None Disabled - - "ADC0: AN022; ADC1: AN022; GPT11: GTIOC11A; IRQ: IRQ23; PDM2: PDMCLK2; SCI7: CTS_RTS7; SCI7: DE7; SDHI1: SD1DAT4; USB FS: USB_EXICEN" - O - - 
      P813 B1 - SDRAM_CS - - Disabled - - "CEU: VIO_D13; GPT7: GTIOC7B; GPT_POEGA: GTETRGA; IRQ: IRQ15; PDM2: PDMCLK2; SCI7: DE7; SCI7: SCK7; SDRAM: SDCS" - None - - 
      P814 U16 - USBFS_DP - - Disabled - - "CANFD0: CRX0; GPT8: GTIOC8B; IRQ: IRQ16; USB FS: USB_DP" - None - - 
      P815 T16 - USBFS_DN - - Disabled - - "CANFD0: CTX0; GPT8: GTIOC8A; IRQ: IRQ15; USB FS: USB_DM" - None - - 
      P902 E9 - CAM_D1_LCD_D3 - - Disabled - - "BUS: ALE; CEU: VIO_D1; ETHPHYCLK: ETHPHYCLK; GLCDC: LCD_DATA3; GPT13: GTCPPO13; IRQ: IRQ0; SSIE: AUDIO_CLK" - None - - 
      P903 D9 - LCD_D2 - - Disabled - - "GLCDC: LCD_DATA2; GPT11: GTIOC11A; IRQ: IRQ1" - None - - 
      P904 A16 - LCD_D8 - - Disabled - - "ESWM_GMII/MII1: ET1_RXD4; GLCDC: LCD_DATA8; GPT11: GTIOC11B; IRQ: IRQ2" - None - - 
      P905 A14 - ETH_RX_CLK - - Disabled - - "ADC1(Digital): AD1FLAG1; CEU: VIO_D6; ESWM_GMII/MII1: ET1_RX_CLK; ESWM_RGMII1: RGMII1_RXC; ESWM_RMII1: RMII1_REF50CK; GLCDC: LCD_DATA19; GPT13: GTCPPO13; IRQ: IRQ8; PDM1: PDMDAT1; SCI3: RXD3" - None - - 
      P906 A13 - ETH_RXD0 - - Disabled - - "ADC0(Digital): AD0FLAG1; CEU: VIO_D5; ESWM_GMII/MII1: ET1_RXD0; ESWM_RGMII1: RGMII1_RXD0; ESWM_RMII1: RMII1_RXD0; GLCDC: LCD_DATA20; GPT13: GTIOC13B; IRQ: IRQ9; PDM0: PDMDAT0; SCI6: CTS6; SSIE1: SSILRCK1; ULPT1: ULPTO1; USB FS: USB_ID" - None - - 
      P907 A15 - ETH_RXD1 - - Disabled - - "ADC(Digital): ADSYNC; CEU: VIO_D4; ESWM_GMII/MII1: ET1_RXD1; ESWM_RGMII1: RGMII1_RXD1; ESWM_RMII1: RMII1_RXD1; GLCDC: LCD_DATA21; GPT13: GTIOC13A; IRQ: IRQ10; PDM2: PDMCLK2; SCI6: DE6; SCI6: SCK6; SSIE1: SSIBCK1; ULPT1: ULPTEE1; USB FS: USB_EXICEN" - None - - 
      P908 B13 - ETH_RXD2 - - Disabled - - "ADC1(Digital): ADST1; CANFD1: CRX1; CEU: VIO_D3; ESWM_GMII/MII1: ET1_RXD2; ESWM_RGMII1: RGMII1_RXD2; GLCDC: LCD_DATA22; GPT12: GTIOC12B; IRQ: IRQ11; PDM1: PDMCLK1; SCI6: TXD6; ULPT1: ULPTEVI1; USB FS: USB_OVRCURB; USB HS: USBHS_ID" - None - - 
      P909 B14 - ETH_RXD3 - - Disabled - - "ADC0(Digital): ADST0; CANFD1: CTX1; CEU: VIO_D2; ESWM_GMII/MII1: ET1_RXD3; ESWM_RGMII1: RGMII1_RXD3; GLCDC: LCD_DATA23; GPT12: GTIOC12A; IRQ: IRQ21-DS; PDM0: PDMCLK0; SCI6: RXD6; ULPT1: ULPTOA1; USB FS: USB_OVRCURA; USB HS: USBHS_EXICEN" - None - - 
      P910 E11 - LCD_D4 - - Disabled - - "ESWM_GMII/MII1: ET1_TXD4; GLCDC: LCD_DATA4; GPT12: GTCPPO12; IRQ: IRQ7" - None - - 
      P911 C12 - LCD_D5 - - Disabled - - "ESWM_GMII/MII1: ET1_TXD5; GLCDC: LCD_DATA5; GPT3: GTIOC3B; IRQ: IRQ6" - None - - 
      P912 D12 - LCD_D6 - - Disabled - - "ESWM_GMII/MII1: ET1_TXD6; GLCDC: LCD_DATA6; GPT3: GTIOC3A; IRQ: IRQ5" - None - - 
      P913 E12 - LCD_D7 - - Disabled - - "CLKOUT: CLKOUT; ESWM_GMII/MII1: ET1_TXD7; GLCDC: LCD_DATA7; GPT11: GTCPPO11; IRQ: IRQ3" - None - - 
      P914 E5 - LCD_D0 - - Disabled - - "GLCDC: LCD_DATA0; GPT5: GTIOC5B; IRQ: IRQ9; SCI6: CTS_RTS6; SCI6: DE6" - None - - 
      P915 A6 - LCD_D1 - - Disabled - - "GLCDC: LCD_DATA1; GPT5: GTIOC5A; IRQ: IRQ8; SCI6: CTS6" - None - - 
      PA00 G1 - SDRAM_A3 - - Disabled - - "ADC1(Digital): AD1FLAG1; BUS: A5; CEU: VIO_D5; GLCDC: LCD_CLK; GPT7: GTCPPO7; GPT_OPS: GTOVLO; IRQ: IRQ22; SCI5: CTS_RTS5; SCI5: DE5; SDHI0: SD0DAT7; SDRAM: A5" - None - - 
      PA01 H4 - SDRAM_A2 - - Disabled - - "ADC0(Digital): AD0FLAG1; BUS: A4; CEU: VIO_D6; GLCDC: LCD_TCON0; GPT8: GTCPPO8; GPT_OPS: GTOVUP; IRQ: IRQ21; SCI5: CTS5; SDHI0: SD0DAT6; SDRAM: A4" - None - - 
      PA02 F1 - SDRAM_A1 L None Disabled - - "ADC(Digital): ADSYNC; BUS: A3; CEU: VIO_D7; GPT9: GTCPPO9; GPT_OPS: GTIW; IRQ: IRQ31; SCI2: RXD2; SDHI0: SD0DAT5; SDRAM: A3" - I - - 
      PA03 G2 - SDRAM_A0 - - Disabled - - "ADC1(Digital): ADST1; BUS: A2; CEU: VIO_D8; GPT10: GTCPPO10; GPT_OPS: GTIV; IRQ: IRQ20; SCI2: TXD2; SDHI0: SD0DAT4; SDRAM: A2" - None - - 
      PA04 D1 - SDRAM_DQM3 - - Disabled - - "ADC0(Digital): ADST0; BUS: A1; CEU: VIO_D9; GPT4: GTIOC4B; GPT_OPS: GTIU; IRQ: IRQ19; SCI2: DE2; SCI2: SCK2; SDHI0: SD0DAT3; SDRAM: A1; SDRAM: DQM3" - None - - 
      PA05 G3 - SDRAM_DQM1 - - Disabled - - "BUS: A0; BUS: BC0; CEU: VIO_D10; GPT4: GTIOC4A; GPT_POEGD: GTETRGD; IRQ: IRQ18; PDM2: PDMDAT2; SCI2: CTS_RTS2; SCI2: DE2; SDHI0: SD0DAT2; SDRAM: A0; SDRAM: DQM1" - None - - 
      PA06 C1 - SDRAM_CKE - - Disabled - - "BUS: CS1; CEU: VIO_D11; GPT7: GTIOC7B; GPT_POEGC: GTETRGC; IRQ: IRQ17; PDM1: PDMDAT1; SCI2: CTS2; SDHI0: SD0DAT1; SDRAM: CKE" - None - - 
      PA07 G4 - USER_LED3_RED - - Disabled - - "BUS: RD; CEU: VIO_D12; CMPOUT: VCOUT; GPT7: GTIOC7A; GPT_POEGB: GTETRGB; IRQ: IRQ16; PDM0: PDMDAT0; SCI7: CTS7; SDHI0: SD0DAT0" - None - - 
      PA08 F3 - SDRAM_WE - - Disabled - - "BUS: CS0; GLCDC: LCD_TCON3; GPT11: GTCPPO11; GPT_POEGD: GTETRGD; IRQ: IRQ6; SCI5: RXD5; SDRAM: WE" - None - - 
      PA09 F4 - SDRAM_CAS - - Disabled - - "BUS: CS3; GLCDC: LCD_TCON2; GPT12: GTCPPO12; IRQ: IRQ5; SCI5: TXD5; SDRAM: CAS" - None - - 
      PA10 F2 - SDRAM_RAS - - Disabled - - "BUS: CS2; CEU: VIO_D15; GLCDC: LCD_TCON1; GPT13: GTCPPO13; IRQ: IRQ4; PDM0: PDMCLK0; SCI5: DE5; SCI5: SCK5; SDRAM: RAS" - None - - 
      PA11 B4 - SDRAM_DQ8 - - Disabled - - "BUS: D8; GPT6: GTIOC6A; GPT_OPS: GTIV; IRQ: IRQ10; SCI9: DE9; SCI9: SCK9; SDRAM: DQ8" - None - - 
      PA12 B2 - SDRAM_DQ9 - - Disabled - - "BUS: D9; GPT6: GTIOC6B; GPT_OPS: GTIW; IRQ: IRQ11; SCI9: RXD9; SDRAM: DQ9" - None - - 
      PA13 C3 - SDRAM_DQ10 - - Disabled - - "BUS: D10; GPT10: GTIOC10A; GPT_OPS: GTOVUP; IRQ: IRQ12; SCI9: CTS_RTS9; SCI9: DE9; SDRAM: DQ10" - None - - 
      PA14 D4 - SDRAM_DQ11 - - Disabled - - "BUS: D11; GPT10: GTIOC10B; GPT_OPS: GTOVLO; IRQ: IRQ13; SCI9: TXD9; SDRAM: DQ11" - None - - 
      PA15 E1 - SDRAM_CLK - - Disabled - - "BUS: EBCLK; CEU: VIO_D14; GPT7: GTIOC7A; IRQ: IRQ14; PDM1: PDMCLK1; SCI9: CTS9; SDRAM: SDCLK" - None - - 
      PB00 E16 - LCD_D17 - - Disabled - - "ADC0(Digital): ADST0; ESWM_GMII/MII0: ET0_TXD0; ESWM_RGMII0: RGMII0_TXD0; ESWM_RMII0: RMII0_TXD0; GLCDC: LCD_DATA17; GPT4: GTCPPO4; IRQ: IRQ10; PDM2: PDMDAT2; SCI1: DE1; SCI1: SCK1; USB HS: USBHS_VBUSEN" - None - - 
      PB01 D17 - LCD_D13 - - Disabled - - "ADC1(Digital): AD1FLAG1; BUS: ALE; CEU: VIO_FLD; ESWM_GMII/MII0: ET0_TX_CLK; GLCDC: LCD_DATA13; GPT2: GTCPPO2; IRQ: IRQ12; SCI1: CTS_RTS1; SCI1: DE1" - None - - 
      PB02 E13 - CAM_VSYNC_LCD_D16 - - Disabled - - "ADC1(Digital): ADST1; CEU: VIO_VD; ESWM_GMII/MII0: ET0_TXD1; ESWM_RGMII0: RGMII0_TXD1; ESWM_RMII0: RMII0_TXD1; GLCDC: LCD_DATA16; GPT0: GTCPPO0; IRQ: IRQ11; SCI5: RXD5" - None - - 
      PB03 D16 - CAM_HSYNC_LCD_D15 - - Disabled - - "ADC(Digital): ADSYNC; CEU: VIO_HD; ESWM_GMII/MII0: ET0_TXD2; ESWM_RGMII0: RGMII0_TXD2; GLCDC: LCD_DATA15; GPT1: GTCPPO1; IRQ: IRQ13; SCI5: TXD5" - None - - 
      PB04 D13 - CAM_PCLK_LCD_D14 - - Disabled - - "ADC0(Digital): AD0FLAG1; CEU: VIO_CLK; ESWM_GMII/MII0: ET0_TXD3; ESWM_RGMII0: RGMII0_TXD3; GLCDC: LCD_DATA14; GPT3: GTCPPO3; IRQ: IRQ9; SCI5: DE5; SCI5: SCK5" - None - - 
      PB05 D15 - LCD_D12 - - Disabled - - "ESWM_GMII/MII0: ET0_TXD7; GLCDC: LCD_DATA12; GPT4: GTCPPO4; IRQ: IRQ15; SCI5: CTS5" - None - - 
      PB06 E14 - LCD_D11 - - Disabled - - "ESWM_GMII/MII0: ET0_TXD6; GLCDC: LCD_DATA11; GPT9: GTIOC9A; IRQ: IRQ0; SCI5: CTS_RTS5; SCI5: DE5" - None - - 
      PB07 D14 - LCD_D10 - - Disabled - - "ESWM_GMII/MII0: ET0_TXD5; GLCDC: LCD_DATA10; GPT9: GTIOC9B; IRQ: IRQ1" - None - - 
      PC00 M1 - SDRAM_DQ30 - - Disabled - - "BUS: D30; GPT7: GTCPPO7; IRQ: IRQ28; OSPI1: OM_1_SIO5; SCI7: CTS_RTS7; SCI7: DE7; SDRAM: DQ30" - None - - 
      PC01 M3 - SDRAM_DQ29 - - Disabled - - "BUS: D29; GPT6: GTCPPO6; IRQ: IRQ27; OSPI1: OM_1_SIO0; SCI7: CTS7; SDRAM: DQ29" - None - - 
      PC02 L2 - SDRAM_DQ28 - - Disabled - - "BUS: D28; GPT5: GTCPPO5; IRQ: IRQ26; OSPI1: OM_1_SIO3; SCI7: DE7; SCI7: SCK7; SDRAM: DQ28" - None - - 
      PC03 L1 - SDRAM_DQ27 - - Disabled - - "BUS: D27; GPT4: GTCPPO4; IRQ: IRQ25; OSPI1: OM_1_SIO4; SCI7: TXD7; SDRAM: DQ27" - None - - 
      PC04 L3 - SDRAM_DQ26 - - Disabled - - "BUS: D26; GPT3: GTCPPO3; IRQ: IRQ24; OSPI1: OM_1_SIO2; SCI7: RXD7; SDRAM: DQ26" - None - - 
      PC05 L5 - SDRAM_DQ25 - - Disabled - - "BUS: D25; GPT2: GTCPPO2; IRQ: IRQ23; OSPI1: OM_1_CS1; SDRAM: DQ25" - None - - 
      PC06 N4 - SDRAM_DQ24 - - Disabled - - "BUS: D24; GPT1: GTCPPO1; IRQ: IRQ22; OSPI1: OM_1_ECSINT1; SDRAM: DQ24" - None - - 
      PC07 K5 - SDRAM_DQ23 - - Disabled - - "BUS: D23; GPT0: GTCPPO0; IRQ: IRQ21; OSPI1: OM_1_RESET; SDRAM: DQ23" - None - - 
      PC08 M4 - SDRAM_DQ22 - - Disabled - - "BUS: D22; GPT8: GTCPPO8; IRQ: IRQ29; OSPI1: OM_1_CS0; SDRAM: DQ22" - None - - 
      PC09 L4 - SDRAM_DQ21 - - Disabled - - "BUS: D21; IRQ: IRQ5; OSPI1: OM_1_RSTO1; SDRAM: DQ21" - None - - 
      PC10 M5 - SDRAM_DQ20 - - Disabled - - "BUS: D20; GPT13: GTCPPO13; IRQ: IRQ4; OSPI1: OM_1_WP1; SDRAM: DQ20" - None - - 
      PC11 H5 - SDRAM_DQ19 - - Disabled - - "BUS: D19; ESWM_GMII/MII: ET0_MDC; ESWM_RGMII0: ET0_MDC; ESWM_RMII0: ET0_MDC; GPT12: GTCPPO12; IRQ: IRQ3; SCI6: CTS_RTS6; SCI6: DE6; SDRAM: DQ19" - None - - 
      PC12 G5 - SDRAM_DQ18 - - Disabled - - "BUS: D18; ESWM_GMII/MII: ET0_MDIO; ESWM_RGMII0: ET0_MDIO; ESWM_RMII0: ET0_MDIO; GPT11: GTCPPO11; IRQ: IRQ2; SCI6: DE6; SCI6: SCK6; SDRAM: DQ18" - None - - 
      PC13 J5 - SDRAM_DQ17 - - Disabled - - "BUS: D17; ESWM_GMII/MII: ET0_INT; ESWM_RGMII0: ET0_INT; ESWM_RMII0: ET0_INT; GPT10: GTCPPO10; IRQ: IRQ1; SCI6: RXD6; SDRAM: DQ17" - None - - 
      PC14 F5 - SDRAM_DQ16 - - Disabled - - "BUS: D16; ESWM_GMII/MII: ET0_WOL; ESWM_RGMII0: ET0_WOL; ESWM_RMII0: ET0_WOL; GPT: GTADSM1; GPT9: GTCPPO9; IRQ: IRQ0; SCI6: TXD6; SDRAM: DQ16" - None - - 
      PC15 K1 - SDRAM_BA1 - - Disabled - - "BUS: A16; CANFD1: CRX1; GPT: GTADSM0; IRQ: IRQ30; SCI6: CTS6; SDRAM: A16" - None - - 
      PD00 K4 - SDRAM_BA0 - - Disabled - - "BUS: A15; CANFD1: CTX1; GPT5: GTCPPO5; GPT_OPS: GTOWLO; IRQ: IRQ23; SCI5: DE5; SCI5: SCK5; SDRAM: A15" - None - - 
      PD01 B16 - ARDUINO_D8_MIKROBUS_INT - - Disabled - - "ESWM_GMII/MII1: ET1_RXD6; GPT2: GTCPPO2; IRQ: IRQ22; SCI8: DE8; SCI8: SCK8; SDHI0: SD0DAT2" - None - - 
      PD02 B17 - JLINK_VCOM_TX L None Disabled - - "ESWM_GMII/MII1: ET1_RXD7; GPT1: GTCPPO1; IRQ: IRQ21; SCI8: TXD8; SDHI0: SD0DAT1" - O - - 
      PD03 C15 - JLINK_VCOM_RXD L None Disabled - - "ESWM_GMII/MII0: ET0_RXD4; GPT3: GTIOC3B; IRQ: IRQ21; SCI8: RXD8; SDHI0: SD0DAT0; USB HS: USBHS_EXICEN" - I - - 
      PD04 C14 - JLINK_VCOM_CTS_RTS - - Disabled - - "ESWM_GMII/MII0: ET0_RXD5; GPT3: GTIOC3A; IRQ: IRQ20; SCI8: CTS_RTS8; SCI8: DE8; SDHI0: SD0CMD; USB HS: USBHS_ID" - None - - 
      PD05 C16 - JLINK_VCOM_CTS - - Disabled - - "ESWM_GMII/MII0: ET0_RXD6; GPT2: GTIOC2B; IRQ: IRQ19; SCI8: CTS8; SDHI0: SD0CLK; USB HS: USBHS_OVRCURB" - None - - 
      PD06 C17 - AUDIO_MCLK - - Disabled - - "ESWM_GMII/MII0: ET0_RXD7; GPT2: GTIOC2A; IRQ: IRQ18; SDHI0: SD0WP; USB HS: USBHS_OVRCURA" - None - - 
      PD07 E15 - USB_HS_VBUS_SEL - - Disabled - - "ESWM_GMII/MII0: ET0_TXD4; GPT0: GTCPPO0; IRQ: IRQ17; SDHI0: SD0CD; USB HS: USBHS_VBUSEN" - None - - 
      RES D5 CGC_RES - - - - - - - - IO "Read only" - 
      USBHS_DM H17 CGC_USBHS_DM - - - - - - - - IO "Read only" - 
      USBHS_DP H16 CGC_USBHS_DP - - - - - - - - IO "Read only" - 
      USBHS_RREF J15 CGC_USBHS_RREF - - - - - - - - IO "Read only" - 
      VBATT M16 CGC_VBATT - - - - - - - - IO "Read only" - 
      VCC H11 CGC_VCC - - - - - - - - IO "Read only" - 
      VCC H14 CGC_VCC - - - - - - - - IO "Read only" - 
      VCC G11 CGC_VCC - - - - - - - - IO "Read only" - 
      VCC G16 CGC_VCC - - - - - - - - IO "Read only" - 
      VCC F6 CGC_VCC - - - - - - - - IO "Read only" - 
      VCC G6 CGC_VCC - - - - - - - - IO "Read only" - 
      VCC F11 CGC_VCC - - - - - - - - IO "Read only" - 
      VCC H6 CGC_VCC - - - - - - - - IO "Read only" - 
      VCC L15 CGC_VCC - - - - - - - - IO "Read only" - 
      VCC K14 CGC_VCC - - - - - - - - IO "Read only" - 
      VCC18_MIPI R2 CGC_VCC18_MIPI - - - - - - - - IO "Read only" - 
      VCC2 R1 CGC_VCC2 - - - - - - - - IO "Read only" - 
      VCC2 J6 CGC_VCC2 - - - - - - - - IO "Read only" - 
      VCC2 L6 CGC_VCC2 - - - - - - - - IO "Read only" - 
      VCC2 M7 CGC_VCC2 - - - - - - - - IO "Read only" - 
      VCC2 M8 CGC_VCC2 - - - - - - - - IO "Read only" - 
      VCC_DCDC A10 CGC_VCC_DCDC - - - - - - - - IO "Read only" - 
      VCC_DCDC A11 CGC_VCC_DCDC - - - - - - - - IO "Read only" - 
      VCC_DCDC B10 CGC_VCC_DCDC - - - - - - - - IO "Read only" - 
      VCC_DCDC B11 CGC_VCC_DCDC - - - - - - - - IO "Read only" - 
      VCC_USB U17 CGC_VCC_USB - - - - - - - - IO "Read only" - 
      VCC_USBHS H15 CGC_VCC_USBHS - - - - - - - - IO "Read only" - 
      VCL F9 CGC_VCL - - - - - - - - IO "Read only" - 
      VCL G9 CGC_VCL - - - - - - - - IO "Read only" - 
      VCL H9 CGC_VCL - - - - - - - - IO "Read only" - 
      VCL M11 CGC_VCL - - - - - - - - IO "Read only" - 
      VCL J8 CGC_VCL - - - - - - - - IO "Read only" - 
      VCL J9 CGC_VCL - - - - - - - - IO "Read only" - 
      VCL K8 CGC_VCL - - - - - - - - IO "Read only" - 
      VCL K9 CGC_VCL - - - - - - - - IO "Read only" - 
      VCL L10 CGC_VCL - - - - - - - - IO "Read only" - 
      VCL L11 CGC_VCL - - - - - - - - IO "Read only" - 
      VCL K11 CGC_VCL - - - - - - - - IO "Read only" - 
      VCL J11 CGC_VCL - - - - - - - - IO "Read only" - 
      VLO A7 CGC_VLO - - - - - - - - IO "Read only" - 
      VLO A8 CGC_VLO - - - - - - - - IO "Read only" - 
      VLO B7 CGC_VLO - - - - - - - - IO "Read only" - 
      VLO B8 CGC_VLO - - - - - - - - IO "Read only" - 
      VREFH U9 CGC_VREFH - - - - - - - - IO "Read only" - 
      VREFH0 U10 CGC_VREFH0 - - - - - - - - IO "Read only" - 
      VREFL T9 CGC_VREFL - - - - - - - - IO "Read only" - 
      VREFL0 T10 CGC_VREFL0 - - - - - - - - IO "Read only" - 
      VSS A9 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS B9 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS H10 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS H12 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS U4 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS G10 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS G15 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS G17 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS F7 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS F8 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS G7 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS G8 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS F10 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS H7 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS H8 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS M10 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS J7 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS M17 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS K6 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS K7 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS L7 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS L8 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS L12 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS L9 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS K10 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS K12 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS J10 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS J12 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS J14 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS1_USBHS J17 CGC_VSS1_USBHS - - - - - - - - IO "Read only" - 
      VSS2_USBHS J16 CGC_VSS2_USBHS - - - - - - - - IO "Read only" - 
      VSS_MIPI R3 CGC_VSS_MIPI - - - - - - - - IO "Read only" - 
      VSS_USB T17 CGC_VSS_USB - - - - - - - - IO "Read only" - 
    R7FA4E10D2CFM.pincfg -> 
      AVCC0 R9 CGC_AVCC0 - - - - - - - - IO "Read only" - 
      AVCC_MIPI T4 CGC_AVCC_MIPI - - - - - - - - IO "Read only" - 
      AVCC_USBHS K15 CGC_AVCC_USBHS - - - - - - - - IO "Read only" - 
      AVSS0 R10 CGC_AVSS0 - - - - - - - - IO "Read only" - 
      MIPI_CLN U2 CGC_MIPI_CLN - - - - - - - - IO "Read only" - 
      MIPI_CLP T2 CGC_MIPI_CLP - - - - - - - - IO "Read only" - 
      MIPI_DL0N U1 CGC_MIPI_DL0N - - - - - - - - IO "Read only" - 
      MIPI_DL0P T1 CGC_MIPI_DL0P - - - - - - - - IO "Read only" - 
      MIPI_DL1N U3 CGC_MIPI_DL1N - - - - - - - - IO "Read only" - 
      MIPI_DL1P T3 CGC_MIPI_DL1P - - - - - - - - IO "Read only" - 
      P000 U13 - S4_INT - - Disabled - - "ACMPHS: IVCMP2; ADC0: AN000; IRQ: IRQ6-DS" - None - - 
      P001 T13 - ARDUINO_A0 - - Disabled - - "ACMPHS: IVCMP3; ADC0: AN001; IRQ: IRQ7-DS" - None - - 
      P002 U14 - GROVE2_2_AN - - Disabled - - "ACMPHS: IVCMP2; ADC0: AN002; IRQ: IRQ8-DS" - None - - 
      P003 R12 - ARDUINO_A2 - - Disabled - - "ACMPHS: IVCMP3; ADC0: AN003; IRQ: IRQ29" - None - - 
      P004 T11 - ARDUINO_A3_MIKROBUS_AN - - Disabled - - "ACMPHS: IVCMP2; ADC0: AN004; IRQ: IRQ9-DS" - None - - 
      P005 R11 - GROVE2_1_AN - - Disabled - - "ACMPHS: IVCMP3; ADC0: AN005; IRQ: IRQ10-DS" - None - - 
      P006 U12 - PMOD1_7_INT - - Disabled - - "ACMPHS: IVCMP2; ADC1: AN006; IRQ: IRQ11-DS" - None - - 
      P007 T12 - ARDUINO_A1 - - Disabled - - "ACMPHS: IVCMP3; ADC1: AN007; IRQ: IRQ28" - None - - 
      P008 U11 - USER_S2 - - Disabled - - "ACMPHS: IVREF0; ADC1: AN008; IRQ: IRQ12-DS" - None - - 
      P009 P11 - USER_S1 - - Disabled - - "ACMPHS: IVREF1; ADC1: AN009; IRQ: IRQ13-DS" - None - - 
      P010 P10 - CAM_INT - - Disabled - - "ADC1: AN010; IRQ: IRQ14" - None - - 
      P011 N10 - ARDUINO_D2 - - Disabled - - "ADC1: AN011; IRQ: IRQ16" - None - - 
      P012 P9 - PMOD2_7_IRQ15 - - Disabled - - "ADC0: AN012; IRQ: IRQ15" - None - - 
      P013 N9 - I2C_SCL0_PULLUP - - Disabled - - "ADC1: AN013; IRQ: IRQ14" - None - - 
      P014 T8 - ARDUINO_A4 - - Disabled - - "ACMPHS: IVCMP0; ADC0: AN014; DAC120: DA0; IRQ: IRQ27" - None - - 
      P015 U8 - ARDUINO_A5 - - Disabled - - "ACMPHS: IVCMP0; ADC1: AN015; DAC121: DA1; IRQ: IRQ13" - None - - 
      P100 U6 - OSPI_DQ0_ARDUINO_D12_MISOB_MIKROBUS_MISOB - - Disabled - - "AGT0: AGTIO0; ESWM_GMII/MII: GPTP1_MATCH; ESWM_RGMII1: GPTP1_MATCH; ESWM_RMII1: GPTP1_MATCH; GPT8: GTIOC8B; GPT_POEGA: GTETRGA; IRQ: IRQ2; OSPI0: OM_0_SIO0; SCI9: DE9; SCI9: SCK9; SPI1: MISO1" - None - - 
      P101 R5 - OSPI_DQ3_ARDUINO_D11_MOSIB_MIKROBUS_MOSIB - - Disabled - - "AGT0: AGTEE0; ESWM_GMII/MII: GPTP1_CAPTURE; ESWM_RGMII1: GPTP1_CAPTURE; ESWM_RMII1: GPTP1_CAPTURE; GPT8: GTIOC8A; GPT_POEGB: GTETRGB; IRQ: IRQ1; OSPI0: OM_0_SIO3; SCI9: RXD9; SPI1: MOSI1" - None - - 
      P102 P5 - OSPI_DQ4_ARDUINO_D13_RSPCKB_MIKROBUS_RSPCKB - - Disabled - - "ADC0(Digital): ADTRG0; AGT0: AGTO0; CANFD0: CRX0; GPT2: GTIOC2B; GPT_OPS: GTOWLO; IRQ: IRQ17; OSPI0: OM_0_SIO4; SCI9: TXD9; SPI1: RSPCK1" - None - - 
      P103 R4 - OSPI_DQ2_ARDUINO_D10_SSLB_MIKROBUS_SSLB - - Disabled - - "ADC1(Digital): AD1FLAG1; CANFD0: CTX0; ESWM_GMII/MII: GPTP0_PPS; ESWM_RGMII0: GPTP0_PPS; ESWM_RMII0: GPTP0_PPS; GPT2: GTIOC2A; GPT_OPS: GTOWUP; IRQ: IRQ16; OSPI0: OM_0_SIO2; SCI9: CTS_RTS9; SCI9: DE9; SPI1: SSLB0" - None - - 
      P104 M6 - OSPI_CS_ARDUINO_D5 - - Disabled - - "ADC0(Digital): AD0FLAG1; ESWM_GMII/MII: GPTP0_MATCH; ESWM_RGMII0: GPTP0_MATCH; ESWM_RMII0: GPTP0_MATCH; GPT1: GTIOC1B; GPT_POEGB: GTETRGB; IRQ: IRQ1; OSPI0: OM_0_CS1; SCI9: CTS9; SPI1: SSLB1" - None - - 
      P105 N7 - OSPI_INT_ARDUINO_D6 - - Disabled - - "ADC(Digital): ADSYNC; ESWM_GMII/MII: GPTP0_CAPTURE; ESWM_RGMII0: GPTP0_CAPTURE; ESWM_RMII0: GPTP0_CAPTURE; GPT1: GTIOC1A; IRQ: IRQ0; OSPI0: OM_0_ECSINT1; SCI8: CTS_RTS8; SCI8: DE8; SPI1: SSLB2; ULPT1: ULPTO1-DS" - None - - 
      P106 N6 - OSPI_RES - - Disabled - - "ADC1(Digital): ADST1; AGT0: AGTOB0; ESWM_GMII/MII: ET1_LINKSTA; ESWM_RGMII1: ET1_LINKSTA; ESWM_RMII1: ET1_LINKSTA; GPT8: GTIOC8B; GPT_OPS: GTOWLO; IRQ: IRQ16; OSPI0: OM_0_RESET; SCI8: CTS8; SPI1: SSLB3; ULPT1: ULPTEE1-DS" - None - - 
      P107 N5 - ETH_MDINT - - Disabled - - "ADC0(Digital): ADST0; AGT0: AGTOA0; ESWM_GMII/MII: ET1_INT; ESWM_RGMII1: ET1_INT; ESWM_RMII1: ET1_INT; GPT8: GTIOC8A; GPT_OPS: GTOWUP; IRQ: IRQ31; OSPI0: OM_0_CS0; SCI4: CTS4" - None - - 
      P108 D8 - - - - Disabled - - "GPT10: GTIOC10B; IRQ: IRQ24; SDHI0: SD0DAT6" - None - - 
      P109 D7 - I2C_SDA0_PULLUP - - Disabled - - "GPT10: GTIOC10A; IRQ: IRQ23; SDHI0: SD0DAT5" - None - - 
      P110 C8 - ARDUINO_D9 - - Disabled - - "GPT9: GTIOC9B; IRQ: IRQ20; SDHI0: SD0DAT4" - None - - 
      P111 E8 - LCD_INT_MIPI_IRQ19 - - Disabled - - "GPT9: GTIOC9A; IRQ: IRQ19; SDHI0: SD0DAT3" - None - - 
      P112 A4 - SDRAM_DQ3 - - Disabled - - "ADC0(Digital): ADST0; BUS: D3; GLCDC: LCD_DATA10; GPT3: GTIOC3B; GPT_POEGA: GTETRGA; IRQ: IRQ27; SCI0: TXD0; SDHI0: SD0DAT4; SDRAM: DQ3; SPI0: SSLA2; SSIE0: SSIBCK0; ULPT0: ULPTOB0-DS" - None - - 
      P113 A2 - SDRAM_DQ4 - - Disabled - - "ADC1(Digital): ADST1; BUS: D4; GLCDC: LCD_DATA9; GPT2: GTIOC2A; GPT_POEGB: GTETRGB; IRQ: IRQ28; SCI0: RXD0; SDHI0: SD0DAT5; SDRAM: DQ4; SPI0: SSLA1; SSIE0: SSILRCK0; ULPT0: ULPTOA0-DS" - None - - 
      P114 B3 - SDRAM_DQ5 - - Disabled - - "ADC(Digital): ADSYNC; BUS: D5; GLCDC: LCD_DATA8; GPT2: GTIOC2B; GPT_POEGC: GTETRGC; IRQ: IRQ30-DS; SCI0: CTS_RTS0; SCI0: DE0; SDHI0: SD0DAT6; SDRAM: DQ5; SPI0: SSLA0; SSIE0: SSIRXD0" - None - - 
      P115 A3 - SDRAM_DQ6 - - Disabled - - "ADC0(Digital): AD0FLAG1; BUS: D6; GLCDC: LCD_DATA7; GPT5: GTIOC5A; GPT_POEGD: GTETRGD; IRQ: IRQ31-DS; SCI0: CTS0; SDHI0: SD0DAT7; SDRAM: DQ6; SPI0: MOSI0; SSIE0: SSITXD0" - None - - 
      P200 C5 - NMI - - Disabled - - "IRQ: NMI" - None - - 
      P201 E6 - MD_MIKROBUS_RES - - Disabled - - "CGC: MD; IRQ: IRQ4" - None - - 
      P206 B15 - ENET_RX_CTL - - Disabled - - "BUS: CS7; CEU: VIO_D0; CLKOUT: CLKOUT; ESWM_GMII/MII1: ET1_RX_DV; ESWM_RGMII1: RGMII1_RX_CTL; ESWM_RMII1: RMII1_CRS_DV; GPT0: GTCPPO0; GPT_OPS: GTIU; IRQ: IRQ0-DS; SDHI0: SD0DAT7; SSIE1: SSIDATA1; ULPT1: ULPTOB1; USB FS: USB_VBUSEN" - None - - 
      P207 A17 - LCD_D9 - - Disabled - - "ESWM_GMII/MII1: ET1_RXD5; GLCDC: LCD_DATA9; GPT3: GTCPPO3; IRQ: IRQ25" - None - - 
      P208 C7 - DEBUG_TDI - - Disabled - - "CANFD1: CRX1; CMPOUT: VCOUT; GPT1: GTIOC1B; GPT_OPS: GTOVLO; IRQ: IRQ3; JTAG/SWD: TDI; SCI9: RXD9" - None - - 
      P209 E7 - DEBUG_TDO_SWO - - Disabled - - "CANFD1: CTX1; CLKOUT: CLKOUT; GPT1: GTIOC1A; GPT_OPS: GTOVUP; IRQ: IRQ25; JTAG/SWD: TDO; SCI9: TXD9; TRACE: SWO" - None - - 
      P210 C6 - DEBUG_TMS_SWDIO L None Disabled - - "GPT0: GTIOC0B; GPT_OPS: GTOULO; IRQ: IRQ24; JTAG/SWD: SWDIO; JTAG/SWD: TMS; SCI9: CTS_RTS9; SCI9: DE9" - IO - - 
      P211 D6 - DEBUG_TCLK_SWCLK L None Disabled - - "GPT0: GTIOC0A; GPT_OPS: GTOUUP; IRQ: IRQ23; JTAG/SWD: SWCLK; JTAG/SWD: TCK; SCI9: DE9; SCI9: SCK9" - IO - - 
      P212 K17 - EXTAL - - Disabled - - "AGT1: AGTEE1; CGC: EXTAL; GPT0: GTIOC0B; GPT_POEGD: GTETRGD; IRQ: IRQ3; SCI1: RXD1" - None - - 
      P213 K16 - XTAL - - Disabled - - "ADC1(Digital): ADTRG1; CGC: XTAL; GPT0: GTIOC0A; GPT_POEGC: GTETRGC; IRQ: IRQ2; SCI1: TXD1; ULPT0: ULPTEE0" - None - - 
      P214 L16 - XCOUT - - Disabled - - "CGC: XCOUT; IRQ: IRQ21" - None - - 
      P215 L17 - XCIN - - Disabled - - "CGC: EXCIN; CGC: XCIN; IRQ: IRQ20" - None - - 
      P300 B5 - SDRAM_DQ2 - - Disabled - - "BUS: D2; GLCDC: LCD_DATA11; GPT3: GTIOC3A; IRQ: IRQ4; SCI0: DE0; SCI0: SCK0; SDHI0: SD0DAT3; SDRAM: DQ2; SPI0: SSLA3; ULPT0: ULPTEVI0-DS" - None - - 
      P301 C4 - SDRAM_DQ1 - - Disabled - - "AGT0: AGTIO0; BUS: D1; GLCDC: LCD_DATA12; GPT4: GTIOC4B; GPT_OPS: GTOULO; IRQ: IRQ6; SCI6: TXD6; SDHI0: SD0DAT2; SDRAM: DQ1; ULPT0: ULPTEE0-DS" - None - - 
      P302 A5 - SDRAM_DQ0 - - Disabled - - "BUS: D0; GLCDC: LCD_DATA13; GPT4: GTIOC4A; GPT_OPS: GTOUUP; IRQ: IRQ5; SCI6: RXD6; SDHI0: SD0DAT1; SDRAM: DQ0; ULPT0: ULPTO0-DS" - None - - 
      P303 B6 - USER_LED2_GREEN - - Disabled - - "GLCDC: LCD_DATA14; GPT7: GTIOC7B; IRQ: IRQ29-DS; SCI6: DE6; SCI6: SCK6" - None - - 
      P304 D10 - ETH_TXD3_TRACE_TDATA3 - - Disabled - - "CEU: VIO_D15; ESWM_GMII/MII1: ET1_TXD3; ESWM_RGMII1: RGMII1_TXD3; GPT7: GTIOC7A; GPT_OPS: GTOVLO; IRQ: IRQ9; SDHI0: SD0DAT0; TRACE: TDATA3; ULPT1: ULPTO1" - None - - 
      P305 C10 - ETH_TXD2_TRACE_TDATA2 - - Disabled - - "CEU: VIO_D14; ESWM_GMII/MII1: ET1_TXD2; ESWM_RGMII1: RGMII1_TXD2; GPT12: GTCPPO12; GPT_OPS: GTOVUP; IRQ: IRQ8; SDHI0: SD0WP; TRACE: TDATA2; ULPT1: ULPTEE1" - None - - 
      P306 D11 - ETH_TXD1_TRACE_TDATA1 - - Disabled - - "CEU: VIO_D13; ESWM_GMII/MII1: ET1_TXD1; ESWM_RGMII1: RGMII1_TXD1; ESWM_RMII1: RMII1_TXD1; GPT11: GTCPPO11; GPT_OPS: GTIW; IRQ: IRQ28-DS; SDHI0: SD0CD; TRACE: TDATA1; ULPT1: ULPTEVI1" - None - - 
      P307 C11 - ETH_TXD0_TRACE_TDATA0 - - Disabled - - "CEU: VIO_D12; ESWM_GMII/MII1: ET1_TXD0; ESWM_RGMII1: RGMII1_TXD0; ESWM_RMII1: RMII1_TXD0; GPT10: GTCPPO10; GPT_OPS: GTIV; IRQ: IRQ27-DS; SCI6: CTS_RTS6; SCI6: DE6; SDHI0: SD0CMD; TRACE: TDATA0; ULPT1: ULPTOA1" - None - - 
      P308 C9 - TRACE_TCLK - - Disabled - - "CEU: VIO_D11; ESWM_GMII/MII1: ET1_TX_ER; ETHPHYCLK: ETHPHYCLK; GPT9: GTCPPO9; GPT_OPS: GTIU; IRQ: IRQ26-DS; SCI3: CTS3; SDHI0: SD0CLK; TRACE: TCLK; ULPT1: ULPTOB1" - None - - 
      P309 A12 - ETH_TX_CLK - - Disabled - - "CEU: VIO_D10; CMPOUT: VCOUT; ESWM_GMII/MII1: ET1_GTX_CLK; ESWM_RGMII1: RGMII1_TXC; GLCDC: LCD_DATA15; GPT8: GTCPPO8; IRQ: IRQ25-DS; SCI9: CTS9" - None - - 
      P310 E10 - ETH_TX_CTL - - Disabled - - "AGT1: AGTEE1; CEU: VIO_D9; ESWM_GMII/MII1: ET1_TX_EN; ESWM_RGMII1: RGMII1_TX_CTL; ESWM_RMII1: RMII1_TX_EN; GLCDC: LCD_DATA16; GPT7: GTCPPO7; IRQ: IRQ24-DS; SCI3: TXD3" - None - - 
      P311 B12 - CAM_D8 - - Disabled - - "AGT1: AGTOB1; CANFD0: CRX0; CEU: VIO_D8; ESWM_GMII/MII1: ET1_TX_CLK; GLCDC: LCD_DATA17; GPT: GTADSM1; GPT6: GTCPPO6; IRQ: IRQ23-DS; SCI3: DE3; SCI3: SCK3" - None - - 
      P312 C13 - ARDUINO_D7 - - Disabled - - "AGT1: AGTOA1; CANFD0: CTX0; CEU: VIO_D7; ESWM_GMII/MII1: ET1_RX_ER; ESWM_RMII1: RMII1_RX_ER; GLCDC: LCD_DATA18; GPT: GTADSM0; GPT5: GTCPPO5; IRQ: IRQ22-DS; PDM2: PDMDAT2; SCI3: CTS_RTS3; SCI3: DE3" - None - - 
      P400 P17 - CAM_D0_ARDUINO_GROVE1_SCL0 - - Disabled - - "ADC1(Digital): ADTRG1; AGT1: AGTIO1; CEU: VIO_D0; GPT6: GTIOC6A; I3C0: I3C_SCL0; IRQ: IRQ0; SCI1: TXD1; SDHI1: SD1CLK; SSIE: AUDIO_CLK" - None - - 
      P401 N17 - ARDUINO_GROVE1_SDA0 - - Disabled - - "CANFD0: CTX0; CEU: VIO_D1; GPT6: GTIOC6B; GPT_POEGA: GTETRGA; I3C0: I3C_SDA0; IRQ: IRQ5-DS; SCI1: RXD1; SDHI1: SD1CMD" - None - - 
      P402 L14 - PMOD1_8_GPIO_RST - - Disabled - - "CAC: CACREF; CANFD0: CRX0; ESWM_GMII/MII: ET0_LINKSTA; ESWM_RGMII0: ET0_LINKSTA; ESWM_RMII0: ET0_LINKSTA; IRQ: IRQ4-DS; RTC: RTCIC0; SCI1: DE1; SCI1: SCK1; SDHI1: SD1DAT0; SSIE: AUDIO_CLK" - None - - 
      P403 H13 - AUDIO_BCLK - - Disabled - - "ADC0(Digital): AD0FLAG1; ESWM_GMII/MII: ET1_WOL; ESWM_RGMII1: ET1_WOL; ESWM_RMII1: ET1_WOL; GPT3: GTIOC3A; IRQ: IRQ14-DS; RTC: RTCIC1; SCI1: CTS_RTS1; SCI1: DE1; SDHI1: SD1DAT1; SSIE0: SSIBCK0" - None - - 
      P404 J13 - AUDIO_WCLK - - Disabled - - "ADC1(Digital): AD1FLAG1; ESWM_GMII/MII: ET0_WOL; ESWM_RGMII0: ET0_WOL; ESWM_RMII0: ET0_WOL; GPT3: GTIOC3B; IRQ: IRQ15-DS; RTC: RTCIC2; SCI1: CTS1; SDHI1: SD1DAT2; SSIE0: SSILRCK0" - None - - 
      P405 G12 - CAM_D2_AUDIO_DATIN - - Disabled - - "AGT1: AGTIO1; CEU: VIO_D2; ESWM_GMII/MII0: ET0_RX_DV; ESWM_RGMII0: RGMII0_RX_CTL; ESWM_RMII0: RMII0_CRS_DV; GPT1: GTIOC1A; IRQ: IRQ30; SCI2: DE2; SCI2: SCK2; SDHI1: SD1DAT3; SSIE0: SSITXD0" - None - - 
      P406 F14 - CAM_D3_AUDIO_DOUT - - Disabled - - "CEU: VIO_D3; ESWM_GMII/MII0: ET0_RXD3; ESWM_RGMII0: RGMII0_RXD3; GPT1: GTIOC1B; IRQ: IRQ31; SCI2: TXD2; SDHI1: SD1CD; SPI0: SSLA3; SSIE0: SSIRXD0" - None - - 
      P407 R17 - USBFS_VBUS - - Disabled - - "ADC0(Digital): ADTRG0; AGT0: AGTIO0; BUS: CS6; ESWM_GMII/MII: GPTP_PTPOUT3; ESWM_RGMII: GPTP_PTPOUT3; ESWM_RMII: GPTP_PTPOUT3; GPT10: GTIOC10B; IIC0: SDA0; IRQ: IRQ22; RTC: RTCOUT; SCI1: DE1; SCI1: SCK1; USB FS: USB_VBUS; USB HS: USBHS_VBUSEN" - None - - 
      P408 M15 - USBHS_VBUS - - Disabled - - "ADC(Digital): ADSYNC; BUS: A17; ESWM_GMII/MII: GPTP_PTPOUT2; ESWM_RGMII: GPTP_PTPOUT2; ESWM_RMII: GPTP_PTPOUT2; GPT10: GTIOC10A; GPT_OPS: GTOWLO; IIC0: SCL0; IRQ: IRQ7; SCI3: RXD3; ULPT0: ULPTOB0; USB FS: USB_VBUSEN; USB HS: USBHS_VBUS" - None - - 
      P409 R16 - PMOD2_9_GPIO - - Disabled - - "ADC1(Digital): ADST1; BUS: A18; ESWM_GMII/MII: GPTP0_CAPTURE; ESWM_RGMII0: GPTP0_CAPTURE; ESWM_RMII0: GPTP0_CAPTURE; GPT_OPS: GTOWUP; IIC0: SDA0; IRQ: IRQ6; SCI3: TXD3; ULPT0: ULPTOA0; USB FS: USB_OVRCURA-DS; USB HS: USBHS_OVRCURA" - None - - 
      P410 K13 - PMOD2_8_GPIO_RST - - Disabled - - "ADC0(Digital): ADST0; AGT1: AGTOB1; BUS: A19; ESWM_GMII/MII: GPTP0_MATCH; ESWM_RGMII0: GPTP0_MATCH; ESWM_RMII0: GPTP0_MATCH; GPT9: GTIOC9B; GPT_OPS: GTOVLO; IIC0: SCL0; IRQ: IRQ5; SCI3: DE3; SCI3: SCK3; USB FS: USB_OVRCURB-DS; USB HS: USBHS_OVRCURB" - None - - 
      P411 M14 - DSI_TE - - Disabled - - "AGT1: AGTOA1; BUS: A20; CAC: CACREF; ESWM_GMII/MII: GPTP_PTPOUT1; ESWM_RGMII: GPTP_PTPOUT1; ESWM_RMII: GPTP_PTPOUT1; GPT9: GTIOC9A; GPT_OPS: GTOVUP; IRQ: IRQ4; MIPI: DSI_TE; SCI3: CTS_RTS3; SCI3: DE3; USB FS: USB_ID; USB HS: USBHS_ID" - None - - 
      P412 M12 - PMOD1_9_GPIO - - Disabled - - "AGT1: AGTEE1; BUS: A21; ESWM_GMII/MII: GPTP_PTPOUT0; ESWM_RGMII: GPTP_PTPOUT0; ESWM_RMII: GPTP_PTPOUT0; GPT8: GTCPPO8; GPT_OPS: GTOULO; IRQ: IRQ20-DS; SCI3: CTS3; USB FS: USB_EXICEN; USB HS: USBHS_EXICEN" - None - - 
      P413 P14 - PMOD1_10_GPIO - - Disabled - - "BUS: A22; ESWM_GMII/MII: ET_TAS_STA3; ESWM_RGMII: ET_TAS_STA3; ESWM_RMII: ET_TAS_STA3; GPT7: GTCPPO7; GPT_OPS: GTOUUP; IRQ: IRQ18; ULPT1: ULPTEE1" - None - - 
      P414 L13 - ETH_MDIO - - Disabled - - "BUS: A23; CANFD1: CRX1; CEU: VIO_CLK; ESWM_GMII/MII: ET1_MDIO; ESWM_RGMII1: ET1_MDIO; ESWM_RMII1: ET1_MDIO; GPT0: GTIOC0B; IRQ: IRQ9; SCI4: RXD4; SPI1: SSLB0" - None - - 
      P415 R15 - ETH_MDC - - Disabled - - "BUS: WAIT; CANFD1: CTX1; CEU: VIO_HD; ESWM_GMII/MII: ET1_MDC; ESWM_RGMII1: ET1_MDC; ESWM_RMII1: ET1_MDC; GPT0: GTIOC0A; IRQ: IRQ8; SCI4: TXD4; SPI1: RSPCK1" - None - - 
      P500 U7 - USBFS_VBUSEN - - Disabled - - "ADC0: AN021; ADC1: AN021; CAC: CACREF; GPT11: GTIOC11B; IRQ: IRQ24; PDM0: PDMDAT0; SCI8: RXD8; SDHI1: SD1DAT5; USB FS: USB_VBUSEN" - None - - 
      P501 R8 - CAM_XCLK - - Disabled - - "ADC0: AN020; ADC1: AN020; GPT12: GTIOC12A; IRQ: IRQ25; PDM1: PDMDAT1; SCI8: TXD8; SDHI1: SD1DAT6; USB FS: USB_OVRCURA" - None - - 
      P502 T7 - MEMS_MIC_DATA L None Disabled - - "ADC0: AN019; ADC1: AN019; GPT12: GTIOC12B; IRQ: IRQ26; PDM2: PDMDAT2; SCI8: DE8; SCI8: SCK8; SDHI1: SD1DAT7; USB FS: USB_OVRCURB" - I - - 
      P503 H2 - SDRAM_A4 - - Disabled - - "BUS: A6; CEU: VIO_D4; GPT6: GTCPPO6; GPT_OPS: GTOUUP; IRQ: IRQ6; SDHI0: SD0CD; SDRAM: A6" - None - - 
      P504 H1 - SDRAM_A5 - - Disabled - - "BUS: A7; CEU: VIO_D3; GPT1: GTCPPO1; GPT_OPS: GTOULO; IRQ: IRQ7; SDHI0: SD0WP; SDRAM: A7" - None - - 
      P505 H3 - SDRAM_A6 - - Disabled - - "BUS: A8; CEU: VIO_D2; GPT2: GTCPPO2; GPT_OPS: GTOWUP; IRQ: IRQ8; SDHI0: SD0CLK; SDRAM: A8" - None - - 
      P506 J1 - SDRAM_A7 - - Disabled - - "BUS: A9; CEU: VIO_D1; GPT3: GTCPPO3; GPT_OPS: GTOWLO; IRQ: IRQ9; SDHI0: SD0CMD; SDRAM: A9" - None - - 
      P507 J2 - SDRAM_A8 - - Disabled - - "BUS: A10; CEU: VIO_D0; ESWM_GMII/MII: ET_TAS_STA0; ESWM_RGMII: ET_TAS_STA0; ESWM_RMII: ET_TAS_STA0; GLCDC: LCD_EXTCLK; GPT: GTADSM0; GPT0: GTIOC0A; IRQ: IRQ10; SCI7: CTS_RTS7; SCI7: DE7; SDRAM: A10" - None - - 
      P508 J3 - SDRAM_A9 - - Disabled - - "BUS: A11; CEU: VIO_VD; ESWM_GMII/MII: ET_TAS_STA1; ESWM_RGMII: ET_TAS_STA1; ESWM_RMII: ET_TAS_STA1; GPT: GTADSM1; GPT0: GTIOC0B; IRQ: IRQ1; SCI5: CTS5; SDRAM: A11" - None - - 
      P509 J4 - SDRAM_A10 - - Disabled - - "BUS: A12; CEU: VIO_HD; ESWM_GMII/MII: ET_TAS_STA2; ESWM_RGMII: ET_TAS_STA2; ESWM_RMII: ET_TAS_STA2; GPT1: GTIOC1A; IRQ: IRQ2; SCI5: CTS_RTS5; SCI5: DE5; SDRAM: A12; ULPT1: ULPTEVI1" - None - - 
      P510 K3 - SDRAM_A11 - - Disabled - - "BUS: A13; CEU: VIO_CLK; ESWM_GMII/MII: ET_TAS_STA3; ESWM_RGMII: ET_TAS_STA3; ESWM_RMII: ET_TAS_STA3; GPT1: GTIOC1B; IRQ: IRQ3; SCI5: RXD5; SDRAM: A13; ULPT0: ULPTEVI0" - None - - 
      P511 U15 - IIC_SYSTEM_SDA1 - - Disabled - - "CANFD1: CRX1; ESWM_GMII/MII: ET1_LINKSTA; ESWM_RGMII1: ET1_LINKSTA; ESWM_RMII1: ET1_LINKSTA; GPT0: GTIOC0B; IIC1: SDA1; IRQ: IRQ15; SCI8: CTS_RTS8; SCI8: DE8" - None - - 
      P512 P13 - IIC_SYSTEM_SCL1 - - Disabled - - "CANFD1: CTX1; ESWM_GMII/MII: ET1_INT; ESWM_RGMII1: ET1_INT; ESWM_RMII1: ET1_INT; GPT0: GTIOC0A; IIC1: SCL1; IRQ: IRQ14; SCI8: CTS8" - None - - 
      P513 R13 - LCD_TCON3 - - Disabled - - "ACMPHS: IVCMP0; ADC0: AN016; ADC1: AN016; CEU: VIO_FLD; ESWM_GMII/MII: ET0_INT; ESWM_RGMII0: ET0_INT; ESWM_RMII0: ET0_INT; GLCDC: LCD_TCON3; GPT13: GTIOC13B; IRQ: IRQ31; SCI8: DE8; SCI8: SCK8" - None - - 
      P514 R14 - ETH_RST - - Disabled - - "ESWM_GMII/MII: ET_TAS_STA1; ESWM_RGMII: ET_TAS_STA1; ESWM_RMII: ET_TAS_STA1; GLCDC: LCD_EXTCLK; GPT13: GTIOC13B; IIC2: SDA2; IRQ: IRQ13; SCI4: DE4; SCI4: SCK4" - None - - 
      P515 P15 - LCD_CLK - - Disabled - - "ESWM_GMII/MII: ET_TAS_STA0; ESWM_RGMII: ET_TAS_STA0; ESWM_RMII: ET_TAS_STA0; GLCDC: LCD_CLK; GPT13: GTIOC13A; IIC2: SCL2; IRQ: IRQ12; SCI4: CTS_RTS4; SCI4: DE4" - None - - 
      P600 P3 - USER_LED1_BLUE - - Disabled - - "CAC: CACREF; ESWM_GMII/MII: ET1_WOL; ESWM_RGMII1: ET1_WOL; ESWM_RMII1: ET1_WOL; GPT6: GTIOC6B; IRQ: IRQ30; OSPI0: OM_0_RSTO1; ULPT1: ULPTEVI1-DS" - None - - 
      P601 P4 - PMOD2_4_RSPCKB - - Disabled - - "GPT6: GTIOC6A; IRQ: IRQ29; OSPI0: OM_0_WP1; RTC: RTCOUT; SCI0: DE0; SCI0: SCK0; ULPT0: ULPTEVI0" - None - - 
      P602 P2 - PMOD2_3_MISOB_RXD0 - - Disabled - - "GPT7: GTIOC7B; IRQ: IRQ28; OSPI1: OM_1_SCLKN; SCI0: RXD0; ULPT0: ULPTEE0" - None - - 
      P603 P1 - PMOD2_2_MOSIB_TXD0 - - Disabled - - "GPT7: GTIOC7A; IRQ: IRQ27; OSPI1: OM_1_SCLK; SCI0: TXD0; ULPT0: ULPTO0" - None - - 
      P604 N2 - PMOD2_1_SSLB0_CTS_RTS0 - - Disabled - - "GPT8: GTIOC8B; IRQ: IRQ26; OSPI1: OM_1_SIO7; SCI0: CTS_RTS0; SCI0: DE0" - None - - 
      P605 N1 - PMOD2_1_CTS0 - - Disabled - - "GPT8: GTIOC8A; IRQ: IRQ25; OSPI1: OM_1_SIO1; SCI0: CTS0" - None - - 
      P606 N3 - LCD_RST - - Disabled - - "BUS: BC3; BUS: WR3; IRQ: IRQ24; OSPI1: OM_1_SIO6" - None - - 
      P607 M2 - SDRAM_DQ31 - - Disabled - - "BUS: D31; IRQ: IRQ23; OSPI1: OM_1_DQS; SDRAM: DQ31" - None - - 
      P608 K2 - SDRAM_A12 - - Disabled - - "BUS: A14; CAC: CACREF; CEU: VIO_FLD; GPT4: GTCPPO4; GPT_OPS: GTOWUP; IRQ: IRQ22; SCI5: TXD5; SDRAM: A14" - None - - 
      P609 A1 - SDRAM_DQ7 - - Disabled - - "ADC1(Digital): AD1FLAG1; BUS: D7; CANFD1: CTX1; GLCDC: LCD_DATA6; GPT5: GTIOC5B; GPT_OPS: GTIU; IRQ: IRQ29; SCI0: TXD0; SDRAM: DQ7; SPI0: MISO0; ULPT1: ULPTOA1-DS" - None - - 
      P610 D3 - SDRAM_DQ12 - - Disabled - - "BUS: D12; CANFD1: CRX1; GLCDC: LCD_DATA5; GPT4: GTIOC4A; GPT_OPS: GTOUUP; IRQ: IRQ16; SCI0: RXD0; SDRAM: DQ12; SPI0: RSPCK0; ULPT1: ULPTOB1-DS" - None - - 
      P611 D2 - SDRAM_DQ13 - - Disabled - - "BUS: D13; CAC: CACREF; CLKOUT: CLKOUT; GLCDC: LCD_DATA4; GPT4: GTIOC4B; GPT_OPS: GTOULO; IRQ: IRQ17; SCI0: DE0; SCI0: SCK0; SDRAM: DQ13; SPI0: MOSI0; USB HS: USBHS_VBUSEN" - None - - 
      P612 E4 - SDRAM_DQ14 - - Disabled - - "BUS: D14; GLCDC: LCD_DATA3; GPT9: GTIOC9A; IRQ: IRQ18; SCI0: CTS_RTS0; SCI0: DE0; SDRAM: DQ14; SPI0: SSLA0; USB HS: USBHS_OVRCURA" - None - - 
      P613 C2 - SDRAM_DQ15 - - Disabled - - "AGT1: AGTO1; BUS: D15; GLCDC: LCD_DATA2; GPT9: GTIOC9B; GPT_POEGA: GTETRGA; IRQ: IRQ19; SCI0: CTS0; SDRAM: DQ15; USB HS: USBHS_OVRCURB" - None - - 
      P614 E3 - SDRAM_DQM0 - - Disabled - - "AGT0: AGTO0; BUS: WR; BUS: WR0; GLCDC: LCD_DATA1; GPT9: GTCPPO9; GPT_POEGB: GTETRGB; IRQ: IRQ20; SCI7: RXD7; SDRAM: DQM0; USB HS: USBHS_ID" - None - - 
      P615 E2 - SDRAM_DQM2 - - Disabled - - "BUS: BC2; BUS: WR2; GLCDC: LCD_DATA0; GPT10: GTCPPO10; GPT_POEGC: GTETRGC; IRQ: IRQ7; SCI7: TXD7; SDRAM: DQM2; USB HS: USBHS_EXICEN" - None - - 
      P700 F12 - CAM_D4 - - Disabled - - "CEU: VIO_D4; ESWM_GMII/MII0: ET0_RXD2; ESWM_RGMII0: RGMII0_RXD2; GPT5: GTIOC5A; IRQ: IRQ16-DS; SCI2: RXD2; SDHI1: SD1WP; SPI0: MISO0; SSIE1: SSIDATA1" - None - - 
      P701 F15 - CAM_D5 - - Disabled - - "CEU: VIO_D5; ESWM_GMII/MII0: ET0_RXD1; ESWM_RGMII0: RGMII0_RXD1; ESWM_RMII0: RMII0_RXD1; GPT5: GTIOC5B; IRQ: IRQ17-DS; SCI2: CTS_RTS2; SCI2: DE2; SDHI1: SD1DAT4; SPI0: MOSI0; SSIE1: SSILRCK1; ULPT1: ULPTO1" - None - - 
      P702 F13 - CAM_D6 - - Disabled - - "CEU: VIO_D6; ESWM_GMII/MII0: ET0_RXD0; ESWM_RGMII0: RGMII0_RXD0; ESWM_RMII0: RMII0_RXD0; GPT6: GTIOC6A; IRQ: IRQ18-DS; SCI2: CTS2; SDHI1: SD1DAT5; SPI0: RSPCK0; SSIE1: SSIBCK1; ULPT0: ULPTO0" - None - - 
      P703 G14 - CAM_D7 - - Disabled - - "AGT1: AGTO1; CEU: VIO_D7; CMPOUT: VCOUT; ESWM_GMII/MII0: ET0_RX_CLK; ESWM_RGMII0: RGMII0_RXC; ESWM_RMII0: RMII0_REF50CK; GPT6: GTIOC6B; IRQ: IRQ19-DS; PDM0: PDMCLK0; SDHI1: SD1DAT6; SPI0: SSLA0" - None - - 
      P704 G13 - PMOD2_10_GPIO - - Disabled - - "AGT0: AGTO0; CANFD0: CTX0; CEU: VIO_D8; ESWM_GMII/MII0: ET0_RX_ER; ESWM_RMII0: RMII0_RX_ER; GPT: GTADSM0; GPT0: GTCPPO0; IRQ: IRQ26; PDM1: PDMCLK1; SDHI1: SD1DAT7; SPI0: SSLA1" - None - - 
      P705 F17 - CAM_D9 - - Disabled - - "AGT0: AGTIO0; CANFD0: CRX0; CEU: VIO_D9; ESWM_GMII/MII0: ET0_TX_EN; ESWM_RGMII0: RGMII0_TX_CTL; ESWM_RMII0: RMII0_TX_EN; GPT: GTADSM1; GPT1: GTCPPO1; IRQ: IRQ19; PDM2: PDMCLK2; SCI1: CTS1; SPI0: SSLA2" - None - - 
      P706 E17 - CAM_D10 - - Disabled - - "AGT0: AGTIO0; CEU: VIO_D10; ESWM_GMII/MII0: ET0_GTX_CLK; ESWM_RGMII0: RGMII0_TXC; ETHPHYCLK: ETHPHYCLK; GPT2: GTCPPO2; IRQ: IRQ7; PDM0: PDMDAT0; SCI1: RXD1; USB HS: USBHS_OVRCURB-DS" - None - - 
      P707 F16 - LCD_D18_CAM_D11 - - Disabled - - "CEU: VIO_D11; ESWM_GMII/MII0: ET0_TX_ER; ETHPHYCLK: ETHPHYCLK; GLCDC: LCD_DATA18; GPT3: GTCPPO3; IRQ: IRQ8; PDM1: PDMDAT1; SCI1: TXD1; USB HS: USBHS_OVRCURA-DS" - None - - 
      P708 N12 - LCD_BLEN - - Disabled - - "BUS: BC1; BUS: WR1; CAC: CACREF; CEU: VIO_VD; ESWM_GMII/MII: ET0_MDC; ESWM_RGMII0: ET0_MDC; ESWM_RMII0: ET0_MDC; GPT6: GTCPPO6; IIC2: SDA2; IRQ: IRQ11; SCI4: DE4; SCI4: SCK4; SPI1: MOSI1; SSIE: AUDIO_CLK" - None - - 
      P709 P16 - CAM_RST - - Disabled - - "BUS: CS4; CEU: VIO_D13; ESWM_GMII/MII: ET0_MDIO; ESWM_RGMII0: ET0_MDIO; ESWM_RMII0: ET0_MDIO; GPT5: GTCPPO5; IIC2: SCL2; IRQ: IRQ10; SCI4: CTS_RTS4; SCI4: DE4; SPI1: MISO1" - None - - 
      P710 M13 - LCD_EXTCLK - - Disabled - - "BUS: CS5; CEU: VIO_D12; ESWM_GMII/MII: ET0_LINKSTA; ESWM_RGMII0: ET0_LINKSTA; ESWM_RMII0: ET0_LINKSTA; GLCDC: LCD_EXTCLK; GPT11: GTIOC11B; IRQ: IRQ17; SCI4: CTS4; SPI1: SSLB3" - None - - 
      P711 N15 - LCD_D19 - - Disabled - - "AGT0: AGTEE0; ESWM_GMII/MII: GPTP0_PPS; ESWM_RGMII0: GPTP0_PPS; ESWM_RMII0: GPTP0_PPS; GLCDC: LCD_DATA19; GPT11: GTIOC11A; IRQ: IRQ3; SCI1: CTS_RTS1; SCI1: DE1; SPI1: SSLB2" - None - - 
      P712 N13 - LCD_D20 - - Disabled - - "AGT0: AGTOB0; ESWM_GMII/MII: GPTP1_CAPTURE; ESWM_RGMII1: GPTP1_CAPTURE; ESWM_RMII1: GPTP1_CAPTURE; GLCDC: LCD_DATA20; GPT2: GTIOC2B; IRQ: IRQ2; SCI1: CTS1; SPI1: SSLB1" - None - - 
      P713 N16 - LCD_D21 - - Disabled - - "AGT0: AGTOA0; ESWM_GMII/MII: GPTP1_MATCH; ESWM_RGMII1: GPTP1_MATCH; ESWM_RMII1: GPTP1_MATCH; GLCDC: LCD_DATA21; GPT2: GTIOC2A; IRQ: IRQ14; SCI4: CTS4" - None - - 
      P714 N14 - LCD_D22 - - Disabled - - "ESWM_GMII/MII: GPTP1_PPS; ESWM_RGMII1: GPTP1_PPS; ESWM_RMII1: GPTP1_PPS; GLCDC: LCD_DATA22; GPT12: GTIOC12B; IRQ: IRQ13; MIPI: DSI_TE; SCI4: TXD4" - None - - 
      P715 T15 - LCD_D23 - - Disabled - - "ESWM_GMII/MII: ET_TAS_STA2; ESWM_RGMII: ET_TAS_STA2; ESWM_RMII: ET_TAS_STA2; GLCDC: LCD_DATA23; GPT12: GTIOC12A; IRQ: IRQ12; SCI4: RXD4" - None - - 
      P800 T6 - OSPI_DQ5_PMOD1_1_CTS2 - - Disabled - - "AGT0: AGTOA0; GPT11: GTIOC11A; GPT_OPS: GTIU; IRQ: IRQ11; OSPI0: OM_0_SIO5; SCI2: CTS2" - None - - 
      P801 P6 - OSPI_DS L None Disabled - - "AGT0: AGTOB0; ESWM_GMII/MII: GPTP1_PPS; ESWM_RGMII1: GPTP1_PPS; ESWM_RMII1: GPTP1_PPS; GPT11: GTIOC11B; GPT_OPS: GTIV; IRQ: IRQ12; OSPI0: OM_0_DQS; SCI2: TXD2" - O - - 
      P802 R6 - OSPI_DQ6 - - Disabled - - "GPT12: GTIOC12A; GPT_OPS: GTIW; IRQ: IRQ18; OSPI0: OM_0_SIO6; SCI2: RXD2" - None - - 
      P803 P7 - OSPI_DQ1 - - Disabled - - "GPT12: GTIOC12B; GPT_POEGC: GTETRGC; IRQ: IRQ19; OSPI0: OM_0_SIO1; SCI2: DE2; SCI2: SCK2" - None - - 
      P804 R7 - OSPI_DQ7 - - Disabled - - "GPT13: GTIOC13A; GPT_POEGD: GTETRGD; IRQ: IRQ14; MIPI: DSI_TE; OSPI0: OM_0_SIO7; SCI2: CTS_RTS2; SCI2: DE2" - None - - 
      P805 P12 - LCD_HSYNC_TCON1 - - Disabled - - "ACMPHS: IVCMP0; ADC0: AN017; ADC1: AN017; CEU: VIO_D15; ESWM_GMII/MII: ET1_MDIO; ESWM_RGMII1: ET1_MDIO; ESWM_RMII1: ET1_MDIO; GLCDC: LCD_TCON1; IRQ: IRQ30; SCI8: TXD8" - None - - 
      P806 T14 - LCD_VSYNC_TCON0 - - Disabled - - "ADC0: AN018; ADC1: AN018; CEU: VIO_D14; ESWM_GMII/MII: ET1_MDC; ESWM_RGMII1: ET1_MDC; ESWM_RMII1: ET1_MDC; GLCDC: LCD_TCON0; IRQ: IRQ0; SCI8: RXD8" - None - - 
      P807 N11 - LCD_DE_TCON2 - - Disabled - - "GLCDC: LCD_TCON2; GPT13: GTIOC13A; IRQ: IRQ11" - None - - 
      P808 U5 - OSPI_SCLK_ARDUINO_D0_RXD_MIKROBUS_RXD - - Disabled - - "GPT13: GTIOC13B; IRQ: IRQ15; OSPI0: OM_0_SCLK; SCI7: RXD7" - None - - 
      P809 T5 - ARDUINO_D1_TXD_MIKROBUS_TXD - - Disabled - - "IRQ: IRQ20; OSPI0: OM_0_SCLKN; SCI7: TXD7" - None - - 
      P810 M9 - ARDUINO_D4_MIKROBUS_1_PWM - - Disabled - - "GPT10: GTIOC10A; IRQ: IRQ21; PDM0: PDMCLK0; SCI7: DE7; SCI7: SCK7; SDHI1: SD1DAT2; ULPT0: ULPTOA0" - None - - 
      P811 N8 - ARDUINO_D3 - - Disabled - - "GPT10: GTIOC10B; IRQ: IRQ22; PDM1: PDMCLK1; SCI7: CTS7; SDHI1: SD1DAT3; ULPT0: ULPTOB0; USB FS: USB_ID" - None - - 
      P812 P8 - MEMS_MIC_CLK L None Disabled - - "ADC0: AN022; ADC1: AN022; GPT11: GTIOC11A; IRQ: IRQ23; PDM2: PDMCLK2; SCI7: CTS_RTS7; SCI7: DE7; SDHI1: SD1DAT4; USB FS: USB_EXICEN" - O - - 
      P813 B1 - SDRAM_CS - - Disabled - - "CEU: VIO_D13; GPT7: GTIOC7B; GPT_POEGA: GTETRGA; IRQ: IRQ15; PDM2: PDMCLK2; SCI7: DE7; SCI7: SCK7; SDRAM: SDCS" - None - - 
      P814 U16 - USBFS_DP - - Disabled - - "CANFD0: CRX0; GPT8: GTIOC8B; IRQ: IRQ16; USB FS: USB_DP" - None - - 
      P815 T16 - USBFS_DN - - Disabled - - "CANFD0: CTX0; GPT8: GTIOC8A; IRQ: IRQ15; USB FS: USB_DM" - None - - 
      P902 E9 - CAM_D1_LCD_D3 - - Disabled - - "BUS: ALE; CEU: VIO_D1; ETHPHYCLK: ETHPHYCLK; GLCDC: LCD_DATA3; GPT13: GTCPPO13; IRQ: IRQ0; SSIE: AUDIO_CLK" - None - - 
      P903 D9 - LCD_D2 - - Disabled - - "GLCDC: LCD_DATA2; GPT11: GTIOC11A; IRQ: IRQ1" - None - - 
      P904 A16 - LCD_D8 - - Disabled - - "ESWM_GMII/MII1: ET1_RXD4; GLCDC: LCD_DATA8; GPT11: GTIOC11B; IRQ: IRQ2" - None - - 
      P905 A14 - ETH_RX_CLK - - Disabled - - "ADC1(Digital): AD1FLAG1; CEU: VIO_D6; ESWM_GMII/MII1: ET1_RX_CLK; ESWM_RGMII1: RGMII1_RXC; ESWM_RMII1: RMII1_REF50CK; GLCDC: LCD_DATA19; GPT13: GTCPPO13; IRQ: IRQ8; PDM1: PDMDAT1; SCI3: RXD3" - None - - 
      P906 A13 - ETH_RXD0 - - Disabled - - "ADC0(Digital): AD0FLAG1; CEU: VIO_D5; ESWM_GMII/MII1: ET1_RXD0; ESWM_RGMII1: RGMII1_RXD0; ESWM_RMII1: RMII1_RXD0; GLCDC: LCD_DATA20; GPT13: GTIOC13B; IRQ: IRQ9; PDM0: PDMDAT0; SCI6: CTS6; SSIE1: SSILRCK1; ULPT1: ULPTO1; USB FS: USB_ID" - None - - 
      P907 A15 - ETH_RXD1 - - Disabled - - "ADC(Digital): ADSYNC; CEU: VIO_D4; ESWM_GMII/MII1: ET1_RXD1; ESWM_RGMII1: RGMII1_RXD1; ESWM_RMII1: RMII1_RXD1; GLCDC: LCD_DATA21; GPT13: GTIOC13A; IRQ: IRQ10; PDM2: PDMCLK2; SCI6: DE6; SCI6: SCK6; SSIE1: SSIBCK1; ULPT1: ULPTEE1; USB FS: USB_EXICEN" - None - - 
      P908 B13 - ETH_RXD2 - - Disabled - - "ADC1(Digital): ADST1; CANFD1: CRX1; CEU: VIO_D3; ESWM_GMII/MII1: ET1_RXD2; ESWM_RGMII1: RGMII1_RXD2; GLCDC: LCD_DATA22; GPT12: GTIOC12B; IRQ: IRQ11; PDM1: PDMCLK1; SCI6: TXD6; ULPT1: ULPTEVI1; USB FS: USB_OVRCURB; USB HS: USBHS_ID" - None - - 
      P909 B14 - ETH_RXD3 - - Disabled - - "ADC0(Digital): ADST0; CANFD1: CTX1; CEU: VIO_D2; ESWM_GMII/MII1: ET1_RXD3; ESWM_RGMII1: RGMII1_RXD3; GLCDC: LCD_DATA23; GPT12: GTIOC12A; IRQ: IRQ21-DS; PDM0: PDMCLK0; SCI6: RXD6; ULPT1: ULPTOA1; USB FS: USB_OVRCURA; USB HS: USBHS_EXICEN" - None - - 
      P910 E11 - LCD_D4 - - Disabled - - "ESWM_GMII/MII1: ET1_TXD4; GLCDC: LCD_DATA4; GPT12: GTCPPO12; IRQ: IRQ7" - None - - 
      P911 C12 - LCD_D5 - - Disabled - - "ESWM_GMII/MII1: ET1_TXD5; GLCDC: LCD_DATA5; GPT3: GTIOC3B; IRQ: IRQ6" - None - - 
      P912 D12 - LCD_D6 - - Disabled - - "ESWM_GMII/MII1: ET1_TXD6; GLCDC: LCD_DATA6; GPT3: GTIOC3A; IRQ: IRQ5" - None - - 
      P913 E12 - LCD_D7 - - Disabled - - "CLKOUT: CLKOUT; ESWM_GMII/MII1: ET1_TXD7; GLCDC: LCD_DATA7; GPT11: GTCPPO11; IRQ: IRQ3" - None - - 
      P914 E5 - LCD_D0 - - Disabled - - "GLCDC: LCD_DATA0; GPT5: GTIOC5B; IRQ: IRQ9; SCI6: CTS_RTS6; SCI6: DE6" - None - - 
      P915 A6 - LCD_D1 - - Disabled - - "GLCDC: LCD_DATA1; GPT5: GTIOC5A; IRQ: IRQ8; SCI6: CTS6" - None - - 
      PA00 G1 - SDRAM_A3 - - Disabled - - "ADC1(Digital): AD1FLAG1; BUS: A5; CEU: VIO_D5; GLCDC: LCD_CLK; GPT7: GTCPPO7; GPT_OPS: GTOVLO; IRQ: IRQ22; SCI5: CTS_RTS5; SCI5: DE5; SDHI0: SD0DAT7; SDRAM: A5" - None - - 
      PA01 H4 - SDRAM_A2 - - Disabled - - "ADC0(Digital): AD0FLAG1; BUS: A4; CEU: VIO_D6; GLCDC: LCD_TCON0; GPT8: GTCPPO8; GPT_OPS: GTOVUP; IRQ: IRQ21; SCI5: CTS5; SDHI0: SD0DAT6; SDRAM: A4" - None - - 
      PA02 F1 - SDRAM_A1 L None Disabled - - "ADC(Digital): ADSYNC; BUS: A3; CEU: VIO_D7; GPT9: GTCPPO9; GPT_OPS: GTIW; IRQ: IRQ31; SCI2: RXD2; SDHI0: SD0DAT5; SDRAM: A3" - I - - 
      PA03 G2 - SDRAM_A0 - - Disabled - - "ADC1(Digital): ADST1; BUS: A2; CEU: VIO_D8; GPT10: GTCPPO10; GPT_OPS: GTIV; IRQ: IRQ20; SCI2: TXD2; SDHI0: SD0DAT4; SDRAM: A2" - None - - 
      PA04 D1 - SDRAM_DQM3 - - Disabled - - "ADC0(Digital): ADST0; BUS: A1; CEU: VIO_D9; GPT4: GTIOC4B; GPT_OPS: GTIU; IRQ: IRQ19; SCI2: DE2; SCI2: SCK2; SDHI0: SD0DAT3; SDRAM: A1; SDRAM: DQM3" - None - - 
      PA05 G3 - SDRAM_DQM1 - - Disabled - - "BUS: A0; BUS: BC0; CEU: VIO_D10; GPT4: GTIOC4A; GPT_POEGD: GTETRGD; IRQ: IRQ18; PDM2: PDMDAT2; SCI2: CTS_RTS2; SCI2: DE2; SDHI0: SD0DAT2; SDRAM: A0; SDRAM: DQM1" - None - - 
      PA06 C1 - SDRAM_CKE - - Disabled - - "BUS: CS1; CEU: VIO_D11; GPT7: GTIOC7B; GPT_POEGC: GTETRGC; IRQ: IRQ17; PDM1: PDMDAT1; SCI2: CTS2; SDHI0: SD0DAT1; SDRAM: CKE" - None - - 
      PA07 G4 - USER_LED3_RED - - Disabled - - "BUS: RD; CEU: VIO_D12; CMPOUT: VCOUT; GPT7: GTIOC7A; GPT_POEGB: GTETRGB; IRQ: IRQ16; PDM0: PDMDAT0; SCI7: CTS7; SDHI0: SD0DAT0" - None - - 
      PA08 F3 - SDRAM_WE - - Disabled - - "BUS: CS0; GLCDC: LCD_TCON3; GPT11: GTCPPO11; GPT_POEGD: GTETRGD; IRQ: IRQ6; SCI5: RXD5; SDRAM: WE" - None - - 
      PA09 F4 - SDRAM_CAS - - Disabled - - "BUS: CS3; GLCDC: LCD_TCON2; GPT12: GTCPPO12; IRQ: IRQ5; SCI5: TXD5; SDRAM: CAS" - None - - 
      PA10 F2 - SDRAM_RAS - - Disabled - - "BUS: CS2; CEU: VIO_D15; GLCDC: LCD_TCON1; GPT13: GTCPPO13; IRQ: IRQ4; PDM0: PDMCLK0; SCI5: DE5; SCI5: SCK5; SDRAM: RAS" - None - - 
      PA11 B4 - SDRAM_DQ8 - - Disabled - - "BUS: D8; GPT6: GTIOC6A; GPT_OPS: GTIV; IRQ: IRQ10; SCI9: DE9; SCI9: SCK9; SDRAM: DQ8" - None - - 
      PA12 B2 - SDRAM_DQ9 - - Disabled - - "BUS: D9; GPT6: GTIOC6B; GPT_OPS: GTIW; IRQ: IRQ11; SCI9: RXD9; SDRAM: DQ9" - None - - 
      PA13 C3 - SDRAM_DQ10 - - Disabled - - "BUS: D10; GPT10: GTIOC10A; GPT_OPS: GTOVUP; IRQ: IRQ12; SCI9: CTS_RTS9; SCI9: DE9; SDRAM: DQ10" - None - - 
      PA14 D4 - SDRAM_DQ11 - - Disabled - - "BUS: D11; GPT10: GTIOC10B; GPT_OPS: GTOVLO; IRQ: IRQ13; SCI9: TXD9; SDRAM: DQ11" - None - - 
      PA15 E1 - SDRAM_CLK - - Disabled - - "BUS: EBCLK; CEU: VIO_D14; GPT7: GTIOC7A; IRQ: IRQ14; PDM1: PDMCLK1; SCI9: CTS9; SDRAM: SDCLK" - None - - 
      PB00 E16 - LCD_D17 - - Disabled - - "ADC0(Digital): ADST0; ESWM_GMII/MII0: ET0_TXD0; ESWM_RGMII0: RGMII0_TXD0; ESWM_RMII0: RMII0_TXD0; GLCDC: LCD_DATA17; GPT4: GTCPPO4; IRQ: IRQ10; PDM2: PDMDAT2; SCI1: DE1; SCI1: SCK1; USB HS: USBHS_VBUSEN" - None - - 
      PB01 D17 - LCD_D13 - - Disabled - - "ADC1(Digital): AD1FLAG1; BUS: ALE; CEU: VIO_FLD; ESWM_GMII/MII0: ET0_TX_CLK; GLCDC: LCD_DATA13; GPT2: GTCPPO2; IRQ: IRQ12; SCI1: CTS_RTS1; SCI1: DE1" - None - - 
      PB02 E13 - CAM_VSYNC_LCD_D16 - - Disabled - - "ADC1(Digital): ADST1; CEU: VIO_VD; ESWM_GMII/MII0: ET0_TXD1; ESWM_RGMII0: RGMII0_TXD1; ESWM_RMII0: RMII0_TXD1; GLCDC: LCD_DATA16; GPT0: GTCPPO0; IRQ: IRQ11; SCI5: RXD5" - None - - 
      PB03 D16 - CAM_HSYNC_LCD_D15 - - Disabled - - "ADC(Digital): ADSYNC; CEU: VIO_HD; ESWM_GMII/MII0: ET0_TXD2; ESWM_RGMII0: RGMII0_TXD2; GLCDC: LCD_DATA15; GPT1: GTCPPO1; IRQ: IRQ13; SCI5: TXD5" - None - - 
      PB04 D13 - CAM_PCLK_LCD_D14 - - Disabled - - "ADC0(Digital): AD0FLAG1; CEU: VIO_CLK; ESWM_GMII/MII0: ET0_TXD3; ESWM_RGMII0: RGMII0_TXD3; GLCDC: LCD_DATA14; GPT3: GTCPPO3; IRQ: IRQ9; SCI5: DE5; SCI5: SCK5" - None - - 
      PB05 D15 - LCD_D12 - - Disabled - - "ESWM_GMII/MII0: ET0_TXD7; GLCDC: LCD_DATA12; GPT4: GTCPPO4; IRQ: IRQ15; SCI5: CTS5" - None - - 
      PB06 E14 - LCD_D11 - - Disabled - - "ESWM_GMII/MII0: ET0_TXD6; GLCDC: LCD_DATA11; GPT9: GTIOC9A; IRQ: IRQ0; SCI5: CTS_RTS5; SCI5: DE5" - None - - 
      PB07 D14 - LCD_D10 - - Disabled - - "ESWM_GMII/MII0: ET0_TXD5; GLCDC: LCD_DATA10; GPT9: GTIOC9B; IRQ: IRQ1" - None - - 
      PC00 M1 - SDRAM_DQ30 - - Disabled - - "BUS: D30; GPT7: GTCPPO7; IRQ: IRQ28; OSPI1: OM_1_SIO5; SCI7: CTS_RTS7; SCI7: DE7; SDRAM: DQ30" - None - - 
      PC01 M3 - SDRAM_DQ29 - - Disabled - - "BUS: D29; GPT6: GTCPPO6; IRQ: IRQ27; OSPI1: OM_1_SIO0; SCI7: CTS7; SDRAM: DQ29" - None - - 
      PC02 L2 - SDRAM_DQ28 - - Disabled - - "BUS: D28; GPT5: GTCPPO5; IRQ: IRQ26; OSPI1: OM_1_SIO3; SCI7: DE7; SCI7: SCK7; SDRAM: DQ28" - None - - 
      PC03 L1 - SDRAM_DQ27 - - Disabled - - "BUS: D27; GPT4: GTCPPO4; IRQ: IRQ25; OSPI1: OM_1_SIO4; SCI7: TXD7; SDRAM: DQ27" - None - - 
      PC04 L3 - SDRAM_DQ26 - - Disabled - - "BUS: D26; GPT3: GTCPPO3; IRQ: IRQ24; OSPI1: OM_1_SIO2; SCI7: RXD7; SDRAM: DQ26" - None - - 
      PC05 L5 - SDRAM_DQ25 - - Disabled - - "BUS: D25; GPT2: GTCPPO2; IRQ: IRQ23; OSPI1: OM_1_CS1; SDRAM: DQ25" - None - - 
      PC06 N4 - SDRAM_DQ24 - - Disabled - - "BUS: D24; GPT1: GTCPPO1; IRQ: IRQ22; OSPI1: OM_1_ECSINT1; SDRAM: DQ24" - None - - 
      PC07 K5 - SDRAM_DQ23 - - Disabled - - "BUS: D23; GPT0: GTCPPO0; IRQ: IRQ21; OSPI1: OM_1_RESET; SDRAM: DQ23" - None - - 
      PC08 M4 - SDRAM_DQ22 - - Disabled - - "BUS: D22; GPT8: GTCPPO8; IRQ: IRQ29; OSPI1: OM_1_CS0; SDRAM: DQ22" - None - - 
      PC09 L4 - SDRAM_DQ21 - - Disabled - - "BUS: D21; IRQ: IRQ5; OSPI1: OM_1_RSTO1; SDRAM: DQ21" - None - - 
      PC10 M5 - SDRAM_DQ20 - - Disabled - - "BUS: D20; GPT13: GTCPPO13; IRQ: IRQ4; OSPI1: OM_1_WP1; SDRAM: DQ20" - None - - 
      PC11 H5 - SDRAM_DQ19 - - Disabled - - "BUS: D19; ESWM_GMII/MII: ET0_MDC; ESWM_RGMII0: ET0_MDC; ESWM_RMII0: ET0_MDC; GPT12: GTCPPO12; IRQ: IRQ3; SCI6: CTS_RTS6; SCI6: DE6; SDRAM: DQ19" - None - - 
      PC12 G5 - SDRAM_DQ18 - - Disabled - - "BUS: D18; ESWM_GMII/MII: ET0_MDIO; ESWM_RGMII0: ET0_MDIO; ESWM_RMII0: ET0_MDIO; GPT11: GTCPPO11; IRQ: IRQ2; SCI6: DE6; SCI6: SCK6; SDRAM: DQ18" - None - - 
      PC13 J5 - SDRAM_DQ17 - - Disabled - - "BUS: D17; ESWM_GMII/MII: ET0_INT; ESWM_RGMII0: ET0_INT; ESWM_RMII0: ET0_INT; GPT10: GTCPPO10; IRQ: IRQ1; SCI6: RXD6; SDRAM: DQ17" - None - - 
      PC14 F5 - SDRAM_DQ16 - - Disabled - - "BUS: D16; ESWM_GMII/MII: ET0_WOL; ESWM_RGMII0: ET0_WOL; ESWM_RMII0: ET0_WOL; GPT: GTADSM1; GPT9: GTCPPO9; IRQ: IRQ0; SCI6: TXD6; SDRAM: DQ16" - None - - 
      PC15 K1 - SDRAM_BA1 - - Disabled - - "BUS: A16; CANFD1: CRX1; GPT: GTADSM0; IRQ: IRQ30; SCI6: CTS6; SDRAM: A16" - None - - 
      PD00 K4 - SDRAM_BA0 - - Disabled - - "BUS: A15; CANFD1: CTX1; GPT5: GTCPPO5; GPT_OPS: GTOWLO; IRQ: IRQ23; SCI5: DE5; SCI5: SCK5; SDRAM: A15" - None - - 
      PD01 B16 - ARDUINO_D8_MIKROBUS_INT - - Disabled - - "ESWM_GMII/MII1: ET1_RXD6; GPT2: GTCPPO2; IRQ: IRQ22; SCI8: DE8; SCI8: SCK8; SDHI0: SD0DAT2" - None - - 
      PD02 B17 - JLINK_VCOM_TX L None Disabled - - "ESWM_GMII/MII1: ET1_RXD7; GPT1: GTCPPO1; IRQ: IRQ21; SCI8: TXD8; SDHI0: SD0DAT1" - O - - 
      PD03 C15 - JLINK_VCOM_RXD L None Disabled - - "ESWM_GMII/MII0: ET0_RXD4; GPT3: GTIOC3B; IRQ: IRQ21; SCI8: RXD8; SDHI0: SD0DAT0; USB HS: USBHS_EXICEN" - I - - 
      PD04 C14 - JLINK_VCOM_CTS_RTS - - Disabled - - "ESWM_GMII/MII0: ET0_RXD5; GPT3: GTIOC3A; IRQ: IRQ20; SCI8: CTS_RTS8; SCI8: DE8; SDHI0: SD0CMD; USB HS: USBHS_ID" - None - - 
      PD05 C16 - JLINK_VCOM_CTS - - Disabled - - "ESWM_GMII/MII0: ET0_RXD6; GPT2: GTIOC2B; IRQ: IRQ19; SCI8: CTS8; SDHI0: SD0CLK; USB HS: USBHS_OVRCURB" - None - - 
      PD06 C17 - AUDIO_MCLK - - Disabled - - "ESWM_GMII/MII0: ET0_RXD7; GPT2: GTIOC2A; IRQ: IRQ18; SDHI0: SD0WP; USB HS: USBHS_OVRCURA" - None - - 
      PD07 E15 - USB_HS_VBUS_SEL - - Disabled - - "ESWM_GMII/MII0: ET0_TXD4; GPT0: GTCPPO0; IRQ: IRQ17; SDHI0: SD0CD; USB HS: USBHS_VBUSEN" - None - - 
      RES D5 CGC_RES - - - - - - - - IO "Read only" - 
      USBHS_DM H17 CGC_USBHS_DM - - - - - - - - IO "Read only" - 
      USBHS_DP H16 CGC_USBHS_DP - - - - - - - - IO "Read only" - 
      USBHS_RREF J15 CGC_USBHS_RREF - - - - - - - - IO "Read only" - 
      VBATT M16 CGC_VBATT - - - - - - - - IO "Read only" - 
      VCC H11 CGC_VCC - - - - - - - - IO "Read only" - 
      VCC H14 CGC_VCC - - - - - - - - IO "Read only" - 
      VCC G11 CGC_VCC - - - - - - - - IO "Read only" - 
      VCC G16 CGC_VCC - - - - - - - - IO "Read only" - 
      VCC F6 CGC_VCC - - - - - - - - IO "Read only" - 
      VCC G6 CGC_VCC - - - - - - - - IO "Read only" - 
      VCC F11 CGC_VCC - - - - - - - - IO "Read only" - 
      VCC H6 CGC_VCC - - - - - - - - IO "Read only" - 
      VCC L15 CGC_VCC - - - - - - - - IO "Read only" - 
      VCC K14 CGC_VCC - - - - - - - - IO "Read only" - 
      VCC18_MIPI R2 CGC_VCC18_MIPI - - - - - - - - IO "Read only" - 
      VCC2 R1 CGC_VCC2 - - - - - - - - IO "Read only" - 
      VCC2 J6 CGC_VCC2 - - - - - - - - IO "Read only" - 
      VCC2 L6 CGC_VCC2 - - - - - - - - IO "Read only" - 
      VCC2 M7 CGC_VCC2 - - - - - - - - IO "Read only" - 
      VCC2 M8 CGC_VCC2 - - - - - - - - IO "Read only" - 
      VCC_DCDC A10 CGC_VCC_DCDC - - - - - - - - IO "Read only" - 
      VCC_DCDC A11 CGC_VCC_DCDC - - - - - - - - IO "Read only" - 
      VCC_DCDC B10 CGC_VCC_DCDC - - - - - - - - IO "Read only" - 
      VCC_DCDC B11 CGC_VCC_DCDC - - - - - - - - IO "Read only" - 
      VCC_USB U17 CGC_VCC_USB - - - - - - - - IO "Read only" - 
      VCC_USBHS H15 CGC_VCC_USBHS - - - - - - - - IO "Read only" - 
      VCL F9 CGC_VCL - - - - - - - - IO "Read only" - 
      VCL G9 CGC_VCL - - - - - - - - IO "Read only" - 
      VCL H9 CGC_VCL - - - - - - - - IO "Read only" - 
      VCL M11 CGC_VCL - - - - - - - - IO "Read only" - 
      VCL J8 CGC_VCL - - - - - - - - IO "Read only" - 
      VCL J9 CGC_VCL - - - - - - - - IO "Read only" - 
      VCL K8 CGC_VCL - - - - - - - - IO "Read only" - 
      VCL K9 CGC_VCL - - - - - - - - IO "Read only" - 
      VCL L10 CGC_VCL - - - - - - - - IO "Read only" - 
      VCL L11 CGC_VCL - - - - - - - - IO "Read only" - 
      VCL K11 CGC_VCL - - - - - - - - IO "Read only" - 
      VCL J11 CGC_VCL - - - - - - - - IO "Read only" - 
      VLO A7 CGC_VLO - - - - - - - - IO "Read only" - 
      VLO A8 CGC_VLO - - - - - - - - IO "Read only" - 
      VLO B7 CGC_VLO - - - - - - - - IO "Read only" - 
      VLO B8 CGC_VLO - - - - - - - - IO "Read only" - 
      VREFH U9 CGC_VREFH - - - - - - - - IO "Read only" - 
      VREFH0 U10 CGC_VREFH0 - - - - - - - - IO "Read only" - 
      VREFL T9 CGC_VREFL - - - - - - - - IO "Read only" - 
      VREFL0 T10 CGC_VREFL0 - - - - - - - - IO "Read only" - 
      VSS A9 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS B9 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS H10 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS H12 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS U4 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS G10 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS G15 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS G17 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS F7 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS F8 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS G7 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS G8 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS F10 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS H7 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS H8 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS M10 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS J7 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS M17 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS K6 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS K7 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS L7 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS L8 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS L12 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS L9 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS K10 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS K12 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS J10 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS J12 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS J14 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS1_USBHS J17 CGC_VSS1_USBHS - - - - - - - - IO "Read only" - 
      VSS2_USBHS J16 CGC_VSS2_USBHS - - - - - - - - IO "Read only" - 
      VSS_MIPI R3 CGC_VSS_MIPI - - - - - - - - IO "Read only" - 
      VSS_USB T17 CGC_VSS_USB - - - - - - - - IO "Read only" - 
    RA8P1 WSB EK -> 
      AVCC0 R9 CGC_AVCC0 - - - - - - - - IO "Read only" - 
      AVCC_MIPI T4 CGC_AVCC_MIPI - - - - - - - - IO "Read only" - 
      AVCC_USBHS K15 CGC_AVCC_USBHS - - - - - - - - IO "Read only" - 
      AVSS0 R10 CGC_AVSS0 - - - - - - - - IO "Read only" - 
      MIPI_CLN U2 CGC_MIPI_CLN - - - - - - - - IO "Read only" - 
      MIPI_CLP T2 CGC_MIPI_CLP - - - - - - - - IO "Read only" - 
      MIPI_DL0N U1 CGC_MIPI_DL0N - - - - - - - - IO "Read only" - 
      MIPI_DL0P T1 CGC_MIPI_DL0P - - - - - - - - IO "Read only" - 
      MIPI_DL1N U3 CGC_MIPI_DL1N - - - - - - - - IO "Read only" - 
      MIPI_DL1P T3 CGC_MIPI_DL1P - - - - - - - - IO "Read only" - 
      P000 U13 GPIO S4_INT - - "Input mode" - - "ACMPHS: IVCMP2; ADC0: AN000; IRQ: IRQ6-DS" - None - - 
      P001 T13 - ARDUINO_A0 - - Disabled - - "ACMPHS: IVCMP3; ADC0: AN001; IRQ: IRQ7-DS" - None - - 
      P002 U14 - GROVE2_2_AN - - Disabled - - "ACMPHS: IVCMP2; ADC0: AN002; IRQ: IRQ8-DS" - None - - 
      P003 R12 - ARDUINO_A2 - - Disabled - - "ACMPHS: IVCMP3; ADC0: AN003; IRQ: IRQ29" - None - - 
      P004 T11 - ARDUINO_A3_MIKROBUS_AN - - Disabled - - "ACMPHS: IVCMP2; ADC0: AN004; IRQ: IRQ9-DS" - None - - 
      P005 R11 - GROVE2_1_AN - - Disabled - - "ACMPHS: IVCMP3; ADC0: AN005; IRQ: IRQ10-DS" - None - - 
      P006 U12 - PMOD1_7_INT - - Disabled - - "ACMPHS: IVCMP2; ADC1: AN006; IRQ: IRQ11-DS" - None - - 
      P007 T12 - ARDUINO_A1 - - Disabled - - "ACMPHS: IVCMP3; ADC1: AN007; IRQ: IRQ28" - None - - 
      P008 U11 - USER_S2 - - Disabled - - "ACMPHS: IVREF0; ADC1: AN008; IRQ: IRQ12-DS" - None - - 
      P009 P11 - USER_S1 - - Disabled - - "ACMPHS: IVREF1; ADC1: AN009; IRQ: IRQ13-DS" - None - - 
      P010 P10 - CAM_INT - - Disabled - - "ADC1: AN010; IRQ: IRQ14" - None - - 
      P011 N10 - ARDUINO_D2 - - Disabled - - "ADC1: AN011; IRQ: IRQ16" - None - - 
      P012 P9 - PMOD2_7_IRQ15 - - Disabled - - "ADC0: AN012; IRQ: IRQ15" - None - - 
      P013 N9 - I2C_SCL0_PULLUP - - Disabled - - "ADC1: AN013; IRQ: IRQ14" - None - - 
      P014 T8 - ARDUINO_A4 - - Disabled - - "ACMPHS: IVCMP0; ADC0: AN014; DAC120: DA0; IRQ: IRQ27" - None - - 
      P015 U8 - ARDUINO_A5 - - Disabled - - "ACMPHS: IVCMP0; ADC1: AN015; DAC121: DA1; IRQ: IRQ13" - None - - 
      P100 U6 - OSPI_DQ0_ARDUINO_D12_MISOB_MIKROBUS_MISOB - - Disabled - - "AGT0: AGTIO0; ESWM_GMII/MII: GPTP1_MATCH; ESWM_RGMII1: GPTP1_MATCH; ESWM_RMII1: GPTP1_MATCH; GPT8: GTIOC8B; GPT_POEGA: GTETRGA; IRQ: IRQ2; OSPI0: OM_0_SIO0; SCI9: DE9; SCI9: SCK9; SPI1: MISO1" - None - - 
      P101 R5 - OSPI_DQ3_ARDUINO_D11_MOSIB_MIKROBUS_MOSIB - - Disabled - - "AGT0: AGTEE0; ESWM_GMII/MII: GPTP1_CAPTURE; ESWM_RGMII1: GPTP1_CAPTURE; ESWM_RMII1: GPTP1_CAPTURE; GPT8: GTIOC8A; GPT_POEGB: GTETRGB; IRQ: IRQ1; OSPI0: OM_0_SIO3; SCI9: RXD9; SPI1: MOSI1" - None - - 
      P102 P5 - OSPI_DQ4_ARDUINO_D13_RSPCKB_MIKROBUS_RSPCKB - - Disabled - - "ADC0(Digital): ADTRG0; AGT0: AGTO0; CANFD0: CRX0; GPT2: GTIOC2B; GPT_OPS: GTOWLO; IRQ: IRQ17; OSPI0: OM_0_SIO4; SCI9: TXD9; SPI1: RSPCK1" - None - - 
      P103 R4 - OSPI_DQ2_ARDUINO_D10_SSLB_MIKROBUS_SSLB - - Disabled - - "ADC1(Digital): AD1FLAG1; CANFD0: CTX0; ESWM_GMII/MII: GPTP0_PPS; ESWM_RGMII0: GPTP0_PPS; ESWM_RMII0: GPTP0_PPS; GPT2: GTIOC2A; GPT_OPS: GTOWUP; IRQ: IRQ16; OSPI0: OM_0_SIO2; SCI9: CTS_RTS9; SCI9: DE9; SPI1: SSLB0" - None - - 
      P104 M6 - OSPI_CS_ARDUINO_D5 - - Disabled - - "ADC0(Digital): AD0FLAG1; ESWM_GMII/MII: GPTP0_MATCH; ESWM_RGMII0: GPTP0_MATCH; ESWM_RMII0: GPTP0_MATCH; GPT1: GTIOC1B; GPT_POEGB: GTETRGB; IRQ: IRQ1; OSPI0: OM_0_CS1; SCI9: CTS9; SPI1: SSLB1" - None - - 
      P105 N7 - OSPI_INT_ARDUINO_D6 - - Disabled - - "ADC(Digital): ADSYNC; ESWM_GMII/MII: GPTP0_CAPTURE; ESWM_RGMII0: GPTP0_CAPTURE; ESWM_RMII0: GPTP0_CAPTURE; GPT1: GTIOC1A; IRQ: IRQ0; OSPI0: OM_0_ECSINT1; SCI8: CTS_RTS8; SCI8: DE8; SPI1: SSLB2; ULPT1: ULPTO1-DS" - None - - 
      P106 N6 - OSPI_RES - - Disabled - - "ADC1(Digital): ADST1; AGT0: AGTOB0; ESWM_GMII/MII: ET1_LINKSTA; ESWM_RGMII1: ET1_LINKSTA; ESWM_RMII1: ET1_LINKSTA; GPT8: GTIOC8B; GPT_OPS: GTOWLO; IRQ: IRQ16; OSPI0: OM_0_RESET; SCI8: CTS8; SPI1: SSLB3; ULPT1: ULPTEE1-DS" - None - - 
      P107 N5 - ETH_MDINT - - Disabled - - "ADC0(Digital): ADST0; AGT0: AGTOA0; ESWM_GMII/MII: ET1_INT; ESWM_RGMII1: ET1_INT; ESWM_RMII1: ET1_INT; GPT8: GTIOC8A; GPT_OPS: GTOWUP; IRQ: IRQ31; OSPI0: OM_0_CS0; SCI4: CTS4" - None - - 
      P108 D8 - - - - Disabled - - "GPT10: GTIOC10B; IRQ: IRQ24; SDHI0: SD0DAT6" - None - - 
      P109 D7 - I2C_SDA0_PULLUP - - Disabled - - "GPT10: GTIOC10A; IRQ: IRQ23; SDHI0: SD0DAT5" - None - - 
      P110 C8 - ARDUINO_D9 - - Disabled - - "GPT9: GTIOC9B; IRQ: IRQ20; SDHI0: SD0DAT4" - None - - 
      P111 E8 - LCD_INT_MIPI_IRQ19 - - Disabled - - "GPT9: GTIOC9A; IRQ: IRQ19; SDHI0: SD0DAT3" - None - - 
      P112 A4 - SDRAM_DQ3 - - Disabled - - "ADC0(Digital): ADST0; BUS: D3; GLCDC: LCD_DATA10; GPT3: GTIOC3B; GPT_POEGA: GTETRGA; IRQ: IRQ27; SCI0: TXD0; SDHI0: SD0DAT4; SDRAM: DQ3; SPI0: SSLA2; SSIE0: SSIBCK0; ULPT0: ULPTOB0-DS" - None - - 
      P113 A2 - SDRAM_DQ4 - - Disabled - - "ADC1(Digital): ADST1; BUS: D4; GLCDC: LCD_DATA9; GPT2: GTIOC2A; GPT_POEGB: GTETRGB; IRQ: IRQ28; SCI0: RXD0; SDHI0: SD0DAT5; SDRAM: DQ4; SPI0: SSLA1; SSIE0: SSILRCK0; ULPT0: ULPTOA0-DS" - None - - 
      P114 B3 - SDRAM_DQ5 - - Disabled - - "ADC(Digital): ADSYNC; BUS: D5; GLCDC: LCD_DATA8; GPT2: GTIOC2B; GPT_POEGC: GTETRGC; IRQ: IRQ30-DS; SCI0: CTS_RTS0; SCI0: DE0; SDHI0: SD0DAT6; SDRAM: DQ5; SPI0: SSLA0; SSIE0: SSIRXD0" - None - - 
      P115 A3 - SDRAM_DQ6 - - Disabled - - "ADC0(Digital): AD0FLAG1; BUS: D6; GLCDC: LCD_DATA7; GPT5: GTIOC5A; GPT_POEGD: GTETRGD; IRQ: IRQ31-DS; SCI0: CTS0; SDHI0: SD0DAT7; SDRAM: DQ6; SPI0: MOSI0; SSIE0: SSITXD0" - None - - 
      P200 C5 - NMI - - Disabled - - "IRQ: NMI" - None - - 
      P201 E6 - MD_MIKROBUS_RES - - Disabled - - "CGC: MD; IRQ: IRQ4" - None - - 
      P206 B15 - ENET_RX_CTL - - Disabled - - "BUS: CS7; CEU: VIO_D0; CLKOUT: CLKOUT; ESWM_GMII/MII1: ET1_RX_DV; ESWM_RGMII1: RGMII1_RX_CTL; ESWM_RMII1: RMII1_CRS_DV; GPT0: GTCPPO0; GPT_OPS: GTIU; IRQ: IRQ0-DS; SDHI0: SD0DAT7; SSIE1: SSIDATA1; ULPT1: ULPTOB1; USB FS: USB_VBUSEN" - None - - 
      P207 A17 - LCD_D9 - - Disabled - - "ESWM_GMII/MII1: ET1_RXD5; GLCDC: LCD_DATA9; GPT3: GTCPPO3; IRQ: IRQ25" - None - - 
      P208 C7 - DEBUG_TDI - - Disabled - - "CANFD1: CRX1; CMPOUT: VCOUT; GPT1: GTIOC1B; GPT_OPS: GTOVLO; IRQ: IRQ3; JTAG/SWD: TDI; SCI9: RXD9" - None - - 
      P209 E7 - DEBUG_TDO_SWO - - Disabled - - "CANFD1: CTX1; CLKOUT: CLKOUT; GPT1: GTIOC1A; GPT_OPS: GTOVUP; IRQ: IRQ25; JTAG/SWD: TDO; SCI9: TXD9; TRACE: SWO" - None - - 
      P210 C6 - DEBUG_TMS_SWDIO L None Disabled - - "GPT0: GTIOC0B; GPT_OPS: GTOULO; IRQ: IRQ24; JTAG/SWD: SWDIO; JTAG/SWD: TMS; SCI9: CTS_RTS9; SCI9: DE9" - IO - - 
      P211 D6 - DEBUG_TCLK_SWCLK L None Disabled - - "GPT0: GTIOC0A; GPT_OPS: GTOUUP; IRQ: IRQ23; JTAG/SWD: SWCLK; JTAG/SWD: TCK; SCI9: DE9; SCI9: SCK9" - IO - - 
      P212 K17 CGC_EXTAL EXTAL - - "Peripheral mode" - - "AGT1: AGTEE1; CGC: EXTAL; GPT0: GTIOC0B; GPT_POEGD: GTETRGD; IRQ: IRQ3; SCI1: RXD1" - None - - 
      P213 K16 CGC_XTAL XTAL - - "Peripheral mode" - - "ADC1(Digital): ADTRG1; CGC: XTAL; GPT0: GTIOC0A; GPT_POEGC: GTETRGC; IRQ: IRQ2; SCI1: TXD1; ULPT0: ULPTEE0" - None - - 
      P214 L16 - XCOUT - - Disabled - - "CGC: XCOUT; IRQ: IRQ21" - None - - 
      P215 L17 - XCIN - - Disabled - - "CGC: EXCIN; CGC: XCIN; IRQ: IRQ20" - None - - 
      P300 B5 - SDRAM_DQ2 - - Disabled - - "BUS: D2; GLCDC: LCD_DATA11; GPT3: GTIOC3A; IRQ: IRQ4; SCI0: DE0; SCI0: SCK0; SDHI0: SD0DAT3; SDRAM: DQ2; SPI0: SSLA3; ULPT0: ULPTEVI0-DS" - None - - 
      P301 C4 - SDRAM_DQ1 - - Disabled - - "AGT0: AGTIO0; BUS: D1; GLCDC: LCD_DATA12; GPT4: GTIOC4B; GPT_OPS: GTOULO; IRQ: IRQ6; SCI6: TXD6; SDHI0: SD0DAT2; SDRAM: DQ1; ULPT0: ULPTEE0-DS" - None - - 
      P302 A5 - SDRAM_DQ0 - - Disabled - - "BUS: D0; GLCDC: LCD_DATA13; GPT4: GTIOC4A; GPT_OPS: GTOUUP; IRQ: IRQ5; SCI6: RXD6; SDHI0: SD0DAT1; SDRAM: DQ0; ULPT0: ULPTO0-DS" - None - - 
      P303 B6 GPIO USER_LED2_GREEN - - "Output mode (Initial Low)" - - "GLCDC: LCD_DATA14; GPT7: GTIOC7B; IRQ: IRQ29-DS; SCI6: DE6; SCI6: SCK6" - None - - 
      P304 D10 - ETH_TXD3_TRACE_TDATA3 - - Disabled - - "CEU: VIO_D15; ESWM_GMII/MII1: ET1_TXD3; ESWM_RGMII1: RGMII1_TXD3; GPT7: GTIOC7A; GPT_OPS: GTOVLO; IRQ: IRQ9; SDHI0: SD0DAT0; TRACE: TDATA3; ULPT1: ULPTO1" - None - - 
      P305 C10 - ETH_TXD2_TRACE_TDATA2 - - Disabled - - "CEU: VIO_D14; ESWM_GMII/MII1: ET1_TXD2; ESWM_RGMII1: RGMII1_TXD2; GPT12: GTCPPO12; GPT_OPS: GTOVUP; IRQ: IRQ8; SDHI0: SD0WP; TRACE: TDATA2; ULPT1: ULPTEE1" - None - - 
      P306 D11 - ETH_TXD1_TRACE_TDATA1 - - Disabled - - "CEU: VIO_D13; ESWM_GMII/MII1: ET1_TXD1; ESWM_RGMII1: RGMII1_TXD1; ESWM_RMII1: RMII1_TXD1; GPT11: GTCPPO11; GPT_OPS: GTIW; IRQ: IRQ28-DS; SDHI0: SD0CD; TRACE: TDATA1; ULPT1: ULPTEVI1" - None - - 
      P307 C11 - ETH_TXD0_TRACE_TDATA0 - - Disabled - - "CEU: VIO_D12; ESWM_GMII/MII1: ET1_TXD0; ESWM_RGMII1: RGMII1_TXD0; ESWM_RMII1: RMII1_TXD0; GPT10: GTCPPO10; GPT_OPS: GTIV; IRQ: IRQ27-DS; SCI6: CTS_RTS6; SCI6: DE6; SDHI0: SD0CMD; TRACE: TDATA0; ULPT1: ULPTOA1" - None - - 
      P308 C9 - TRACE_TCLK - - Disabled - - "CEU: VIO_D11; ESWM_GMII/MII1: ET1_TX_ER; ETHPHYCLK: ETHPHYCLK; GPT9: GTCPPO9; GPT_OPS: GTIU; IRQ: IRQ26-DS; SCI3: CTS3; SDHI0: SD0CLK; TRACE: TCLK; ULPT1: ULPTOB1" - None - - 
      P309 A12 - ETH_TX_CLK - - Disabled - - "CEU: VIO_D10; CMPOUT: VCOUT; ESWM_GMII/MII1: ET1_GTX_CLK; ESWM_RGMII1: RGMII1_TXC; GLCDC: LCD_DATA15; GPT8: GTCPPO8; IRQ: IRQ25-DS; SCI9: CTS9" - None - - 
      P310 E10 - ETH_TX_CTL - - Disabled - - "AGT1: AGTEE1; CEU: VIO_D9; ESWM_GMII/MII1: ET1_TX_EN; ESWM_RGMII1: RGMII1_TX_CTL; ESWM_RMII1: RMII1_TX_EN; GLCDC: LCD_DATA16; GPT7: GTCPPO7; IRQ: IRQ24-DS; SCI3: TXD3" - None - - 
      P311 B12 - CAM_D8 - - Disabled - - "AGT1: AGTOB1; CANFD0: CRX0; CEU: VIO_D8; ESWM_GMII/MII1: ET1_TX_CLK; GLCDC: LCD_DATA17; GPT: GTADSM1; GPT6: GTCPPO6; IRQ: IRQ23-DS; SCI3: DE3; SCI3: SCK3" - None - - 
      P312 C13 - ARDUINO_D7 - - Disabled - - "AGT1: AGTOA1; CANFD0: CTX0; CEU: VIO_D7; ESWM_GMII/MII1: ET1_RX_ER; ESWM_RMII1: RMII1_RX_ER; GLCDC: LCD_DATA18; GPT: GTADSM0; GPT5: GTCPPO5; IRQ: IRQ22-DS; PDM2: PDMDAT2; SCI3: CTS_RTS3; SCI3: DE3" - None - - 
      P400 P17 - CAM_D0_ARDUINO_GROVE1_SCL0 - - Disabled - - "ADC1(Digital): ADTRG1; AGT1: AGTIO1; CEU: VIO_D0; GPT6: GTIOC6A; I3C0: I3C_SCL0; IRQ: IRQ0; SCI1: TXD1; SDHI1: SD1CLK; SSIE: AUDIO_CLK" - None - - 
      P401 N17 - ARDUINO_GROVE1_SDA0 - - Disabled - - "CANFD0: CTX0; CEU: VIO_D1; GPT6: GTIOC6B; GPT_POEGA: GTETRGA; I3C0: I3C_SDA0; IRQ: IRQ5-DS; SCI1: RXD1; SDHI1: SD1CMD" - None - - 
      P402 L14 - PMOD1_8_GPIO_RST - - Disabled - - "CAC: CACREF; CANFD0: CRX0; ESWM_GMII/MII: ET0_LINKSTA; ESWM_RGMII0: ET0_LINKSTA; ESWM_RMII0: ET0_LINKSTA; IRQ: IRQ4-DS; RTC: RTCIC0; SCI1: DE1; SCI1: SCK1; SDHI1: SD1DAT0; SSIE: AUDIO_CLK" - None - - 
      P403 H13 - AUDIO_BCLK - - Disabled - - "ADC0(Digital): AD0FLAG1; ESWM_GMII/MII: ET1_WOL; ESWM_RGMII1: ET1_WOL; ESWM_RMII1: ET1_WOL; GPT3: GTIOC3A; IRQ: IRQ14-DS; RTC: RTCIC1; SCI1: CTS_RTS1; SCI1: DE1; SDHI1: SD1DAT1; SSIE0: SSIBCK0" - None - - 
      P404 J13 - AUDIO_WCLK - - Disabled - - "ADC1(Digital): AD1FLAG1; ESWM_GMII/MII: ET0_WOL; ESWM_RGMII0: ET0_WOL; ESWM_RMII0: ET0_WOL; GPT3: GTIOC3B; IRQ: IRQ15-DS; RTC: RTCIC2; SCI1: CTS1; SDHI1: SD1DAT2; SSIE0: SSILRCK0" - None - - 
      P405 G12 - CAM_D2_AUDIO_DATIN - - Disabled - - "AGT1: AGTIO1; CEU: VIO_D2; ESWM_GMII/MII0: ET0_RX_DV; ESWM_RGMII0: RGMII0_RX_CTL; ESWM_RMII0: RMII0_CRS_DV; GPT1: GTIOC1A; IRQ: IRQ30; SCI2: DE2; SCI2: SCK2; SDHI1: SD1DAT3; SSIE0: SSITXD0" - None - - 
      P406 F14 - CAM_D3_AUDIO_DOUT - - Disabled - - "CEU: VIO_D3; ESWM_GMII/MII0: ET0_RXD3; ESWM_RGMII0: RGMII0_RXD3; GPT1: GTIOC1B; IRQ: IRQ31; SCI2: TXD2; SDHI1: SD1CD; SPI0: SSLA3; SSIE0: SSIRXD0" - None - - 
      P407 R17 "USB FS_USB_VBUS" USBFS_VBUS - - "Peripheral mode" - - "ADC0(Digital): ADTRG0; AGT0: AGTIO0; BUS: CS6; ESWM_GMII/MII: GPTP_PTPOUT3; ESWM_RGMII: GPTP_PTPOUT3; ESWM_RMII: GPTP_PTPOUT3; GPT10: GTIOC10B; IIC0: SDA0; IRQ: IRQ22; RTC: RTCOUT; SCI1: DE1; SCI1: SCK1; USB FS: USB_VBUS; USB HS: USBHS_VBUSEN" - None - - 
      P408 M15 - USBHS_VBUS - - Disabled - - "ADC(Digital): ADSYNC; BUS: A17; ESWM_GMII/MII: GPTP_PTPOUT2; ESWM_RGMII: GPTP_PTPOUT2; ESWM_RMII: GPTP_PTPOUT2; GPT10: GTIOC10A; GPT_OPS: GTOWLO; IIC0: SCL0; IRQ: IRQ7; SCI3: RXD3; ULPT0: ULPTOB0; USB FS: USB_VBUSEN; USB HS: USBHS_VBUS" - None - - 
      P409 R16 - PMOD2_9_GPIO - - Disabled - - "ADC1(Digital): ADST1; BUS: A18; ESWM_GMII/MII: GPTP0_CAPTURE; ESWM_RGMII0: GPTP0_CAPTURE; ESWM_RMII0: GPTP0_CAPTURE; GPT_OPS: GTOWUP; IIC0: SDA0; IRQ: IRQ6; SCI3: TXD3; ULPT0: ULPTOA0; USB FS: USB_OVRCURA-DS; USB HS: USBHS_OVRCURA" - None - - 
      P410 K13 - PMOD2_8_GPIO_RST - - Disabled - - "ADC0(Digital): ADST0; AGT1: AGTOB1; BUS: A19; ESWM_GMII/MII: GPTP0_MATCH; ESWM_RGMII0: GPTP0_MATCH; ESWM_RMII0: GPTP0_MATCH; GPT9: GTIOC9B; GPT_OPS: GTOVLO; IIC0: SCL0; IRQ: IRQ5; SCI3: DE3; SCI3: SCK3; USB FS: USB_OVRCURB-DS; USB HS: USBHS_OVRCURB" - None - - 
      P411 M14 - DSI_TE - - Disabled - - "AGT1: AGTOA1; BUS: A20; CAC: CACREF; ESWM_GMII/MII: GPTP_PTPOUT1; ESWM_RGMII: GPTP_PTPOUT1; ESWM_RMII: GPTP_PTPOUT1; GPT9: GTIOC9A; GPT_OPS: GTOVUP; IRQ: IRQ4; MIPI: DSI_TE; SCI3: CTS_RTS3; SCI3: DE3; USB FS: USB_ID; USB HS: USBHS_ID" - None - - 
      P412 M12 - PMOD1_9_GPIO - - Disabled - - "AGT1: AGTEE1; BUS: A21; ESWM_GMII/MII: GPTP_PTPOUT0; ESWM_RGMII: GPTP_PTPOUT0; ESWM_RMII: GPTP_PTPOUT0; GPT8: GTCPPO8; GPT_OPS: GTOULO; IRQ: IRQ20-DS; SCI3: CTS3; USB FS: USB_EXICEN; USB HS: USBHS_EXICEN" - None - - 
      P413 P14 - PMOD1_10_GPIO - - Disabled - - "BUS: A22; ESWM_GMII/MII: ET_TAS_STA3; ESWM_RGMII: ET_TAS_STA3; ESWM_RMII: ET_TAS_STA3; GPT7: GTCPPO7; GPT_OPS: GTOUUP; IRQ: IRQ18; ULPT1: ULPTEE1" - None - - 
      P414 L13 - ETH_MDIO - - Disabled - - "BUS: A23; CANFD1: CRX1; CEU: VIO_CLK; ESWM_GMII/MII: ET1_MDIO; ESWM_RGMII1: ET1_MDIO; ESWM_RMII1: ET1_MDIO; GPT0: GTIOC0B; IRQ: IRQ9; SCI4: RXD4; SPI1: SSLB0" - None - - 
      P415 R15 - ETH_MDC - - Disabled - - "BUS: WAIT; CANFD1: CTX1; CEU: VIO_HD; ESWM_GMII/MII: ET1_MDC; ESWM_RGMII1: ET1_MDC; ESWM_RMII1: ET1_MDC; GPT0: GTIOC0A; IRQ: IRQ8; SCI4: TXD4; SPI1: RSPCK1" - None - - 
      P500 U7 "USB FS_USB_VBUSEN" USBFS_VBUSEN - - "Peripheral mode" - - "ADC0: AN021; ADC1: AN021; CAC: CACREF; GPT11: GTIOC11B; IRQ: IRQ24; PDM0: PDMDAT0; SCI8: RXD8; SDHI1: SD1DAT5; USB FS: USB_VBUSEN" - None - - 
      P501 R8 - CAM_XCLK - - Disabled - - "ADC0: AN020; ADC1: AN020; GPT12: GTIOC12A; IRQ: IRQ25; PDM1: PDMDAT1; SCI8: TXD8; SDHI1: SD1DAT6; USB FS: USB_OVRCURA" - None - - 
      P502 T7 - MEMS_MIC_DATA L None Disabled - - "ADC0: AN019; ADC1: AN019; GPT12: GTIOC12B; IRQ: IRQ26; PDM2: PDMDAT2; SCI8: DE8; SCI8: SCK8; SDHI1: SD1DAT7; USB FS: USB_OVRCURB" - I - - 
      P503 H2 - SDRAM_A4 - - Disabled - - "BUS: A6; CEU: VIO_D4; GPT6: GTCPPO6; GPT_OPS: GTOUUP; IRQ: IRQ6; SDHI0: SD0CD; SDRAM: A6" - None - - 
      P504 H1 - SDRAM_A5 - - Disabled - - "BUS: A7; CEU: VIO_D3; GPT1: GTCPPO1; GPT_OPS: GTOULO; IRQ: IRQ7; SDHI0: SD0WP; SDRAM: A7" - None - - 
      P505 H3 - SDRAM_A6 - - Disabled - - "BUS: A8; CEU: VIO_D2; GPT2: GTCPPO2; GPT_OPS: GTOWUP; IRQ: IRQ8; SDHI0: SD0CLK; SDRAM: A8" - None - - 
      P506 J1 - SDRAM_A7 - - Disabled - - "BUS: A9; CEU: VIO_D1; GPT3: GTCPPO3; GPT_OPS: GTOWLO; IRQ: IRQ9; SDHI0: SD0CMD; SDRAM: A9" - None - - 
      P507 J2 - SDRAM_A8 - - Disabled - - "BUS: A10; CEU: VIO_D0; ESWM_GMII/MII: ET_TAS_STA0; ESWM_RGMII: ET_TAS_STA0; ESWM_RMII: ET_TAS_STA0; GLCDC: LCD_EXTCLK; GPT: GTADSM0; GPT0: GTIOC0A; IRQ: IRQ10; SCI7: CTS_RTS7; SCI7: DE7; SDRAM: A10" - None - - 
      P508 J3 - SDRAM_A9 - - Disabled - - "BUS: A11; CEU: VIO_VD; ESWM_GMII/MII: ET_TAS_STA1; ESWM_RGMII: ET_TAS_STA1; ESWM_RMII: ET_TAS_STA1; GPT: GTADSM1; GPT0: GTIOC0B; IRQ: IRQ1; SCI5: CTS5; SDRAM: A11" - None - - 
      P509 J4 - SDRAM_A10 - - Disabled - - "BUS: A12; CEU: VIO_HD; ESWM_GMII/MII: ET_TAS_STA2; ESWM_RGMII: ET_TAS_STA2; ESWM_RMII: ET_TAS_STA2; GPT1: GTIOC1A; IRQ: IRQ2; SCI5: CTS_RTS5; SCI5: DE5; SDRAM: A12; ULPT1: ULPTEVI1" - None - - 
      P510 K3 - SDRAM_A11 - - Disabled - - "BUS: A13; CEU: VIO_CLK; ESWM_GMII/MII: ET_TAS_STA3; ESWM_RGMII: ET_TAS_STA3; ESWM_RMII: ET_TAS_STA3; GPT1: GTIOC1B; IRQ: IRQ3; SCI5: RXD5; SDRAM: A13; ULPT0: ULPTEVI0" - None - - 
      P511 U15 - IIC_SYSTEM_SDA1 - - Disabled - - "CANFD1: CRX1; ESWM_GMII/MII: ET1_LINKSTA; ESWM_RGMII1: ET1_LINKSTA; ESWM_RMII1: ET1_LINKSTA; GPT0: GTIOC0B; IIC1: SDA1; IRQ: IRQ15; SCI8: CTS_RTS8; SCI8: DE8" - None - - 
      P512 P13 - IIC_SYSTEM_SCL1 - - Disabled - - "CANFD1: CTX1; ESWM_GMII/MII: ET1_INT; ESWM_RGMII1: ET1_INT; ESWM_RMII1: ET1_INT; GPT0: GTIOC0A; IIC1: SCL1; IRQ: IRQ14; SCI8: CTS8" - None - - 
      P513 R13 - LCD_TCON3 - - Disabled - - "ACMPHS: IVCMP0; ADC0: AN016; ADC1: AN016; CEU: VIO_FLD; ESWM_GMII/MII: ET0_INT; ESWM_RGMII0: ET0_INT; ESWM_RMII0: ET0_INT; GLCDC: LCD_TCON3; GPT13: GTIOC13B; IRQ: IRQ31; SCI8: DE8; SCI8: SCK8" - None - - 
      P514 R14 - ETH_RST - - Disabled - - "ESWM_GMII/MII: ET_TAS_STA1; ESWM_RGMII: ET_TAS_STA1; ESWM_RMII: ET_TAS_STA1; GLCDC: LCD_EXTCLK; GPT13: GTIOC13B; IIC2: SDA2; IRQ: IRQ13; SCI4: DE4; SCI4: SCK4" - None - - 
      P515 P15 - LCD_CLK - - Disabled - - "ESWM_GMII/MII: ET_TAS_STA0; ESWM_RGMII: ET_TAS_STA0; ESWM_RMII: ET_TAS_STA0; GLCDC: LCD_CLK; GPT13: GTIOC13A; IIC2: SCL2; IRQ: IRQ12; SCI4: CTS_RTS4; SCI4: DE4" - None - - 
      P600 P3 - USER_LED1_BLUE - - Disabled - - "CAC: CACREF; ESWM_GMII/MII: ET1_WOL; ESWM_RGMII1: ET1_WOL; ESWM_RMII1: ET1_WOL; GPT6: GTIOC6B; IRQ: IRQ30; OSPI0: OM_0_RSTO1; ULPT1: ULPTEVI1-DS" - None - - 
      P601 P4 - PMOD2_4_RSPCKB - - Disabled - - "GPT6: GTIOC6A; IRQ: IRQ29; OSPI0: OM_0_WP1; RTC: RTCOUT; SCI0: DE0; SCI0: SCK0; ULPT0: ULPTEVI0" - None - - 
      P602 P2 - PMOD2_3_MISOB_RXD0 - - Disabled - - "GPT7: GTIOC7B; IRQ: IRQ28; OSPI1: OM_1_SCLKN; SCI0: RXD0; ULPT0: ULPTEE0" - None - - 
      P603 P1 - PMOD2_2_MOSIB_TXD0 - - Disabled - - "GPT7: GTIOC7A; IRQ: IRQ27; OSPI1: OM_1_SCLK; SCI0: TXD0; ULPT0: ULPTO0" - None - - 
      P604 N2 - PMOD2_1_SSLB0_CTS_RTS0 - - Disabled - - "GPT8: GTIOC8B; IRQ: IRQ26; OSPI1: OM_1_SIO7; SCI0: CTS_RTS0; SCI0: DE0" - None - - 
      P605 N1 - PMOD2_1_CTS0 - - Disabled - - "GPT8: GTIOC8A; IRQ: IRQ25; OSPI1: OM_1_SIO1; SCI0: CTS0" - None - - 
      P606 N3 - LCD_RST - - Disabled - - "BUS: BC3; BUS: WR3; IRQ: IRQ24; OSPI1: OM_1_SIO6" - None - - 
      P607 M2 - SDRAM_DQ31 - - Disabled - - "BUS: D31; IRQ: IRQ23; OSPI1: OM_1_DQS; SDRAM: DQ31" - None - - 
      P608 K2 - SDRAM_A12 - - Disabled - - "BUS: A14; CAC: CACREF; CEU: VIO_FLD; GPT4: GTCPPO4; GPT_OPS: GTOWUP; IRQ: IRQ22; SCI5: TXD5; SDRAM: A14" - None - - 
      P609 A1 - SDRAM_DQ7 - - Disabled - - "ADC1(Digital): AD1FLAG1; BUS: D7; CANFD1: CTX1; GLCDC: LCD_DATA6; GPT5: GTIOC5B; GPT_OPS: GTIU; IRQ: IRQ29; SCI0: TXD0; SDRAM: DQ7; SPI0: MISO0; ULPT1: ULPTOA1-DS" - None - - 
      P610 D3 - SDRAM_DQ12 - - Disabled - - "BUS: D12; CANFD1: CRX1; GLCDC: LCD_DATA5; GPT4: GTIOC4A; GPT_OPS: GTOUUP; IRQ: IRQ16; SCI0: RXD0; SDRAM: DQ12; SPI0: RSPCK0; ULPT1: ULPTOB1-DS" - None - - 
      P611 D2 - SDRAM_DQ13 - - Disabled - - "BUS: D13; CAC: CACREF; CLKOUT: CLKOUT; GLCDC: LCD_DATA4; GPT4: GTIOC4B; GPT_OPS: GTOULO; IRQ: IRQ17; SCI0: DE0; SCI0: SCK0; SDRAM: DQ13; SPI0: MOSI0; USB HS: USBHS_VBUSEN" - None - - 
      P612 E4 - SDRAM_DQ14 - - Disabled - - "BUS: D14; GLCDC: LCD_DATA3; GPT9: GTIOC9A; IRQ: IRQ18; SCI0: CTS_RTS0; SCI0: DE0; SDRAM: DQ14; SPI0: SSLA0; USB HS: USBHS_OVRCURA" - None - - 
      P613 C2 - SDRAM_DQ15 - - Disabled - - "AGT1: AGTO1; BUS: D15; GLCDC: LCD_DATA2; GPT9: GTIOC9B; GPT_POEGA: GTETRGA; IRQ: IRQ19; SCI0: CTS0; SDRAM: DQ15; USB HS: USBHS_OVRCURB" - None - - 
      P614 E3 - SDRAM_DQM0 - - Disabled - - "AGT0: AGTO0; BUS: WR; BUS: WR0; GLCDC: LCD_DATA1; GPT9: GTCPPO9; GPT_POEGB: GTETRGB; IRQ: IRQ20; SCI7: RXD7; SDRAM: DQM0; USB HS: USBHS_ID" - None - - 
      P615 E2 - SDRAM_DQM2 - - Disabled - - "BUS: BC2; BUS: WR2; GLCDC: LCD_DATA0; GPT10: GTCPPO10; GPT_POEGC: GTETRGC; IRQ: IRQ7; SCI7: TXD7; SDRAM: DQM2; USB HS: USBHS_EXICEN" - None - - 
      P700 F12 - CAM_D4 - - Disabled - - "CEU: VIO_D4; ESWM_GMII/MII0: ET0_RXD2; ESWM_RGMII0: RGMII0_RXD2; GPT5: GTIOC5A; IRQ: IRQ16-DS; SCI2: RXD2; SDHI1: SD1WP; SPI0: MISO0; SSIE1: SSIDATA1" - None - - 
      P701 F15 - CAM_D5 - - Disabled - - "CEU: VIO_D5; ESWM_GMII/MII0: ET0_RXD1; ESWM_RGMII0: RGMII0_RXD1; ESWM_RMII0: RMII0_RXD1; GPT5: GTIOC5B; IRQ: IRQ17-DS; SCI2: CTS_RTS2; SCI2: DE2; SDHI1: SD1DAT4; SPI0: MOSI0; SSIE1: SSILRCK1; ULPT1: ULPTO1" - None - - 
      P702 F13 - CAM_D6 - - Disabled - - "CEU: VIO_D6; ESWM_GMII/MII0: ET0_RXD0; ESWM_RGMII0: RGMII0_RXD0; ESWM_RMII0: RMII0_RXD0; GPT6: GTIOC6A; IRQ: IRQ18-DS; SCI2: CTS2; SDHI1: SD1DAT5; SPI0: RSPCK0; SSIE1: SSIBCK1; ULPT0: ULPTO0" - None - - 
      P703 G14 - CAM_D7 - - Disabled - - "AGT1: AGTO1; CEU: VIO_D7; CMPOUT: VCOUT; ESWM_GMII/MII0: ET0_RX_CLK; ESWM_RGMII0: RGMII0_RXC; ESWM_RMII0: RMII0_REF50CK; GPT6: GTIOC6B; IRQ: IRQ19-DS; PDM0: PDMCLK0; SDHI1: SD1DAT6; SPI0: SSLA0" - None - - 
      P704 G13 - PMOD2_10_GPIO - - Disabled - - "AGT0: AGTO0; CANFD0: CTX0; CEU: VIO_D8; ESWM_GMII/MII0: ET0_RX_ER; ESWM_RMII0: RMII0_RX_ER; GPT: GTADSM0; GPT0: GTCPPO0; IRQ: IRQ26; PDM1: PDMCLK1; SDHI1: SD1DAT7; SPI0: SSLA1" - None - - 
      P705 F17 - CAM_D9 - - Disabled - - "AGT0: AGTIO0; CANFD0: CRX0; CEU: VIO_D9; ESWM_GMII/MII0: ET0_TX_EN; ESWM_RGMII0: RGMII0_TX_CTL; ESWM_RMII0: RMII0_TX_EN; GPT: GTADSM1; GPT1: GTCPPO1; IRQ: IRQ19; PDM2: PDMCLK2; SCI1: CTS1; SPI0: SSLA2" - None - - 
      P706 E17 - CAM_D10 - - Disabled - - "AGT0: AGTIO0; CEU: VIO_D10; ESWM_GMII/MII0: ET0_GTX_CLK; ESWM_RGMII0: RGMII0_TXC; ETHPHYCLK: ETHPHYCLK; GPT2: GTCPPO2; IRQ: IRQ7; PDM0: PDMDAT0; SCI1: RXD1; USB HS: USBHS_OVRCURB-DS" - None - - 
      P707 F16 - LCD_D18_CAM_D11 - - Disabled - - "CEU: VIO_D11; ESWM_GMII/MII0: ET0_TX_ER; ETHPHYCLK: ETHPHYCLK; GLCDC: LCD_DATA18; GPT3: GTCPPO3; IRQ: IRQ8; PDM1: PDMDAT1; SCI1: TXD1; USB HS: USBHS_OVRCURA-DS" - None - - 
      P708 N12 - LCD_BLEN - - Disabled - - "BUS: BC1; BUS: WR1; CAC: CACREF; CEU: VIO_VD; ESWM_GMII/MII: ET0_MDC; ESWM_RGMII0: ET0_MDC; ESWM_RMII0: ET0_MDC; GPT6: GTCPPO6; IIC2: SDA2; IRQ: IRQ11; SCI4: DE4; SCI4: SCK4; SPI1: MOSI1; SSIE: AUDIO_CLK" - None - - 
      P709 P16 - CAM_RST - - Disabled - - "BUS: CS4; CEU: VIO_D13; ESWM_GMII/MII: ET0_MDIO; ESWM_RGMII0: ET0_MDIO; ESWM_RMII0: ET0_MDIO; GPT5: GTCPPO5; IIC2: SCL2; IRQ: IRQ10; SCI4: CTS_RTS4; SCI4: DE4; SPI1: MISO1" - None - - 
      P710 M13 - LCD_EXTCLK - - Disabled - - "BUS: CS5; CEU: VIO_D12; ESWM_GMII/MII: ET0_LINKSTA; ESWM_RGMII0: ET0_LINKSTA; ESWM_RMII0: ET0_LINKSTA; GLCDC: LCD_EXTCLK; GPT11: GTIOC11B; IRQ: IRQ17; SCI4: CTS4; SPI1: SSLB3" - None - - 
      P711 N15 - LCD_D19 - - Disabled - - "AGT0: AGTEE0; ESWM_GMII/MII: GPTP0_PPS; ESWM_RGMII0: GPTP0_PPS; ESWM_RMII0: GPTP0_PPS; GLCDC: LCD_DATA19; GPT11: GTIOC11A; IRQ: IRQ3; SCI1: CTS_RTS1; SCI1: DE1; SPI1: SSLB2" - None - - 
      P712 N13 - LCD_D20 - - Disabled - - "AGT0: AGTOB0; ESWM_GMII/MII: GPTP1_CAPTURE; ESWM_RGMII1: GPTP1_CAPTURE; ESWM_RMII1: GPTP1_CAPTURE; GLCDC: LCD_DATA20; GPT2: GTIOC2B; IRQ: IRQ2; SCI1: CTS1; SPI1: SSLB1" - None - - 
      P713 N16 - LCD_D21 - - Disabled - - "AGT0: AGTOA0; ESWM_GMII/MII: GPTP1_MATCH; ESWM_RGMII1: GPTP1_MATCH; ESWM_RMII1: GPTP1_MATCH; GLCDC: LCD_DATA21; GPT2: GTIOC2A; IRQ: IRQ14; SCI4: CTS4" - None - - 
      P714 N14 - LCD_D22 - - Disabled - - "ESWM_GMII/MII: GPTP1_PPS; ESWM_RGMII1: GPTP1_PPS; ESWM_RMII1: GPTP1_PPS; GLCDC: LCD_DATA22; GPT12: GTIOC12B; IRQ: IRQ13; MIPI: DSI_TE; SCI4: TXD4" - None - - 
      P715 T15 - LCD_D23 - - Disabled - - "ESWM_GMII/MII: ET_TAS_STA2; ESWM_RGMII: ET_TAS_STA2; ESWM_RMII: ET_TAS_STA2; GLCDC: LCD_DATA23; GPT12: GTIOC12A; IRQ: IRQ12; SCI4: RXD4" - None - - 
      P800 T6 - OSPI_DQ5_PMOD1_1_CTS2 - - Disabled - - "AGT0: AGTOA0; GPT11: GTIOC11A; GPT_OPS: GTIU; IRQ: IRQ11; OSPI0: OM_0_SIO5; SCI2: CTS2" - None - - 
      P801 P6 - OSPI_DS L None Disabled - - "AGT0: AGTOB0; ESWM_GMII/MII: GPTP1_PPS; ESWM_RGMII1: GPTP1_PPS; ESWM_RMII1: GPTP1_PPS; GPT11: GTIOC11B; GPT_OPS: GTIV; IRQ: IRQ12; OSPI0: OM_0_DQS; SCI2: TXD2" - O - - 
      P802 R6 - OSPI_DQ6 - - Disabled - - "GPT12: GTIOC12A; GPT_OPS: GTIW; IRQ: IRQ18; OSPI0: OM_0_SIO6; SCI2: RXD2" - None - - 
      P803 P7 - OSPI_DQ1 - - Disabled - - "GPT12: GTIOC12B; GPT_POEGC: GTETRGC; IRQ: IRQ19; OSPI0: OM_0_SIO1; SCI2: DE2; SCI2: SCK2" - None - - 
      P804 R7 - OSPI_DQ7 - - Disabled - - "GPT13: GTIOC13A; GPT_POEGD: GTETRGD; IRQ: IRQ14; MIPI: DSI_TE; OSPI0: OM_0_SIO7; SCI2: CTS_RTS2; SCI2: DE2" - None - - 
      P805 P12 - LCD_HSYNC_TCON1 - - Disabled - - "ACMPHS: IVCMP0; ADC0: AN017; ADC1: AN017; CEU: VIO_D15; ESWM_GMII/MII: ET1_MDIO; ESWM_RGMII1: ET1_MDIO; ESWM_RMII1: ET1_MDIO; GLCDC: LCD_TCON1; IRQ: IRQ30; SCI8: TXD8" - None - - 
      P806 T14 - LCD_VSYNC_TCON0 - - Disabled - - "ADC0: AN018; ADC1: AN018; CEU: VIO_D14; ESWM_GMII/MII: ET1_MDC; ESWM_RGMII1: ET1_MDC; ESWM_RMII1: ET1_MDC; GLCDC: LCD_TCON0; IRQ: IRQ0; SCI8: RXD8" - None - - 
      P807 N11 - LCD_DE_TCON2 - - Disabled - - "GLCDC: LCD_TCON2; GPT13: GTIOC13A; IRQ: IRQ11" - None - - 
      P808 U5 - OSPI_SCLK_ARDUINO_D0_RXD_MIKROBUS_RXD - - Disabled - - "GPT13: GTIOC13B; IRQ: IRQ15; OSPI0: OM_0_SCLK; SCI7: RXD7" - None - - 
      P809 T5 - ARDUINO_D1_TXD_MIKROBUS_TXD - - Disabled - - "IRQ: IRQ20; OSPI0: OM_0_SCLKN; SCI7: TXD7" - None - - 
      P810 M9 - ARDUINO_D4_MIKROBUS_1_PWM - - Disabled - - "GPT10: GTIOC10A; IRQ: IRQ21; PDM0: PDMCLK0; SCI7: DE7; SCI7: SCK7; SDHI1: SD1DAT2; ULPT0: ULPTOA0" - None - - 
      P811 N8 - ARDUINO_D3 - - Disabled - - "GPT10: GTIOC10B; IRQ: IRQ22; PDM1: PDMCLK1; SCI7: CTS7; SDHI1: SD1DAT3; ULPT0: ULPTOB0; USB FS: USB_ID" - None - - 
      P812 P8 - MEMS_MIC_CLK L None Disabled - - "ADC0: AN022; ADC1: AN022; GPT11: GTIOC11A; IRQ: IRQ23; PDM2: PDMCLK2; SCI7: CTS_RTS7; SCI7: DE7; SDHI1: SD1DAT4; USB FS: USB_EXICEN" - O - - 
      P813 B1 - SDRAM_CS - - Disabled - - "CEU: VIO_D13; GPT7: GTIOC7B; GPT_POEGA: GTETRGA; IRQ: IRQ15; PDM2: PDMCLK2; SCI7: DE7; SCI7: SCK7; SDRAM: SDCS" - None - - 
      P814 U16 - USBFS_DP - - Disabled - - "CANFD0: CRX0; GPT8: GTIOC8B; IRQ: IRQ16; USB FS: USB_DP" - None - - 
      P815 T16 - USBFS_DN - - Disabled - - "CANFD0: CTX0; GPT8: GTIOC8A; IRQ: IRQ15; USB FS: USB_DM" - None - - 
      P902 E9 - CAM_D1_LCD_D3 - - Disabled - - "BUS: ALE; CEU: VIO_D1; ETHPHYCLK: ETHPHYCLK; GLCDC: LCD_DATA3; GPT13: GTCPPO13; IRQ: IRQ0; SSIE: AUDIO_CLK" - None - - 
      P903 D9 - LCD_D2 - - Disabled - - "GLCDC: LCD_DATA2; GPT11: GTIOC11A; IRQ: IRQ1" - None - - 
      P904 A16 - LCD_D8 - - Disabled - - "ESWM_GMII/MII1: ET1_RXD4; GLCDC: LCD_DATA8; GPT11: GTIOC11B; IRQ: IRQ2" - None - - 
      P905 A14 - ETH_RX_CLK - - Disabled - - "ADC1(Digital): AD1FLAG1; CEU: VIO_D6; ESWM_GMII/MII1: ET1_RX_CLK; ESWM_RGMII1: RGMII1_RXC; ESWM_RMII1: RMII1_REF50CK; GLCDC: LCD_DATA19; GPT13: GTCPPO13; IRQ: IRQ8; PDM1: PDMDAT1; SCI3: RXD3" - None - - 
      P906 A13 - ETH_RXD0 - - Disabled - - "ADC0(Digital): AD0FLAG1; CEU: VIO_D5; ESWM_GMII/MII1: ET1_RXD0; ESWM_RGMII1: RGMII1_RXD0; ESWM_RMII1: RMII1_RXD0; GLCDC: LCD_DATA20; GPT13: GTIOC13B; IRQ: IRQ9; PDM0: PDMDAT0; SCI6: CTS6; SSIE1: SSILRCK1; ULPT1: ULPTO1; USB FS: USB_ID" - None - - 
      P907 A15 - ETH_RXD1 - - Disabled - - "ADC(Digital): ADSYNC; CEU: VIO_D4; ESWM_GMII/MII1: ET1_RXD1; ESWM_RGMII1: RGMII1_RXD1; ESWM_RMII1: RMII1_RXD1; GLCDC: LCD_DATA21; GPT13: GTIOC13A; IRQ: IRQ10; PDM2: PDMCLK2; SCI6: DE6; SCI6: SCK6; SSIE1: SSIBCK1; ULPT1: ULPTEE1; USB FS: USB_EXICEN" - None - - 
      P908 B13 - ETH_RXD2 - - Disabled - - "ADC1(Digital): ADST1; CANFD1: CRX1; CEU: VIO_D3; ESWM_GMII/MII1: ET1_RXD2; ESWM_RGMII1: RGMII1_RXD2; GLCDC: LCD_DATA22; GPT12: GTIOC12B; IRQ: IRQ11; PDM1: PDMCLK1; SCI6: TXD6; ULPT1: ULPTEVI1; USB FS: USB_OVRCURB; USB HS: USBHS_ID" - None - - 
      P909 B14 - ETH_RXD3 - - Disabled - - "ADC0(Digital): ADST0; CANFD1: CTX1; CEU: VIO_D2; ESWM_GMII/MII1: ET1_RXD3; ESWM_RGMII1: RGMII1_RXD3; GLCDC: LCD_DATA23; GPT12: GTIOC12A; IRQ: IRQ21-DS; PDM0: PDMCLK0; SCI6: RXD6; ULPT1: ULPTOA1; USB FS: USB_OVRCURA; USB HS: USBHS_EXICEN" - None - - 
      P910 E11 - LCD_D4 - - Disabled - - "ESWM_GMII/MII1: ET1_TXD4; GLCDC: LCD_DATA4; GPT12: GTCPPO12; IRQ: IRQ7" - None - - 
      P911 C12 - LCD_D5 - - Disabled - - "ESWM_GMII/MII1: ET1_TXD5; GLCDC: LCD_DATA5; GPT3: GTIOC3B; IRQ: IRQ6" - None - - 
      P912 D12 - LCD_D6 - - Disabled - - "ESWM_GMII/MII1: ET1_TXD6; GLCDC: LCD_DATA6; GPT3: GTIOC3A; IRQ: IRQ5" - None - - 
      P913 E12 - LCD_D7 - - Disabled - - "CLKOUT: CLKOUT; ESWM_GMII/MII1: ET1_TXD7; GLCDC: LCD_DATA7; GPT11: GTCPPO11; IRQ: IRQ3" - None - - 
      P914 E5 - LCD_D0 - - Disabled - - "GLCDC: LCD_DATA0; GPT5: GTIOC5B; IRQ: IRQ9; SCI6: CTS_RTS6; SCI6: DE6" - None - - 
      P915 A6 - LCD_D1 - - Disabled - - "GLCDC: LCD_DATA1; GPT5: GTIOC5A; IRQ: IRQ8; SCI6: CTS6" - None - - 
      PA00 G1 - SDRAM_A3 - - Disabled - - "ADC1(Digital): AD1FLAG1; BUS: A5; CEU: VIO_D5; GLCDC: LCD_CLK; GPT7: GTCPPO7; GPT_OPS: GTOVLO; IRQ: IRQ22; SCI5: CTS_RTS5; SCI5: DE5; SDHI0: SD0DAT7; SDRAM: A5" - None - - 
      PA01 H4 - SDRAM_A2 - - Disabled - - "ADC0(Digital): AD0FLAG1; BUS: A4; CEU: VIO_D6; GLCDC: LCD_TCON0; GPT8: GTCPPO8; GPT_OPS: GTOVUP; IRQ: IRQ21; SCI5: CTS5; SDHI0: SD0DAT6; SDRAM: A4" - None - - 
      PA02 F1 - SDRAM_A1 L None Disabled - - "ADC(Digital): ADSYNC; BUS: A3; CEU: VIO_D7; GPT9: GTCPPO9; GPT_OPS: GTIW; IRQ: IRQ31; SCI2: RXD2; SDHI0: SD0DAT5; SDRAM: A3" - I - - 
      PA03 G2 - SDRAM_A0 - - Disabled - - "ADC1(Digital): ADST1; BUS: A2; CEU: VIO_D8; GPT10: GTCPPO10; GPT_OPS: GTIV; IRQ: IRQ20; SCI2: TXD2; SDHI0: SD0DAT4; SDRAM: A2" - None - - 
      PA04 D1 - SDRAM_DQM3 - - Disabled - - "ADC0(Digital): ADST0; BUS: A1; CEU: VIO_D9; GPT4: GTIOC4B; GPT_OPS: GTIU; IRQ: IRQ19; SCI2: DE2; SCI2: SCK2; SDHI0: SD0DAT3; SDRAM: A1; SDRAM: DQM3" - None - - 
      PA05 G3 - SDRAM_DQM1 - - Disabled - - "BUS: A0; BUS: BC0; CEU: VIO_D10; GPT4: GTIOC4A; GPT_POEGD: GTETRGD; IRQ: IRQ18; PDM2: PDMDAT2; SCI2: CTS_RTS2; SCI2: DE2; SDHI0: SD0DAT2; SDRAM: A0; SDRAM: DQM1" - None - - 
      PA06 C1 - SDRAM_CKE - - Disabled - - "BUS: CS1; CEU: VIO_D11; GPT7: GTIOC7B; GPT_POEGC: GTETRGC; IRQ: IRQ17; PDM1: PDMDAT1; SCI2: CTS2; SDHI0: SD0DAT1; SDRAM: CKE" - None - - 
      PA07 G4 - USER_LED3_RED - - Disabled - - "BUS: RD; CEU: VIO_D12; CMPOUT: VCOUT; GPT7: GTIOC7A; GPT_POEGB: GTETRGB; IRQ: IRQ16; PDM0: PDMDAT0; SCI7: CTS7; SDHI0: SD0DAT0" - None - - 
      PA08 F3 - SDRAM_WE - - Disabled - - "BUS: CS0; GLCDC: LCD_TCON3; GPT11: GTCPPO11; GPT_POEGD: GTETRGD; IRQ: IRQ6; SCI5: RXD5; SDRAM: WE" - None - - 
      PA09 F4 - SDRAM_CAS - - Disabled - - "BUS: CS3; GLCDC: LCD_TCON2; GPT12: GTCPPO12; IRQ: IRQ5; SCI5: TXD5; SDRAM: CAS" - None - - 
      PA10 F2 - SDRAM_RAS - - Disabled - - "BUS: CS2; CEU: VIO_D15; GLCDC: LCD_TCON1; GPT13: GTCPPO13; IRQ: IRQ4; PDM0: PDMCLK0; SCI5: DE5; SCI5: SCK5; SDRAM: RAS" - None - - 
      PA11 B4 - SDRAM_DQ8 - - Disabled - - "BUS: D8; GPT6: GTIOC6A; GPT_OPS: GTIV; IRQ: IRQ10; SCI9: DE9; SCI9: SCK9; SDRAM: DQ8" - None - - 
      PA12 B2 - SDRAM_DQ9 - - Disabled - - "BUS: D9; GPT6: GTIOC6B; GPT_OPS: GTIW; IRQ: IRQ11; SCI9: RXD9; SDRAM: DQ9" - None - - 
      PA13 C3 - SDRAM_DQ10 - - Disabled - - "BUS: D10; GPT10: GTIOC10A; GPT_OPS: GTOVUP; IRQ: IRQ12; SCI9: CTS_RTS9; SCI9: DE9; SDRAM: DQ10" - None - - 
      PA14 D4 - SDRAM_DQ11 - - Disabled - - "BUS: D11; GPT10: GTIOC10B; GPT_OPS: GTOVLO; IRQ: IRQ13; SCI9: TXD9; SDRAM: DQ11" - None - - 
      PA15 E1 - SDRAM_CLK - - Disabled - - "BUS: EBCLK; CEU: VIO_D14; GPT7: GTIOC7A; IRQ: IRQ14; PDM1: PDMCLK1; SCI9: CTS9; SDRAM: SDCLK" - None - - 
      PB00 E16 - LCD_D17 - - Disabled - - "ADC0(Digital): ADST0; ESWM_GMII/MII0: ET0_TXD0; ESWM_RGMII0: RGMII0_TXD0; ESWM_RMII0: RMII0_TXD0; GLCDC: LCD_DATA17; GPT4: GTCPPO4; IRQ: IRQ10; PDM2: PDMDAT2; SCI1: DE1; SCI1: SCK1; USB HS: USBHS_VBUSEN" - None - - 
      PB01 D17 - LCD_D13 - - Disabled - - "ADC1(Digital): AD1FLAG1; BUS: ALE; CEU: VIO_FLD; ESWM_GMII/MII0: ET0_TX_CLK; GLCDC: LCD_DATA13; GPT2: GTCPPO2; IRQ: IRQ12; SCI1: CTS_RTS1; SCI1: DE1" - None - - 
      PB02 E13 - CAM_VSYNC_LCD_D16 - - Disabled - - "ADC1(Digital): ADST1; CEU: VIO_VD; ESWM_GMII/MII0: ET0_TXD1; ESWM_RGMII0: RGMII0_TXD1; ESWM_RMII0: RMII0_TXD1; GLCDC: LCD_DATA16; GPT0: GTCPPO0; IRQ: IRQ11; SCI5: RXD5" - None - - 
      PB03 D16 - CAM_HSYNC_LCD_D15 - - Disabled - - "ADC(Digital): ADSYNC; CEU: VIO_HD; ESWM_GMII/MII0: ET0_TXD2; ESWM_RGMII0: RGMII0_TXD2; GLCDC: LCD_DATA15; GPT1: GTCPPO1; IRQ: IRQ13; SCI5: TXD5" - None - - 
      PB04 D13 - CAM_PCLK_LCD_D14 - - Disabled - - "ADC0(Digital): AD0FLAG1; CEU: VIO_CLK; ESWM_GMII/MII0: ET0_TXD3; ESWM_RGMII0: RGMII0_TXD3; GLCDC: LCD_DATA14; GPT3: GTCPPO3; IRQ: IRQ9; SCI5: DE5; SCI5: SCK5" - None - - 
      PB05 D15 - LCD_D12 - - Disabled - - "ESWM_GMII/MII0: ET0_TXD7; GLCDC: LCD_DATA12; GPT4: GTCPPO4; IRQ: IRQ15; SCI5: CTS5" - None - - 
      PB06 E14 - LCD_D11 - - Disabled - - "ESWM_GMII/MII0: ET0_TXD6; GLCDC: LCD_DATA11; GPT9: GTIOC9A; IRQ: IRQ0; SCI5: CTS_RTS5; SCI5: DE5" - None - - 
      PB07 D14 - LCD_D10 - - Disabled - - "ESWM_GMII/MII0: ET0_TXD5; GLCDC: LCD_DATA10; GPT9: GTIOC9B; IRQ: IRQ1" - None - - 
      PC00 M1 - SDRAM_DQ30 - - Disabled - - "BUS: D30; GPT7: GTCPPO7; IRQ: IRQ28; OSPI1: OM_1_SIO5; SCI7: CTS_RTS7; SCI7: DE7; SDRAM: DQ30" - None - - 
      PC01 M3 - SDRAM_DQ29 - - Disabled - - "BUS: D29; GPT6: GTCPPO6; IRQ: IRQ27; OSPI1: OM_1_SIO0; SCI7: CTS7; SDRAM: DQ29" - None - - 
      PC02 L2 - SDRAM_DQ28 - - Disabled - - "BUS: D28; GPT5: GTCPPO5; IRQ: IRQ26; OSPI1: OM_1_SIO3; SCI7: DE7; SCI7: SCK7; SDRAM: DQ28" - None - - 
      PC03 L1 - SDRAM_DQ27 - - Disabled - - "BUS: D27; GPT4: GTCPPO4; IRQ: IRQ25; OSPI1: OM_1_SIO4; SCI7: TXD7; SDRAM: DQ27" - None - - 
      PC04 L3 - SDRAM_DQ26 - - Disabled - - "BUS: D26; GPT3: GTCPPO3; IRQ: IRQ24; OSPI1: OM_1_SIO2; SCI7: RXD7; SDRAM: DQ26" - None - - 
      PC05 L5 - SDRAM_DQ25 - - Disabled - - "BUS: D25; GPT2: GTCPPO2; IRQ: IRQ23; OSPI1: OM_1_CS1; SDRAM: DQ25" - None - - 
      PC06 N4 - SDRAM_DQ24 - - Disabled - - "BUS: D24; GPT1: GTCPPO1; IRQ: IRQ22; OSPI1: OM_1_ECSINT1; SDRAM: DQ24" - None - - 
      PC07 K5 - SDRAM_DQ23 - - Disabled - - "BUS: D23; GPT0: GTCPPO0; IRQ: IRQ21; OSPI1: OM_1_RESET; SDRAM: DQ23" - None - - 
      PC08 M4 - SDRAM_DQ22 - - Disabled - - "BUS: D22; GPT8: GTCPPO8; IRQ: IRQ29; OSPI1: OM_1_CS0; SDRAM: DQ22" - None - - 
      PC09 L4 - SDRAM_DQ21 - - Disabled - - "BUS: D21; IRQ: IRQ5; OSPI1: OM_1_RSTO1; SDRAM: DQ21" - None - - 
      PC10 M5 - SDRAM_DQ20 - - Disabled - - "BUS: D20; GPT13: GTCPPO13; IRQ: IRQ4; OSPI1: OM_1_WP1; SDRAM: DQ20" - None - - 
      PC11 H5 - SDRAM_DQ19 - - Disabled - - "BUS: D19; ESWM_GMII/MII: ET0_MDC; ESWM_RGMII0: ET0_MDC; ESWM_RMII0: ET0_MDC; GPT12: GTCPPO12; IRQ: IRQ3; SCI6: CTS_RTS6; SCI6: DE6; SDRAM: DQ19" - None - - 
      PC12 G5 - SDRAM_DQ18 - - Disabled - - "BUS: D18; ESWM_GMII/MII: ET0_MDIO; ESWM_RGMII0: ET0_MDIO; ESWM_RMII0: ET0_MDIO; GPT11: GTCPPO11; IRQ: IRQ2; SCI6: DE6; SCI6: SCK6; SDRAM: DQ18" - None - - 
      PC13 J5 - SDRAM_DQ17 - - Disabled - - "BUS: D17; ESWM_GMII/MII: ET0_INT; ESWM_RGMII0: ET0_INT; ESWM_RMII0: ET0_INT; GPT10: GTCPPO10; IRQ: IRQ1; SCI6: RXD6; SDRAM: DQ17" - None - - 
      PC14 F5 - SDRAM_DQ16 - - Disabled - - "BUS: D16; ESWM_GMII/MII: ET0_WOL; ESWM_RGMII0: ET0_WOL; ESWM_RMII0: ET0_WOL; GPT: GTADSM1; GPT9: GTCPPO9; IRQ: IRQ0; SCI6: TXD6; SDRAM: DQ16" - None - - 
      PC15 K1 - SDRAM_BA1 - - Disabled - - "BUS: A16; CANFD1: CRX1; GPT: GTADSM0; IRQ: IRQ30; SCI6: CTS6; SDRAM: A16" - None - - 
      PD00 K4 - SDRAM_BA0 - - Disabled - - "BUS: A15; CANFD1: CTX1; GPT5: GTCPPO5; GPT_OPS: GTOWLO; IRQ: IRQ23; SCI5: DE5; SCI5: SCK5; SDRAM: A15" - None - - 
      PD01 B16 - ARDUINO_D8_MIKROBUS_INT - - Disabled - - "ESWM_GMII/MII1: ET1_RXD6; GPT2: GTCPPO2; IRQ: IRQ22; SCI8: DE8; SCI8: SCK8; SDHI0: SD0DAT2" - None - - 
      PD02 B17 - JLINK_VCOM_TX L None Disabled - - "ESWM_GMII/MII1: ET1_RXD7; GPT1: GTCPPO1; IRQ: IRQ21; SCI8: TXD8; SDHI0: SD0DAT1" - O - - 
      PD03 C15 - JLINK_VCOM_RXD L None Disabled - - "ESWM_GMII/MII0: ET0_RXD4; GPT3: GTIOC3B; IRQ: IRQ21; SCI8: RXD8; SDHI0: SD0DAT0; USB HS: USBHS_EXICEN" - I - - 
      PD04 C14 - JLINK_VCOM_CTS_RTS - - Disabled - - "ESWM_GMII/MII0: ET0_RXD5; GPT3: GTIOC3A; IRQ: IRQ20; SCI8: CTS_RTS8; SCI8: DE8; SDHI0: SD0CMD; USB HS: USBHS_ID" - None - - 
      PD05 C16 - JLINK_VCOM_CTS - - Disabled - - "ESWM_GMII/MII0: ET0_RXD6; GPT2: GTIOC2B; IRQ: IRQ19; SCI8: CTS8; SDHI0: SD0CLK; USB HS: USBHS_OVRCURB" - None - - 
      PD06 C17 - AUDIO_MCLK - - Disabled - - "ESWM_GMII/MII0: ET0_RXD7; GPT2: GTIOC2A; IRQ: IRQ18; SDHI0: SD0WP; USB HS: USBHS_OVRCURA" - None - - 
      PD07 E15 - USB_HS_VBUS_SEL - - Disabled - - "ESWM_GMII/MII0: ET0_TXD4; GPT0: GTCPPO0; IRQ: IRQ17; SDHI0: SD0CD; USB HS: USBHS_VBUSEN" - None - - 
      RES D5 CGC_RES - - - - - - - - IO "Read only" - 
      USBHS_DM H17 CGC_USBHS_DM - - - - - - - - IO "Read only" - 
      USBHS_DP H16 CGC_USBHS_DP - - - - - - - - IO "Read only" - 
      USBHS_RREF J15 CGC_USBHS_RREF - - - - - - - - IO "Read only" - 
      VBATT M16 CGC_VBATT - - - - - - - - IO "Read only" - 
      VCC H11 CGC_VCC - - - - - - - - IO "Read only" - 
      VCC H14 CGC_VCC - - - - - - - - IO "Read only" - 
      VCC G11 CGC_VCC - - - - - - - - IO "Read only" - 
      VCC G16 CGC_VCC - - - - - - - - IO "Read only" - 
      VCC F6 CGC_VCC - - - - - - - - IO "Read only" - 
      VCC G6 CGC_VCC - - - - - - - - IO "Read only" - 
      VCC F11 CGC_VCC - - - - - - - - IO "Read only" - 
      VCC H6 CGC_VCC - - - - - - - - IO "Read only" - 
      VCC L15 CGC_VCC - - - - - - - - IO "Read only" - 
      VCC K14 CGC_VCC - - - - - - - - IO "Read only" - 
      VCC18_MIPI R2 CGC_VCC18_MIPI - - - - - - - - IO "Read only" - 
      VCC2 R1 CGC_VCC2 - - - - - - - - IO "Read only" - 
      VCC2 J6 CGC_VCC2 - - - - - - - - IO "Read only" - 
      VCC2 L6 CGC_VCC2 - - - - - - - - IO "Read only" - 
      VCC2 M7 CGC_VCC2 - - - - - - - - IO "Read only" - 
      VCC2 M8 CGC_VCC2 - - - - - - - - IO "Read only" - 
      VCC_DCDC A10 CGC_VCC_DCDC - - - - - - - - IO "Read only" - 
      VCC_DCDC A11 CGC_VCC_DCDC - - - - - - - - IO "Read only" - 
      VCC_DCDC B10 CGC_VCC_DCDC - - - - - - - - IO "Read only" - 
      VCC_DCDC B11 CGC_VCC_DCDC - - - - - - - - IO "Read only" - 
      VCC_USB U17 CGC_VCC_USB - - - - - - - - IO "Read only" - 
      VCC_USBHS H15 CGC_VCC_USBHS - - - - - - - - IO "Read only" - 
      VCL F9 CGC_VCL - - - - - - - - IO "Read only" - 
      VCL G9 CGC_VCL - - - - - - - - IO "Read only" - 
      VCL H9 CGC_VCL - - - - - - - - IO "Read only" - 
      VCL M11 CGC_VCL - - - - - - - - IO "Read only" - 
      VCL J8 CGC_VCL - - - - - - - - IO "Read only" - 
      VCL J9 CGC_VCL - - - - - - - - IO "Read only" - 
      VCL K8 CGC_VCL - - - - - - - - IO "Read only" - 
      VCL K9 CGC_VCL - - - - - - - - IO "Read only" - 
      VCL L10 CGC_VCL - - - - - - - - IO "Read only" - 
      VCL L11 CGC_VCL - - - - - - - - IO "Read only" - 
      VCL K11 CGC_VCL - - - - - - - - IO "Read only" - 
      VCL J11 CGC_VCL - - - - - - - - IO "Read only" - 
      VLO A7 CGC_VLO - - - - - - - - IO "Read only" - 
      VLO A8 CGC_VLO - - - - - - - - IO "Read only" - 
      VLO B7 CGC_VLO - - - - - - - - IO "Read only" - 
      VLO B8 CGC_VLO - - - - - - - - IO "Read only" - 
      VREFH U9 CGC_VREFH - - - - - - - - IO "Read only" - 
      VREFH0 U10 CGC_VREFH0 - - - - - - - - IO "Read only" - 
      VREFL T9 CGC_VREFL - - - - - - - - IO "Read only" - 
      VREFL0 T10 CGC_VREFL0 - - - - - - - - IO "Read only" - 
      VSS A9 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS B9 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS H10 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS H12 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS U4 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS G10 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS G15 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS G17 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS F7 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS F8 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS G7 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS G8 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS F10 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS H7 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS H8 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS M10 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS J7 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS M17 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS K6 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS K7 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS L7 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS L8 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS L12 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS L9 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS K10 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS K12 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS J10 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS J12 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS J14 CGC_VSS - - - - - - - - IO "Read only" - 
      VSS1_USBHS J17 CGC_VSS1_USBHS - - - - - - - - IO "Read only" - 
      VSS2_USBHS J16 CGC_VSS2_USBHS - - - - - - - - IO "Read only" - 
      VSS_MIPI R3 CGC_VSS_MIPI - - - - - - - - IO "Read only" - 
      VSS_USB T17 CGC_VSS_USB - - - - - - - - IO "Read only" - 
    
  User Events
    
  User Event Links
    
  Linker Section Mappings
    
  Module "I/O Port (r_ioport)"
    Parameter Checking: Default (BSP)
    
  Module "Data Shipper (rm_rai_data_shipper)"
    Parameter Checking: Enabled
    Max Number Of DC Instances: 8
    
  Module "Data Collector (rm_rai_data_collector)"
    Parameter Checking: Enabled
    Max Number Of Channels: 16
    
  Module "UART Communication Device (rm_comms_uart)"
    Parameter Checking: Default (BSP)
    
  Module "UART (r_sci_b_uart)"
    Parameter Checking: Default (BSP)
    FIFO Support: Disable
    DTC Support: Enable
    Flow Control Support: Disable
    
  Module "Transfer (r_dtc)"
    Parameter Checking: Default (BSP)
    Linker section to keep DTC vector table: .fsp_dtc_vector_table
    
  Module "CRC (r_crc)"
    Parameter Checking: Default (BSP)
    
  Module "PDM (r_pdm)"
    Parameter Checking: Default (BSP)
    DMAC Support: Disabled
    
  HAL
    Instance "g_ioport I/O Port (r_ioport)"
      Name: g_ioport
      1st Port ELC Trigger Source: Disabled
      2nd Port ELC Trigger Source: Disabled
      3rd Port ELC Trigger Source: Disabled
      4th Port ELC Trigger Source: Disabled
      Pin Configuration Name: g_bsp_pin_cfg
      
    Instance "g_rai_data_shipper0 Data Shipper (rm_rai_data_shipper)"
      Name: g_rai_data_shipper0
      Frame Rate Divider: 0
      Callback: rai_data_shipper0_callback
      
      Instance "g_comms_uart0 UART Communication Device (rm_comms_uart)"
        Name: g_comms_uart0
        RTOS: Recursive Write Mutex: Do Not Use
        RTOS: Recursive Read Mutex: Do Not Use
        RTOS: Mutex Timeout: 0xFFFFFFFF
        RTOS: Write Semaphore: Do Not Use
        RTOS: Read Semaphore: Do Not Use
        RTOS: Semaphore Timeout: 0xFFFFFFFF
        Callback: NULL
        
        Instance "g_uart8 UART (r_sci_b_uart)"
          General: Name: g_uart8
          General: Channel: 8
          General: Data Bits: 8bits
          General: Parity: None
          General: Stop Bits: 1bit
          Baud: Baud Rate: 460800
          Baud: Baud Rate Modulation: Disabled
          Baud: Max Error (%): 5
          Flow Control: CTS/RTS Selection: Hardware RTS
          Flow Control: Software RTS Port: Disabled
          Flow Control: Software RTS Pin: Disabled
          Extra: Clock Source: Internal Clock
          Extra: Start bit detection: Falling Edge
          Extra: Noise Filter: Disable
          Extra: Receive FIFO Trigger Level: Max
          Extra: RS-485: DE Pin: Disable
          Extra: RS-485: DE Pin Polarity: Active High
          Extra: RS-485: DE Pin Assertion Time: 1
          Extra: RS-485: DE Pin Negation Time: 1
          Interrupts: Callback: NULL
          Interrupts: Receive Interrupt Priority: Priority 12
          Interrupts: Transmit Data Empty Interrupt Priority: Priority 12
          Interrupts: Transmit End Interrupt Priority: Priority 12
          Interrupts: Error Interrupt Priority: Priority 12
          
          Instance "g_transfer0 Transfer (r_dtc) SCI8 TXI (Transmit data empty)"
            Name: g_transfer0
            Mode: Normal
            Transfer Size: 1 Byte
            Destination Address Mode: Fixed
            Source Address Mode: Incremented
            Repeat Area (Unused in Normal Mode): Source
            Interrupt Frequency: After all transfers have completed
            Number of Transfers: 0
            Number of Blocks (Valid only in Block Mode): 0
            Number of Transfer Descriptors: 1
            Activation Source: SCI8 TXI (Transmit data empty)
            
      Instance "g_crc0 CRC (r_crc)"
        Name: g_crc0
        CRC Polynomial: CRC-CCITT
        Bit Order: LSB
        Snoop Address: SCI0_TDR
        
      Instance "g_rai_data_collector0 Data Collector (rm_rai_data_collector)"
        General: Name: g_rai_data_collector0
        General: ID: 0
        General: Frame Buffer Length: 4000
        General: Data Ready Callback: rai_data_collector0_callback
        General: Error Callback: rai_data_collector0_error_callback
        Data Feed Mode: Channels: 1
        Data Feed Mode: Channel 0: Name: audio
        Data Feed Mode: Channel 0: Data Type: 16-bit Signed
        Data Feed Mode: Channel 1: Name: dc0_data_feed_ch1
        Data Feed Mode: Channel 1: Data Type: 8-bit Unsigned
        Data Feed Mode: Channel 2: Name: dc0_data_feed_ch2
        Data Feed Mode: Channel 2: Data Type: 8-bit Unsigned
        Data Feed Mode: Channel 3: Name: dc0_data_feed_ch3
        Data Feed Mode: Channel 3: Data Type: 8-bit Unsigned
        Data Feed Mode: Channel 4: Name: dc0_data_feed_ch4
        Data Feed Mode: Channel 4: Data Type: 8-bit Unsigned
        Data Feed Mode: Channel 5: Name: dc0_data_feed_ch5
        Data Feed Mode: Channel 5: Data Type: 8-bit Unsigned
        Data Feed Mode: Channel 6: Name: dc0_data_feed_ch6
        Data Feed Mode: Channel 6: Data Type: 8-bit Unsigned
        Data Feed Mode: Channel 7: Name: dc0_data_feed_ch7
        Data Feed Mode: Channel 7: Data Type: 8-bit Unsigned
        Snapshot Mode: Channels: 0
        Snapshot Mode: DTC Transfer Count: 1
        Snapshot Mode: Channel 0: Name: dc0_snapshot_ch0
        Snapshot Mode: Channel 0: Data Type: 8-bit Unsigned
        Snapshot Mode: Channel 1: Name: dc0_snapshot_ch1
        Snapshot Mode: Channel 1: Data Type: 8-bit Unsigned
        Snapshot Mode: Channel 2: Name: dc0_snapshot_ch2
        Snapshot Mode: Channel 2: Data Type: 8-bit Unsigned
        Snapshot Mode: Channel 3: Name: dc0_snapshot_ch3
        Snapshot Mode: Channel 3: Data Type: 8-bit Unsigned
        Snapshot Mode: Channel 4: Name: dc0_snapshot_ch4
        Snapshot Mode: Channel 4: Data Type: 8-bit Unsigned
        Snapshot Mode: Channel 5: Name: dc0_snapshot_ch5
        Snapshot Mode: Channel 5: Data Type: 8-bit Unsigned
        Snapshot Mode: Channel 6: Name: dc0_snapshot_ch6
        Snapshot Mode: Channel 6: Data Type: 8-bit Unsigned
        Snapshot Mode: Channel 7: Name: dc0_snapshot_ch7
        Snapshot Mode: Channel 7: Data Type: 8-bit Unsigned
        
    Instance "g_pdm2 PDM (r_pdm)"
      Name: g_pdm2
      Channel: 2
      Input: Edge: Rising
      Input: PDM_CLK Frequency: 4000000 Hz
      Output: Bit Format: 16 Bits mode {1 Sign bit  and [18:4] bits of the buffer}
      Output: Target Sampling Frequency (Hz): 32000
      Filter: Moving Average Mode: 1-order (filter is skipped)
      Filter: Low-pass Filter: Low-pass Filter Input Shift: No shift
      Filter: Low-pass Filter: LPF Coefficient h0(10): 0x0400
      Filter: Low-pass Filter: LPF Coefficient h1(0): 0x1FF8
      Filter: Low-pass Filter: LPF Coefficient h1(1): 0x000A
      Filter: Low-pass Filter: LPF Coefficient h1(2): 0x1FF0
      Filter: Low-pass Filter: LPF Coefficient h1(3): 0x0018
      Filter: Low-pass Filter: LPF Coefficient h1(4): 0x1FDC
      Filter: Low-pass Filter: LPF Coefficient h1(5): 0x0034
      Filter: Low-pass Filter: LPF Coefficient h1(6): 0x1FB3
      Filter: Low-pass Filter: LPF Coefficient h1(7): 0x0076
      Filter: Low-pass Filter: LPF Coefficient h1(8): 0x1F2E
      Filter: Low-pass Filter: LPF Coefficient h1(9): 0x0289
      Filter: Low-pass Filter: LPF Coefficient h1(10): 0x0289
      Filter: Low-pass Filter: LPF Coefficient h1(11): 0x1F2E
      Filter: Low-pass Filter: LPF Coefficient h1(12): 0x0076
      Filter: Low-pass Filter: LPF Coefficient h1(13): 0x1FB3
      Filter: Low-pass Filter: LPF Coefficient h1(14): 0x0034
      Filter: Low-pass Filter: LPF Coefficient h1(15): 0x1FDC
      Filter: Low-pass Filter: LPF Coefficient h1(16): 0x0018
      Filter: Low-pass Filter: LPF Coefficient h1(17): 0x1FF0
      Filter: Low-pass Filter: LPF Coefficient h1(18): 0x000A
      Filter: Low-pass Filter: LPF Coefficient h1(19): 0x1FF8
      Filter: Compensation Filter: Compensation Filter Input Shift: No shift
      Filter: Compensation Filter: Compensation Filter Coefficient h(0): 0x1FE8
      Filter: Compensation Filter: Compensation Filter Coefficient h(1): 0x0039
      Filter: Compensation Filter: Compensation Filter Coefficient h(2): 0x003C
      Filter: Compensation Filter: Compensation Filter Coefficient h(3): 0x1E56
      Filter: Compensation Filter: Compensation Filter Coefficient h(4): 0x01DC
      Filter: Compensation Filter: Compensation Filter Coefficient h(5): 0x06E1
      Filter: Compensation Filter: Compensation Filter Coefficient h(6): 0x01DC
      Filter: Compensation Filter: Compensation Filter Coefficient h(7): 0x1E56
      Filter: Compensation Filter: Compensation Filter Coefficient h(8): 0x003C
      Filter: Compensation Filter: Compensation Filter Coefficient h(9): 0x0039
      Filter: Compensation Filter: Compensation Filter Coefficient h(10): 0x1FE8
      Filter: High-pass Filter: High-pass Filter Input Shift: No shift
      Filter: High-pass Filter: HPF Coefficient s(0): 0x3F61
      Filter: High-pass Filter: HPF Coefficient k(1): 0x3EC1
      Filter: High-pass Filter: HPF Coefficient h(0): 0x4000
      Filter: High-pass Filter: HPF Coefficient h(1): 0xC000
      Filter: Sinc Filter Mode: 4-order
      Data Reception: Buffer Overwrite Detection Enable: Enabled
      Data Reception: Data Reception Interrupt Threshold: 16 or more data
      Short Circuit Detection: Short Circuit Detection Enable: Disabled
      Short Circuit Detection: Short Circuit Detection High Continuous Detection Count: 0x0
      Short Circuit Detection: Short Circuit Detection Low Continuous Detection Count: 0x0
      Overvoltage Detection: Overvoltage Detection Lower Limit Enable: Disabled
      Overvoltage Detection: Overvoltage Detection Lower Limit: 0x0
      Overvoltage Detection: Overvoltage Detection Upper Limit Enable: Disabled
      Overvoltage Detection: Overvoltage Detection Upper Limit: 0x0
      Interrupt: Callback: g_audio_cb
      Interrupt: Sound Detection Interrupt Priority: Disabled
      Interrupt: Data Reception Interrupt Priority: Priority 12
      Interrupt: Error Detection Interrupt Priority: Priority 12
      
